# BeaconReport
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**bssId** | [**List**](string.md) | The BSSID field indicates the BSSID of the BSS(s) for which a beacon report has been received. | [default to null]
**channelId** | [**Integer**](integer.md) | Channel number where the beacon was received. | [default to null]
**measurementId** | [**String**](string.md) | Measurement ID of the Measurement configuration applied to this Beacon Report. | [default to null]
**reportingCondition** | [**Integer**](integer.md) | As in table T9-89 of IEEE 802.11-2012 [8]. | [default to null]
**ssId** | [**List**](string.md) | (Optional) The SSID subelement indicates the ESS(s) or IBSS(s) for which a beacon report is received. | [default to null]
**staId** | [**StaIdentity**](StaIdentity.md) |  | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

