# Go API Server for server

WLAN Access Information Service is AdvantEDGE's implementation of [ETSI MEC ISG MEC028 WAI API](http://www.etsi.org/deliver/etsi_gs/MEC/001_099/028/02.03.01_60/gs_MEC028v020301p.pdf) <p>[Copyright (c) ETSI 2024](https://forge.etsi.org/etsi-forge-copyright-notice.txt) <p>**Micro-service**<br>[meep-wais](https://github.com/InterDigitalInc/AdvantEDGE/tree/master/go-apps/meep-wais) <p>**Type & Usage**<br>Edge Service used by edge applications that want to get information about WLAN access information in the network <p>**Note**<br>AdvantEDGE supports a selected subset of WAI API subscription types. <p>Supported subscriptions: <p> - AssocStaSubscription <p> - StaDataRateSubscription

## Overview
This server was generated by the [swagger-codegen]
(https://github.com/swagger-api/swagger-codegen) project.  
By using the [OpenAPI-Spec](https://github.com/OAI/OpenAPI-Specification) from a remote server, you can easily generate a server stub.  
-

To see how to make this your own, look here:

[README](https://github.com/swagger-api/swagger-codegen/blob/master/README.md)

- API version: 2.3.1
- Build date: 2022-12-19T08:32:00.422413-05:00[America/Toronto]


### Running the server
To run the server, follow these simple steps:

```
go run main.go
```

