# RabModNotification

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**AssociateId** | [**[]AssociateId**](AssociateId.md) | 0 to N identifiers to bind the event for a specific UE or flow.  | [optional] [default to null]
**Ecgi** | [***Ecgi**](Ecgi.md) |  | [default to null]
**ErabId** | **int32** | The attribute that uniquely identifies a Radio Access bearer for specific UE as defined in ETSI TS 136 413 [i.3]. | [default to null]
**ErabQosParameters** | [***RabModNotificationErabQosParameters**](RabModNotification_erabQosParameters.md) |  | [optional] [default to null]
**NotificationType** | **string** | Shall be set to \&quot;RabModNotification\&quot;. | [default to null]
**TimeStamp** | [***TimeStamp**](TimeStamp.md) |  | [optional] [default to null]
**Links** | [***CaReconfNotificationLinks**](CaReconfNotification__links.md) |  | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


