# AccessPointInfo

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**AccessPointId** | **string** | Identifier of access point, &lt;E-CGI&gt;&lt;Cell Portion ID&gt; (reference ETSI TS 129 171). Where the E-CGI is made up of the PLMN and Cell Identity (28 bit string). Then the PLMN is made up of the 3 digit MCC &amp; 2 or 3 digit MNC. The Cell Portion is an optional element | [default to null]
**LocationInfo** | [***LocationInfo**](LocationInfo.md) |  | [optional] [default to null]
**ConnectionType** | [***ConnectionType**](ConnectionType.md) |  | [default to null]
**OperationStatus** | [***OperationStatus**](OperationStatus.md) |  | [default to null]
**NumberOfUsers** | **int32** | The number of users currently on the access point. | [default to null]
**Timezone** | [**time.Time**](time.Time.md) | Time zone of access point | [optional] [default to null]
**InterestRealm** | **string** | Interest realm of access point (e.g. geographical area, a type of industry etc.). | [optional] [default to null]
**ResourceURL** | **string** | Self referring URL. | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


