# UserInfo

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**UserId** | **string** | Unique identifier of a user or client node | [optional] [default to null]
**Address** | **string** | Address of user (e.g. \&quot;sip\&quot; URI, \&quot;tel\&quot; URI, \&quot;acr\&quot; URI). | [default to null]
**AccessPointId** | **string** | Identifier of access point, &lt;E-CGI&gt;&lt;Cell Portion ID&gt; (reference ETSI TS 129 171). Where the E-CGI is made up of the PLMN and Cell Identity (28 bit string). Then the PLMN is made up of the 3 digit MCC &amp; 2 or 3 digit MNC. The Cell Portion is an optional element | [default to null]
**ZoneId** | **string** | Identifier of zone | [default to null]
**ResourceURL** | **string** | URL where the UE may be contacted for some service (application specific) | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


