# Go API Server for server

V2X Information Service is AdvantEDGE's implementation of [ETSI MEC ISG MEC030 V2XI API](http://www.etsi.org/deliver/etsi_gs/MEC/001_099/030/02.02.01_60/gs_MEC030v020201p.pdf) <p>[Copyright (c) ETSI 2017](https://forge.etsi.org/etsi-forge-copyright-notice.txt) <p>**Micro-service**<br>[meep-vis](https://github.com/InterDigitalInc/AdvantEDGE/tree/master/go-apps/meep-vis) <p>**Type & Usage**<br>Edge Service used by edge applications that want to get information about radio conditions in the network <p>**Note**<br>AdvantEDGE supports a selected subset of RNI API endpoints (see below) and a subset of subscription types.

## Overview
This server was generated by the [swagger-codegen]
(https://github.com/swagger-api/swagger-codegen) project.  
By using the [OpenAPI-Spec](https://github.com/OAI/OpenAPI-Specification) from a remote server, you can easily generate a server stub.  
-

To see how to make this your own, look here:

[README](https://github.com/swagger-api/swagger-codegen/blob/master/README.md)

- API version: 2.2.1
- Build date: 2022-11-04T17:14:22.484925-04:00[America/New_York]


### Running the server
To run the server, follow these simple steps:

```
go run main.go
```

