# MeasRepUeNotificationCarrierAggregationMeasInfo
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**cellIdNei** | [**String**](string.md) | String representing the E-UTRAN Cell Identity. Encoded as a bit string (size (28)) as defined in ETSI TS 136 413 [i.3]. | [optional] [default to null]
**cellIdSrv** | [**String**](string.md) | String representing the E-UTRAN Cell Identity. Encoded as a bit string (size (28)) as defined in ETSI TS 136 413 [i.3]. | [optional] [default to null]
**rsrpNei** | [**Integer**](integer.md) | Reference Signal Received Power as defined in ETSI TS 136 214 [i.5]. | [optional] [default to null]
**rsrpNeiEx** | [**Integer**](integer.md) | Extended Reference Signal Received Power, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]
**rsrpSrv** | [**Integer**](integer.md) | Reference Signal Received Power as defined in ETSI TS 136 214 [i.5]. | [optional] [default to null]
**rsrpSrvEx** | [**Integer**](integer.md) | Extended Reference Signal Received Power, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]
**rsrqNei** | [**Integer**](integer.md) | Reference Signal Received Quality as defined in ETSI TS 136 214 [i.5]. | [optional] [default to null]
**rsrqNeiEx** | [**Integer**](integer.md) | Extended Reference Signal Received Quality, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]
**rsrqSrv** | [**Integer**](integer.md) | Reference Signal Received Quality as defined in ETSI TS 136 214 [i.5]. | [optional] [default to null]
**rsrqSrvEx** | [**Integer**](integer.md) | Extended Reference Signal Received Quality, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]
**sinrNei** | [**Integer**](integer.md) | Reference Signal \&quot;Signal to Interference plus Noise Ratio\&quot;, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]
**sinrSrv** | [**Integer**](integer.md) | Reference Signal \&quot;Signal to Interference plus Noise Ratio\&quot;, with value mapping defined in ETSI TS 136 133 [i.16]. | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

