# L2MeasCellInfo
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**dl\_gbr\_pdr\_cell** | [**Integer**](integer.md) | It indicates the packet discard rate in percentage of the downlink GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**dl\_gbr\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates the PRB usage for downlink GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**dl\_nongbr\_pdr\_cell** | [**Integer**](integer.md) | It indicates the packet discard rate in percentage of the downlink non-GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**dl\_nongbr\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the PRB usage for downlink non-GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**dl\_total\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the PRB usage for total downlink traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**ecgi** | [**Ecgi**](Ecgi.md) |  | [optional] [default to null]
**number\_of\_active\_ue\_dl\_gbr\_cell** | [**Integer**](integer.md) | It indicates the number of active UEs with downlink GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**number\_of\_active\_ue\_dl\_nongbr\_cell** | [**Integer**](integer.md) | It indicates the number of active UEs with downlink non-GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**number\_of\_active\_ue\_ul\_gbr\_cell** | [**Integer**](integer.md) | It indicates the number of active UEs with uplink GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**number\_of\_active\_ue\_ul\_nongbr\_cell** | [**Integer**](integer.md) | It indicates the number of active UEs with uplink non-GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**received\_dedicated\_preambles\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the received dedicated preamples, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**received\_randomly\_selected\_preambles\_high\_range\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the received randomly selected preambles in the high range, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**received\_randomly\_selected\_preambles\_low\_range\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the received randomly selected preambles in the low range, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ul\_gbr\_pdr\_cell** | [**Integer**](integer.md) | It indicates the packet discard rate in percentage of the uplink GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ul\_gbr\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the PRB usage for uplink GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**ul\_nongbr\_pdr\_cell** | [**Integer**](integer.md) | It indicates the packet discard rate in percentage of the uplink non-GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ul\_nongbr\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the PRB usage for uplink non-GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**ul\_total\_prb\_usage\_cell** | [**Integer**](integer.md) | It indicates (in percentage) the PRB usage for total uplink traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

