# L2MeasCellUeInfo

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**AssociateId** | [***AssociateId**](AssociateId.md) |  | [optional] [default to null]
**DlGbrDataVolumeUe** | **int32** | It indicates the data volume of the downlink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlGbrDelayUe** | **int32** | It indicates the packet delay of the downlink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlGbrPdrUe** | **int32** | It indicates the packet discard rate in percentage of the downlink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlGbrThroughputUe** | **int32** | It indicates the scheduled throughput of the downlink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlNongbrDataVolumeUe** | **int32** | It indicates the data volume of the downlink non-GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlNongbrDelayUe** | **int32** | It indicates the packet delay of the downlink non-GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlNongbrPdrUe** | **int32** | It indicates the packet discard rate in percentage of the downlink nonGBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlNongbrThroughputUe** | **int32** | It indicates the scheduled throughput of the downlink nonGBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**Ecgi** | [***Ecgi**](Ecgi.md) |  | [optional] [default to null]
**UlGbrDataVolumeUe** | **int32** | It indicates the data volume of the uplink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlGbrDelayUe** | **int32** | It indicates the packet delay of the uplink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlGbrPdrUe** | **int32** | It indicates the packet discard rate in percentage of the uplink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlGbrThroughputUe** | **int32** | It indicates the scheduled throughput of the uplink GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlNongbrDataVolumeUe** | **int32** | It indicates the data volume of the uplink non-GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlNongbrDelayUe** | **int32** | It indicates the packet delay of the uplink non-GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlNongbrPdrUe** | **int32** | It indicates the packet discard rate in percentage of the uplink nonGBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlNongbrThroughputUe** | **int32** | It indicates the scheduled throughput of the uplink non-GBR traffic of a UE, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


