# L2MeasCellInfo

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**DlGbrPdrCell** | **int32** | It indicates the packet discard rate in percentage of the downlink GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlGbrPrbUsageCell** | **int32** | It indicates the PRB usage for downlink GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**DlNongbrPdrCell** | **int32** | It indicates the packet discard rate in percentage of the downlink non-GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**DlNongbrPrbUsageCell** | **int32** | It indicates (in percentage) the PRB usage for downlink non-GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**DlTotalPrbUsageCell** | **int32** | It indicates (in percentage) the PRB usage for total downlink traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**Ecgi** | [***Ecgi**](Ecgi.md) |  | [optional] [default to null]
**NumberOfActiveUeDlGbrCell** | **int32** | It indicates the number of active UEs with downlink GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**NumberOfActiveUeDlNongbrCell** | **int32** | It indicates the number of active UEs with downlink non-GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**NumberOfActiveUeUlGbrCell** | **int32** | It indicates the number of active UEs with uplink GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**NumberOfActiveUeUlNongbrCell** | **int32** | It indicates the number of active UEs with uplink non-GBR traffic, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ReceivedDedicatedPreamblesCell** | **int32** | It indicates (in percentage) the received dedicated preamples, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ReceivedRandomlySelectedPreamblesHighRangeCell** | **int32** | It indicates (in percentage) the received randomly selected preambles in the high range, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**ReceivedRandomlySelectedPreamblesLowRangeCell** | **int32** | It indicates (in percentage) the received randomly selected preambles in the low range, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlGbrPdrCell** | **int32** | It indicates the packet discard rate in percentage of the uplink GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlGbrPrbUsageCell** | **int32** | It indicates (in percentage) the PRB usage for uplink GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**UlNongbrPdrCell** | **int32** | It indicates the packet discard rate in percentage of the uplink non-GBR traffic in a cell, as defined in ETSI TS 136 314 [i.11]. | [optional] [default to null]
**UlNongbrPrbUsageCell** | **int32** | It indicates (in percentage) the PRB usage for uplink non-GBR traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]
**UlTotalPrbUsageCell** | **int32** | It indicates (in percentage) the PRB usage for total uplink traffic, as defined in ETSI TS 136 314 [i.11] and ETSI TS 136 423 [i.12]. | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


