# ExtBssLoad

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**MuMimoStaCount** | **int32** | Indicates the total number of STAs currently associated with this BSS that have a 1 in the MU Beamformee Capable field of their VHT Capabilities element. | [default to null]
**ObsSec20MhzUtil** | **int32** | Observable loading on each of the secondary 20 MHz channel. | [default to null]
**ObsSec40MhzUtil** | **int32** | Observable loading on each of the secondary 40 MHz channel. | [default to null]
**ObsSec80MhzUtil** | **int32** | Observable loading on each of the secondary 80 MHz channel. | [default to null]
**SpatStreamUnderUtil** | **int32** | The percentage of time, linearly scaled with 255 representing 100 %, that the AP has underutilized spatial domain resources for given busy time of the medium. | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


