# ExtBssLoad
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**muMimoStaCount** | [**Integer**](integer.md) | Indicates the total number of STAs currently associated with this BSS that have a 1 in the MU Beamformee Capable field of their VHT Capabilities element. | [default to null]
**obsSec20MhzUtil** | [**Integer**](integer.md) | Observable loading on each of the secondary 20 MHz channel. | [default to null]
**obsSec40MhzUtil** | [**Integer**](integer.md) | Observable loading on each of the secondary 40 MHz channel. | [default to null]
**obsSec80MhzUtil** | [**Integer**](integer.md) | Observable loading on each of the secondary 80 MHz channel. | [default to null]
**spatStreamUnderUtil** | [**Integer**](integer.md) | The percentage of time, linearly scaled with 255 representing 100 %, that the AP has underutilized spatial domain resources for given busy time of the medium. | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

