# RegistrationInfoDeviceInformation
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**associateId** | [**AssociateId**](AssociateId.md) |  | [default to null]
**appMobilityServiceLevel** | [**Integer**](integer.md) | This attribute provides an option for the application instance (server) to communicate with the application client before relocating this application instance to another MEC host. Applicable values are: 1 &#x3D; APP_MOBILITY_NOT_ALLOWED, 2 &#x3D; APP_MOBILITY_WITH_CONFIRMATION, 3 &#x3D; APP_MOBILITY_WITHOUT_CONFIRMATION. | [optional] [default to null]
**contextTransferState** | [**Integer**](integer.md) | If present, it represents the state of transferring the user context to another application instance. The applicable values are: 0 &#x3D; NOT_TRANSFERRED, 1&#x3D; USER_CONTEXT_TRANSEFR_COMPLETED. | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

