## Cross reference for envi classes, properties and dataproperties back to ToC

This section provides details for each class and property defined by envi.

### Classes

- Actuator
- Color
- Communication interface
- Communication protocol
- Compass direction
- Device
- Device
- Digital representation
- Frequency measurement
- Frequency unit
- Geometry
- Height measurement
- Lamppost
- Length unit
- Light
- Light point
- Light property
- Measurement
- Period measurement
- Photometer
- Physical object
- Point
- Property
- Sensor
- Service
- Spatial thing
- System
- Temporal unit
- TESS (Telescope Encoder and Sky Sensor)
- Unit of measure

### Actuatorc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Actuator

Device that can act over at least one property.

has super-classes
  Device c
  affects property op only Property c

### Colorc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Color

Color of the emitted light. It might be indicated by named colors or using other type of color values like hexadecimal for RGB, color temperature, etc.

is disjoint with
  Spatial thing c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Light c, Service c, Unit of measure c

### Communication interfacec back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#CommunicationInterface

An interface defines which primitive operations and services the lower layer makes available to the upper one, when referring to network layers. (Definition adapted from "Tanenbaum, A. S. (2003). Computer networks, 4-th edition. ed: Prentice Hall.")

has super-classes
  has version dp only string
  has version dp max 1
is disjoint with
  Spatial thing c, Color c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Light c, Measurement c, Property c, Unit of measure c

### Communication protocolc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#CommunicationProtocol

A protocol is an agreement between the communicating parties on how communication is to proceed. (Definition taken from "Tanenbaum, A. S. (2003). Computer networks, 4-th edition. ed: Prentice Hall.")

is disjoint with
  Spatial thing c, Color c, Communication interface c, Compass direction c, Digital representation c, Geometry c, Light c, Measurement c, Property c, Service c, Unit of measure c

### Compass directionc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#CompassDirection

The four cardinal directions or cardinal points are the directions of north, east, south, and west, commonly denoted by their initials: N, E, S, W. East and west are at right angles to north and south, with east being in the clockwise direction of rotation from north and west being directly opposite east. Intermediate points between the four cardinal directions form the points of the compass. (definition taken from https://en.wikipedia.org/wiki/Cardinal_direction)

is disjoint with
  Spatial thing c, Color c, Communication interface c, Communication protocol c, Digital representation c, Geometry c, Light c, Measurement c, Property c, Service c, Unit of measure c

### Devicec back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Device

A thing made or adapted for a particular purpose, especially a piece of mechanical or electronic equipment. For example ‘a measuring device’ (definition taken from https://en.oxforddictionaries.com/definition/device). In this ontology it refers to the devices for environmental purposes.

has super-classes
  System c
  Device c
  has frequency measurement op only Frequency measurement c
  has transmission period op only Period measurement c
  is contained in op only Physical object c
  has revision number dp only string
  has version dp only string
  has manufacturer dp only string
  has revision number dp max 1
  has version dp max 1
has sub-classes
  Actuator c, Lamppost c

### Devicec back to ToC or Class ToC

IRI: https://w3id.org/saref#Device

A tangible object designed to accomplish a particular task in households, common public buildings or offices. In order to accomplish this task, the device performs one or more functions. For example, a washing machine is designed to wash (task) and to accomplish this task it performs the start and stop function.

Is defined by
  https://w3id.org/saref#

has sub-classes
  Device c, Sensor c

### Digital representationc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#DigitalRepresentation

A digital representation encapsulates a physical object accessible via Web services

has super-classes
  encapsulates op only Physical object c
  is accesible through op only Service c
  has creation date dp only date time
  has identifier dp only string
  has tag dp only string
  has description dp only string
  has name dp only string
  has creation date dp max 1
  has identifier dp max 1
is disjoint with
  Spatial thing c, Color c, Communication interface c, Communication protocol c, Compass direction c, Geometry c, Light c, Measurement c, Unit of measure c

### Frequency measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#FrequencyMeasurement

Represents the measured value made over a frequency property. It is also linked to the frequency unit of measure in which the value is expressed and the timestamp of the measurement.

has super-classes
  Measurement c
  relates to property op value Frequency
  is measured in op exactly 1 Frequency unit c

### Frequency unitc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#FrequencyUnit

Unit of measure for the quantity frequency.

has super-classes
  Unit of measure c
has members
  Hertz ni, Reciprocal day ni, Reciprocal hour ni, Reciprocal second ni, Reciprocal year ni

### Geometryc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Geometry

Represents the shape of the light emission. It might be instantiated by individuals like "spherical", "cylindrical", etc. even though it is open to more comples representation of geometries using other vocabularies.

is disjoint with
  Spatial thing c, Color c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Light c, Measurement c, Property c, Service c, Unit of measure c

### Height measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#HeightMeasurement

Represents the measured value made over a height property. It is also linked to the height unit of measure in which the value is expressed and the timestamp of the measurement.

has super-classes
  Measurement c
  relates to property op value Height
  is measured in op exactly 1 Length unit c

### Lamppostc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Lamppost

A tall pole with a light at the top.

has super-classes
  Device c
  has light point op only Light point c
  projects light op only Light c
  has shield dp only boolean

### Length unitc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#LengthUnit

Unit of measure for the quantity lenght.

has super-classes
  Unit of measure c
has members
  Centimetre ni, Decametre ni, Decimetre ni, Hectometre ni, Kilometre ni, Metre ni, Milimetre ni

### Lightc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Light

A light source, which may be a lantern, a street light, a floodlight, a signal lamp or any other device whose primary purpose is the generation of light. (Definition taken from http://wiki.openstreetmap.org/wiki/Proposed_features/Key:light_source#Description)

has super-classes
  has color op only Color c
  has geometry op only Geometry c
  is projected from height op only Height measurement c
  is projected in direction op only Compass direction c
  has flash dp only boolean
  has projection angle dp only float
is disjoint with
  Color c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Measurement c, Property c, Service c, Unit of measure c

### Light pointc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#LightPoint

An spatial point from where a light is projected. It might belong to a lamppost.

has super-classes
  Point c
  location op only Spatial thing c
  projects light op only Light c

### Light propertyc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#LightProperty

An aspect of light that can be observable by a sensor.

has super-classes
  Property c
has members
  Fluorescence ni, Illuminance ni, Irradiance ni, Light absorption ni, Light magnitude ni, Luminiscence ni, Phosphorescence ni, Reflection of light ni, Scattering of light ni

### Measurementc back to ToC or Class ToC

IRI: https://w3id.org/saref#Measurement

Represents the measured value made over a property. It is also linked to the unit of measure in which the value is expressed and the timestamp of the measurement.

has super-classes
  is measured in op only Unit of measure c
  relates to property op only Property c
  is measured in op exactly 1 Unit of measure c
  relates to property op exactly 1 Property c
  has timestamp dp only date time
  has value dp only float
  has value dp exactly 1
has sub-classes
  Frequency measurement c, Height measurement c, Period measurement c
is disjoint with
  Spatial thing c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Light c, Property c, Service c, Unit of measure c

### Period measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#PeriodMeasurement

Represents the measured value over a period property. It is also linked to the period unit of measure in which the value is expressed and the timestamp of the measurement.

has super-classes
  Measurement c
  relates to property op value Period
  is measured in op exactly 1 Temporal unit c

### Photometerc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#Photometer

A photometer, generally, is an instrument that measures light intensity or optical properties of solutions or surfaces.

has super-classes
  Sensor c
  measures property op some Light property c
has sub-classes
  TESS (Telescope Encoder and Sky Sensor) c

### Physical objectc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#PhysicalObject

Any Object that has a proper space region. (Definition extracted from DUL ontology)

has super-classes
  Spatial thing c
  location op only Spatial thing c
  contains op only Physical object c
  has digital representation op only Digital representation c
  is contained in op only Physical object c
  has description dp only string
has sub-classes
  System c

### Pointc back to ToC or Class ToC

IRI: http://www.w3.org/2003/01/geo/wgs84_pos#Point

A point, typically described using a coordinate system relative to Earth, such as WGS84. Uniquely identified by lat/long/alt. i.e. spaciallyIntersects(P1, P2) :- lat(P1, LAT), long(P1, LONG), alt(P1, ALT), at(P2, LAT), long(P2, LONG), alt(P2, ALT). sameThing(P1, P2) :- type(P1, Point), type(P2, Point), spaciallyIntersects(P1, P2).

Is defined by
  http://www.w3.org/2003/01/geo/wgs84_pos#

has sub-classes
  Light point c

### Propertyc back to ToC or Class ToC

IRI: https://w3id.org/saref#Property

An aspect of an entity that can be observable by a sensor.

has sub-classes
  Light property c
has members
  Frequency ni, Height ni, Period ni
is disjoint with
  Communication interface c, Communication protocol c, Compass direction c, Geometry c, Light c, Measurement c, Service c, Unit of measure c

### Sensorc back to ToC or Class ToC

IRI: https://w3id.org/saref#Sensor

A device that detects and responds to events or changes in the physical environment such as light, motion, or temperature changes. A device that has category saref:Sensor and performs a saref:SensingFunction.

Is defined by
  https://w3id.org/saref#

has super-classes
  Device c
  makes measurement op only Measurement c
  measures property op only Property c
has sub-classes
  Photometer c

### Servicec back to ToC or Class ToC

IRI: https://w3id.org/saref#Service

A service is a representation of a function to a network that makes the function discoverable, registerable, remotely controllable by other devices in the network. A service can represent one or more functions. A Service is offered by a device that wants (a certain set of) its function(s) to be discoverable, registerable, remotely controllable by other devices in the network. A Service must specify the device that is offering the service, the function(s) to be represented, and the (input and output) parameters necessary to operate the service.

Is defined by
  https://w3id.org/saref#

is disjoint with
  Spatial thing c, Color c, Communication protocol c, Compass direction c, Geometry c, Light c, Measurement c, Property c, Unit of measure c

### Spatial thingc back to ToC or Class ToC

IRI: http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing

Anything with spatial extent, i.e. size, shape, or position. e.g. people, places, bowling balls, as well as abstract areas like cubes.

Is defined by
  http://www.w3.org/2003/01/geo/wgs84_pos#

has sub-classes
  Physical object c
is disjoint with
  Color c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Measurement c, Service c

### Systemc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#System

A group of related hardware units or programs or both, especially when dedicated to a single application. (Definition taken from https://en.oxforddictionaries.com/definition/system)

has super-classes
  Physical object c
  has component op only System c
  is component of op only System c
  is connected to op only System c
  uses communication interface op only Communication interface c
  uses communication protocol op only Communication protocol c
has sub-classes
  Device c

### Temporal unitc back to ToC or Class ToC

IRI: http://www.w3.org/2006/time#TemporalUnit

A temporal unit of measure, which provides a scale factor for a time quantity.

Is defined by
  http://www.w3.org/2006/time#

has super-classes
  Unit of measure c

### TESS (Telescope Encoder and Sky Sensor)c back to ToC or Class ToC

IRI: https://w3id.org/def/saref4envi#TESS

The Telescope Encoder and Sky Sensor (TESS) is a Sky Brightness and Cloud detector developed as a device for a remote observatory. A TESS can observe the light magnitude and other properties as ambient temperature and sky temperature.

has super-classes
  Photometer c

### Unit of measurec back to ToC or Class ToC

IRI: https://w3id.org/saref#UnitOfMeasure

The unit of measure is a standard for measurement of a quantity, such as a Property. For example, Power is a property and Watt is a unit of power that represents a definite predetermined power: when we say 10 Watt, we actually mean 10 times the definite predetermined power called "watt". Our definition is based on the definition of unit of measure in the Ontology of units of Measure (OM). We propose here a list of some units of measure that are relevant for the purpose of the Smart Appliances ontology, but this list can be extended.

Is defined by
  https://w3id.org/saref#

has sub-classes
  Frequency unit c, Length unit c, Temporal unit c
is disjoint with
  Color c, Communication interface c, Communication protocol c, Compass direction c, Digital representation c, Geometry c, Light c, Measurement c, Property c, Service c

### Object Properties

- affects property
- contains
- encapsulates
- has color
- has component
- has digital representation
- has frequency measurement
- has geometry
- has light point
- has transmission period
- is accesible through
- is component of
- is connected to
- is contained in
- is measured in
- is projected from height
- is projected in direction
- location
- makes measurement
- measures property
- projects light
- relates to property
- uses communication interface
- uses communication protocol

### affects propertyop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#affectsProperty

A relation between an actuator with the property or properties it can act on

### containsop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#contains

A relation between a physical object and the physical objects that can be contained in it.

is inverse of
  is contained in op

### encapsulatesop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#encapsulates

A relation between a digital representation and the physical objects it represents.

has characteristics: functional

is inverse of
  has digital representation op

### has colorop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasColor

A relation between a light emitted and its color.

### has componentop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasComponent

A relation between a system and the system in which it might be decomposed.

has characteristics: transitive

is inverse of
  is component of op

### has digital representationop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasDigitalRepresentation

A relation between a physical object and the digital representation in which it is encapsulated.

has characteristics: inverse functional

is inverse of
  encapsulates op

### has frequency measurementop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasFrequencyMeasurement

The relation between a device and the frequency in which it makes measurements.

### has geometryop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasGeometry

A relation between a light emitted and the shape it is projected in.

### has light pointop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasLightPoint

A relation between a lamppost and its light points

### has transmission periodop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#hasTransmissionPeriod

The relation between a device and the period in which it transmit information.

### is accesible throughop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isAccesibleThrough

The relation between a digital representation and the service which it is accesible through.

### is component ofop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isComponentOf

A relation between a system and the system it belongs to as a component.

has characteristics: transitive

is inverse of
  has component op

### is connected toop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isConnectedTo

A relation between a system and the system to which it is connected.

### is contained inop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isContainedIn

A relation between a physical object and the physical object in which it might be contained.

is inverse of
  contains op

### is measured inop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#isMeasuredIn

A relation between a measurement and the unit of measure in which the measurement value is expressed.

Is defined by
  http://saref.linkeddata.es/def/envi#

### is projected from heightop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isProjectedFromHeight

A relation between a light and the height measurement from which it is projected.

### is projected in directionop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#isProjectedInDirection

A relation between a light and the direction in which it is projected.

### locationop back to ToC or Object Property ToC

IRI: http://www.w3.org/2003/01/geo/wgs84_pos#location

The relation between something and the point, or other geometrical thing in space, where it is. For example, the realtionship between a radio tower and a Point with a given lat and long. Or a relationship between a park and its outline as a closed arc of points, or a road and its location as a arc (a sequence of points). Clearly in practice there will be limit to the accuracy of any such statement, but one would expect an accuracy appropriate for the size of the object and uses such as mapping .

Is defined by
  http://www.w3.org/2003/01/geo/wgs84_pos#

### makes measurementop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#makesMeasurement

A relation between a sensor and the measurements it makes. Such measurement will link together the valur of the measurement, its unit of measure and the property to which it relates.

Is defined by
  http://saref.linkeddata.es/def/envi#

### measures propertyop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#measuresProperty

A relation between a sensor and the property o properties it can take measurement about.

Is defined by
  http://saref.linkeddata.es/def/envi#

### projects lightop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#projectsLight

A relation between a lamppost or a light point and the light (or lights) they might project.

### relates to propertyop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#relatesToProperty

A relation between a measurement and the property such measurement is about.

Is defined by
  http://saref.linkeddata.es/def/envi#

### uses communication interfaceop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#usesCommunicationInterface

A relation between a system and the communication interface it uses.

### uses communication protocolop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4envi#usesCommunicationProtocol

A relation between a system and the communication protocol it uses.

### Data Properties

- has creation date
- has description
- has flash
- has identifier
- has manufacturer
- has name
- has projection angle
- has revision number
- has shield
- has tag
- has timestamp
- has value
- has version

### has creation datedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasCreationDate

A relationship defining the creation date of an entity (e.g., a digital representation).

has characteristics: functional

has range
  date time

### has descriptiondp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasDescription

A relationship providing a description of an entity (e.g., device)

Is defined by
  https://w3id.org/saref#

### has flashdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasFlash

A relationship stating whether a light has flash.

has characteristics: functional

has range
  boolean

### has identifierdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasIdentifier

A relationship providing the identifier of an entity (e.g., digital representation)

has range
  string

### has manufacturerdp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasManufacturer

A relationship identifying the manufacturer of an entity (e.g., device)

Is defined by
  https://w3id.org/saref#

### has namedp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasName

A relationship providing the name of an entity (e.g., device)

Is defined by
  https://w3id.org/saref#

### has projection angledp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasProjectionAngle

A relationship defining the projection angle of an entity (e.g., a light).

has characteristics: functional

has range
  float

### has revision numberdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasRevisionNumber

A relationship defining the revision number of a certain entity (e.g., a device)

has range
  string

### has shielddp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasShield

A relationship stating whether a lamppost has a shield.

has characteristics: functional

has range
  boolean

### has tagdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasTag

A relationship stating the tags that can be assigned to an entity (e.g., a digital representation).

has range
  string

### has timestampdp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasTimestamp

A relationship stating the timestamp of an entity (e.g. a measurement).

Is defined by
  http://saref.linkeddata.es/def/envi#

has characteristics: functional

has range
  date time

### has valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasValue

A relationship defining the value of a certain property, e.g., energy or power

Is defined by
  https://w3id.org/saref#

### has versiondp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4envi#hasVersion

A relationship defining the version of a certain entity (e.g., a device)

has characteristics: functional

has range
  string

### Named Individuals

- Centimetre
- Decametre
- Decimetre
- Fluorescence
- Frequency
- Hectometre
- Height
- Hertz
- Illuminance
- Irradiance
- Kilometre
- Light absorption
- Light magnitude
- Luminiscence
- Metre
- Milimetre
- Period
- Phosphorescence
- Reciprocal day
- Reciprocal hour
- Reciprocal second
- Reciprocal year
- Reflection of light
- Scattering of light

### Centimetreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/centimetre

belongs to
  Length unit c

### Decametreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/decametre

belongs to
  Length unit c

### Decimetreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/decimetre

belongs to
  Length unit c

### Fluorescenceni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Fluorescence

An individual representing the light property fluorescence.

belongs to
  Light property c

### Frequencyni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Frequency

An individual representing the property frequency.

belongs to
  Property c

### Hectometreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/hectometre

belongs to
  Length unit c

### Heightni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Height

An individual representing the property height.

belongs to
  Property c

### Hertzni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/hertz

belongs to
  Frequency unit c

### Illuminanceni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Illuminance

An individual representing the light property illuminance.

belongs to
  Light property c

### Irradianceni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Irradiance

An individual representing the light property irradiance.

belongs to
  Light property c

### Kilometreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/kilometre

belongs to
  Length unit c

### Light absorptionni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#LightAbsorption

An individual representing the light property light absorption.

belongs to
  Light property c

### Light magnitudeni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#LightMagnitude

An individual representing the light property light magnitude.

belongs to
  Light property c

### Luminiscenceni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Luminiscence

An individual representing the light property luminiscence.

belongs to
  Light property c

### Metreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/metre

belongs to
  Length unit c

### Milimetreni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/millimetre

belongs to
  Length unit c

### Periodni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Period

An individual representing the property period.

belongs to
  Property c

### Phosphorescenceni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#Phosphorescence

An individual representing the light property phosphorescence.

belongs to
  Light property c

### Reciprocal dayni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/reciprocal_day

belongs to
  Frequency unit c

### Reciprocal hourni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/reciprocal_hour

belongs to
  Frequency unit c

### Reciprocal secondni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/reciprocal_second-time

belongs to
  Frequency unit c

### Reciprocal yearni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/reciprocal_year

belongs to
  Frequency unit c

### Reflection of lightni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#ReflectionOfLight

An individual representing the light property reflection of light.

belongs to
  Light property c

### Scattering of lightni back to ToC or Named Individual ToC

IRI: https://w3id.org/def/saref4envi#ScatteringOfLight

An individual representing the light property scattering of light.

belongs to
  Light property c

## Legend back to ToC

c: Classes
op: Object Properties
dp: Data Properties
ni: Named Individuals