## 4. Cross reference for [Ontology Name] classes, properties and dataproperties

This section provides details for each class and property defined by [Ontology Name].

## Classes

- actuator
- air to air heat recovery
- audio visual appliance
- boiler
- burner
- chiller
- coil
- compressor
- condenser
- cooled beam
- cooling tower
- damper
- duct silencer
- electric flow storage device
- electric generator
- electric motor
- engine
- evaporative cooler
- evaporator
- fan
- filter
- flow meter
- heat exchanger
- humidifier
- interceptor
- lamp
- outlet
- protective device tripping unit
- pump
- shading device
- space heater
- switching device
- tank
- transformer
- transport element
- tube bundle
- valve
- vibration isolator

### actuatorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Actuator

has super-classes
  manual override dp only boolean
  fail position dp only string

### air to air heat recoveryc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#AirToAirHeatRecovery

has super-classes
  has defrost dp only boolean
  secondary air flow rate range dp only real real range c
  primary air flow rate range dp only real real range c
  operational temperature range dp only real real range c
  heat transfer type enum dp only string

### audio visual appliancec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#AudioVisualAppliance

has super-classes
  audio volume dp only float
  media source dp only string

### boilerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Boiler

has super-classes
  nominal part load ratio dp only real real range c
  water inlet temperature range dp only real real range c
  operating mode dp only string
  is water storage heater dp only boolean
  water storage capacity dp only float
  energy source dp only string
  nominal energy consumption dp only float
  outlet temperature range dp only real real range c
  pressure rating dp only float
  heat transfer surface area dp only float

### burnerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Burner

has super-classes
  energy source dp only string

### chillerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Chiller

has super-classes
  nominal heat rejection rate dp only float
  nominal condensing temperature dp only float
  nominal efficiency dp only float
  nominal power consumption dp only float
  nominal capacity dp only float
  nominal evaporating temmperature dp only float

### coilc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Coil

has super-classes
  placement type dp only string
  nominal latent capacity dp only float
  nominal ua dp only float
  nominal sensible capacity dp only float
  operational temperature range dp only real real range c
  air flow rate range op only real real range c

### compressorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Compressor

has super-classes
  compressor speed dp only float
  ideal shaft power dp only float
  minimun part load ratio dp only float
  power source dp only string
  refrigerant class dp only string
  nominal capacity dp only float
  ideal capacity dp only float
  impeller diameter dp only float
  maximum part load ratio dp only float
  has hot gas bypass dp only boolean

### condenserc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Condenser

has super-classes
  nominal heat transfer coefficient dp only float
  internal surface area dp only float
  internal water volume dp only float
  internal refrigerant volume dp only float
  external surface area dp only float
  refrigerant class dp only string
  nominal heat transfer area dp only float

### cooled beamc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#CooledBeam

has super-classes
  is free hanging dp only boolean
  integrated lighting type dp only string
  nominal return water temperature heating dp only float
  nominal sorrounding temperature heating dp only float
  pipe connection enum dp only string
  nominal supply water temperature heating dp only float
  coil width dp only float
  nominal supply water temperature cooling dp only float
  nominal water flow heating dp only float
  nominal heating capacity dp only float
  water pressure range dp only real real range c
  coil length dp only float
  water flow control system type dp only string
  nominal sorrounding temperature cooling dp only float
  nominal return water temperature cooling dp only float
  finish color dp only string
  nominal cooling capacity dp only float
  nominal water flow cooling dp only float
  nominal sorrounding humidity cooling dp only float

### cooling towerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#CoolingTower

has super-classes
  number of cells dp only integer
  spray type dp only string
  lift elevation difference dp only float
  ambient design dry bulb temperature dp only float
  basin reserve volume dp only float
  circuit type dp only string
  control strategy dp only string
  flow arrangement dp only string
  ambient design wet bulb temperature dp only float
  water requirement dp only float
  operation temperature range dp only float
  nominal capcity dp only float
  capacity control dp only string

### damperc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Damper

has super-classes
  number of blades dp only integer
  temperature rating dp only float
  leakage fully closed dp only float
  frame thickness dp only float
  close off rating dp only float
  open pressure drop dp only float
  operation dp only string
  blade action dp only string
  blade thickness dp only float
  frame depth dp only float
  temperature range dp only real real range c
  blade edge dp only string
  maximum air flow rate dp only float
  frame type dp only string
  nominal air flow rate dp only float
  orientation dp only string
  face area dp only float
  maximum working pressure dp only float
  blade shape dp only string

### duct silencerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#DuctSilencer

has super-classes
  working pressure range dp only real real range c
  has exterior insulation dp only boolean
  air flow rate range op only real real range c
  weight dp only float
  hydraulic diameter dp only float
  temperature range dp only real real range c
  length dp only float

### electric flow storage devicec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#ElectricFlowStorageDevice

has super-classes
  nominal frequency dp only float
  nominal supply voltage dp only float
  nominal supply voltage offset dp only real real range c

### electric generatorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#ElectricGenerator

has super-classes
  maximum power output dp only float
  electric generator efficiency dp only float
  start current factor dp only float

### electric motorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#ElectricMotor

has super-classes
  starting time dp only float
  has part winding dp only boolean
  locked rotor current dp only float
  te time dp only float
  motor enclosure type dp only string
  frame size dp only string
  electric motor efficiency dp only float
  start current factor dp only float
  maximum power output dp only float
  is guarded dp only boolean

### enginec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Engine

has super-classes
  energy source dp only string

### evaporative coolerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#EvaporativeCooler

has super-classes
  operational temperature range dp only real real range c
  water requirement dp only float
  flow arrangement dp only string
  heat exchange area dp only float

### evaporatorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Evaporator

has super-classes
  nominal heat transfer coefficient dp only float
  external surface area dp only float
  nominal heat transfer area dp only float
  evaporation coolant dp only string
  internal water volume dp only float
  internal refrigerant volume dp only float
  refrigerant class dp only string
  evaporation medium type dp only string
  internal surface area dp only float

### fanc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Fan

has super-classes
  nominal power rate dp only float
  operational riterial dp only float
  nominal total pressure dp only float
  motor drive type dp only string
  nominal static pressure dp only float
  operation temperature range dp only real real range c
  nominal rotation speed dp only float
  nominal air flow rate dp only float
  capacity control type dp only string

### filterc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Filter

has super-classes
  nominal media surface velocity dp only float
  initial resistance dp only float
  nominal pressure drop dp only float
  operation temperature range dp only real real range c
  nominal filter face velocity dp only float
  flow rate range dp only real real range c
  nominal flow rate dp only float
  final resistance dp only float
  nominal particle geometric standard deviation dp only float
  nominal particle geometric mean diameter dp only float
  weight dp only float

### flow meterc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#FlowMeter

has super-classes
  read out type dp only string
  remote reading dp only boolean

### heat exchangerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#HeatExchanger

has super-classes
  arrangement dp only string

### humidifierc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Humidifier

has super-classes
  nominal moisture gain dp only float
  water requirement dp only float
  nominal air flow rate dp only float
  application dp only string
  internal control dp only string
  weight dp only float

### interceptorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Interceptor

has super-classes
  nominal body length dp only float
  nominal body depth dp only float
  inlet connection size dp only float
  ventilating pipe size dp only float
  cover width dp only float
  cover length dp only float
  nominal body width dp only float
  outlet connection size dp only float

### lampc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Lamp

has super-classes
  spectrum dp only real real range c
  lamp compensation type dp only string
  color rendering index dp only integer
  color appearance dp only string
  color tempeature dp only float
  lamp ballast type dp only string
  lamp maintenance factor dp only float
  light emitter nominal power dp only float
  contributed luminous flux dp only float

### outletc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Outlet

has super-classes
  is pluggable outlet dp only boolean
  number os sockets dp only integer

### protective device tripping unitc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#ProtectiveDeviceTrippingUnit

has super-classes
  limiting terminal size dp only float
  standard dp only string

### pumpc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Pump

has super-classes
  flow resistance range dp only real real range c
  nomminal rotation speed dp only float
  net positive suction head dp only float
  temperature range dp only real real range c
  connection size dp only float
  flow rate range dp only real real range c

### shading devicec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#ShadingDevice

has super-classes
  solar transmittance dp only float
  shading device type dp only string
  solar reflectance dp only float
  is external dp only boolean
  roughness dp only string
  mechanical operated dp only boolean
  thermal transmittance dp only float
  visible light transmittance dp only float
  visible light reflectance dp only float

### space heaterc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#SpaceHeater

has super-classes
  temperature classification dp only string
  thermal efficiency dp only float
  body mass dp only float
  output capacity dp only float
  number of sections dp only integer
  number of panels dp only integer
  thermal mass heat capacity dp only float
  placement type dp only string
  heat transfer medium dp only string
  energy source dp only string
  heat transfer dimension dp only string

### switching devicec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#SwitchingDevice

has super-classes
  is illuminated dp only boolean
  legend dp only string
  number of gangs dp only integer
  switch function dp only string
  has lock dp only boolean

### tankc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Tank

has super-classes
  first curvature radius dp only float
  number of sections dp only integer
  nominal capacity dp only float
  storage type dp only string
  second curvature radius dp only float
  access type dp only string
  pattern type dp only string
  nominal depth dp only float
  end shape type dp only string
  effective capacity dp only float
  nominal length or diameter dp only float
  nominal width or diameter dp only float
  operating wight dp only float

### transformerc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Transformer

has super-classes
  secondary current type dp only string
  is neutral primary terminal available dp only boolean
  is neutral secondary terminal available dp only boolean
  primary frequency dp only float
  secondary current dp only float
  secondary apparent power dp only float
  imaginary impedance ratio dp only float
  primary voltage dp only float
  primary apparent power dp only float
  secondary frequency dp only float
  secondary voltage dp only float
  real impedance ratio dp only float
  primary current dp only float
  maximum apparent power dp only float
  transformer vector group dp only string
  short circuit voltage op only complex number c

### transport elementc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#TransportElement

has super-classes
  fire exit dp only boolean
  capacity people dp only positive integer
  capacity weight dp only float

### tube bundlec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#TubeBundle

has super-classes
  nominal diameter dp only float
  volumen dp only float
  outside diameter dp only float
  inside diameter dp only float
  has turbulator dp only boolean
  number of circuits dp only integer
  in line row spacing dp only float
  vertical spacing dp only float
  length dp only float
  fouling factor dp only float
  number of rows dp only integer
  staggered row spacing dp only float
  thermal conductivity dp only float
  horizontal spacing dp only float

### valvec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#Valve

has super-classes
  flow coefficient dp only float
  close off rating dp only float
  size dp only float
  working pressure dp only float
  test pressure dp only float
  valve mechanism dp only string
  valve operation dp only string
  valve pattern dp only string

### vibration isolatorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/def/bldg#VibrationIsolator

has super-classes
  maximum supported weight dp only float
  height dp only float
  vibration transmissibility dp only float
  isolator static deflection dp only float
  isolator compressibility dp only float

## Object Properties

- air flow rate range
- short circuit voltage

### air flow rate rangeop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/def/bldg#airFlowRateRange

Possible range of airflow that can be delivered. For cases where there is no airflow across the coil (e.g. electric coil in a floor slab), then the value is zero. Usually measured in m3/s.

has range
  real real range c
is also defined as
  data property

### short circuit voltageop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/def/bldg#shortCircuitVoltage

A complex number that specifies the real and imaginary parts of the short-circuit voltage at rated current of a transformer given in %.

has range
  complex number c
is also defined as
  data property

## Data Properties

- access type
- air flow rate range
- ambient design dry bulb temperature
- ambient design wet bulb temperature
- application
- arrangement
- audio volume
- basin reserve volume
- blade action
- blade edge
- blade shape
- blade thickness
- body mass
- capacity control
- capacity control type
- capacity people
- capacity weight
- circuit type
- close off rating
- coil length
- coil width
- color appearance
- color rendering index
- color tempeature
- compressor speed
- connection size
- contributed luminous flux
- control strategy
- cover length
- cover width
- effective capacity
- electric generator efficiency
- electric motor efficiency
- end shape type
- energy source
- evaporation coolant
- evaporation medium type
- external surface area
- face area
- fail position
- final resistance
- finish color
- fire exit
- first curvature radius
- flow arrangement
- flow coefficient
- flow rate range
- flow resistance range
- fouling factor
- frame depth
- frame size
- frame thickness
- frame type
- has defrost
- has exterior insulation
- has hot gas bypass
- has lock
- has part winding
- has turbulator
- heat exchange area
- heat transfer dimension
- heat transfer medium
- heat transfer surface area
- heat transfer type enum
- height
- horizontal spacing
- hydraulic diameter
- ideal capacity
- ideal shaft power
- imaginary impedance ratio
- impeller diameter
- in line row spacing
- initial resistance
- inlet connection size
- inside diameter
- integrated lighting type
- internal control
- internal refrigerant volume
- internal surface area
- internal water volume
- is external
- is free hanging
- is guarded
- is illuminated
- is neutral primary terminal available
- is neutral secondary terminal available
- is pluggable outlet
- is water storage heater
- isolator compressibility
- isolator static deflection
- lamp ballast type
- lamp compensation type
- lamp maintenance factor
- leakage fully closed
- legend
- length
- lift elevation difference
- light emitter nominal power
- limiting terminal size
- locked rotor current
- manual override
- maximum air flow rate
- maximum apparent power
- maximum part load ratio
- maximum power output
- maximum supported weight
- maximum working pressure
- mechanical operated
- media source
- minimun part load ratio
- motor drive type
- motor enclosure type
- net positive suction head
- nominal air flow rate
- nominal body depth
- nominal body length
- nominal body width
- nominal capacity
- nominal capcity
- nominal condensing temperature
- nominal cooling capacity
- nominal depth
- nominal diameter
- nominal efficiency
- nominal energy consumption
- nominal evaporating temmperature
- nominal filter face velocity
- nominal flow rate
- nominal frequency
- nominal heat rejection rate
- nominal heat transfer area
- nominal heat transfer coefficient
- nominal heating capacity
- nominal latent capacity
- nominal length or diameter
- nominal media surface velocity
- nominal moisture gain
- nominal part load ratio
- nominal particle geometric mean diameter
- nominal particle geometric standard deviation
- nominal power consumption
- nominal power rate
- nominal pressure drop
- nominal return water temperature cooling
- nominal return water temperature heating
- nominal rotation speed
- nominal sensible capacity
- nominal sorrounding humidity cooling
- nominal sorrounding temperature cooling
- nominal sorrounding temperature heating
- nominal static pressure
- nominal supply voltage
- nominal supply voltage offset
- nominal supply water temperature cooling
- nominal supply water temperature heating
- nominal total pressure
- nominal ua
- nominal water flow cooling
- nominal water flow heating
- nominal width or diameter
- nomminal rotation speed
- number of blades
- number of cells
- number of circuits
- number of gangs
- number of panels
- number of rows
- number of sections
- number os sockets
- open pressure drop
- operating mode
- operating wight
- operation
- operation temperature range
- operational riterial
- operational temperature range
- orientation
- outlet connection size
- outlet temperature range
- output capacity
- outside diameter
- pattern type
- pipe connection enum
- placement type
- power source
- pressure rating
- primary air flow rate range
- primary apparent power
- primary current
- primary frequency
- primary voltage
- read out type
- real impedance ratio
- refrigerant class
- remote reading
- roughness
- second curvature radius
- secondary air flow rate range
- secondary apparent power
- secondary current
- secondary current type
- secondary frequency
- secondary voltage
- shading device type
- short circuit voltage
- size
- solar reflectance
- solar transmittance
- spectrum
- spray type
- staggered row spacing
- standard
- start current factor
- starting time
- storage type
- switch function
- te time
- temperature classification
- temperature range
- temperature rating
- test pressure
- thermal conductivity
- thermal efficiency
- thermal mass heat capacity
- thermal transmittance
- transformer vector group
- valve mechanism
- valve operation
- valve pattern
- ventilating pipe size
- vertical spacing
- vibration transmissibility
- visible light reflectance
- visible light transmittance
- volumen
- water flow control system type
- water inlet temperature range
- water pressure range
- water requirement
- water storage capacity
- weight
- working pressure
- working pressure range

### access typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#accessType

Defines the types of access (or cover) to a tank that may be specified. Note that covers are generally specified for rectangular tanks. For cylindrical tanks, access will normally be via a manhole.

has range
  string

### air flow rate rangeop back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#airFlowRateRange

Possible range of airflow that can be delivered. For cases where there is no airflow across the coil (e.g. electric coil in a floor slab), then the value is zero. Usually measured in m3/s.

is also defined as
  object property

### ambient design dry bulb temperaturedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#ambientDesignDryBulbTemperature

Ambient design dry bulb temperature used for selecting the cooling tower. Usually measured in degrees Kelvin (K).

has range
  float

### ambient design wet bulb temperaturedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#ambientDesignWetBulbTemperature

Ambient design wet bulb temperature used for selecting the cooling tower. Usually measured in degrees Kelvin (K).

has range
  float

### applicationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#application

Humidifier application. Fixed: Humidifier installed in a ducted flow distribution system. Portable: Humidifier is not installed in a ducted flow distribution system.

has range
  string

### arrangementdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#arrangement

Defines the basic flow arrangements for the heat exchanger: COUNTERFLOW: Counterflow heat exchanger arrangement. CROSSFLOW: Crossflow heat exchanger arrangement. PARALLELFLOW: Parallel flow heat exchanger arrangement. MULTIPASS: Multipass flow heat exchanger arrangement. OTHER: Other type of heat exchanger flow arrangement not defined above.

has range
  string

### audio volumedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#audioVolume

Indicates discrete audio volume levels and corresponding sound power offsets, if applicable. Missing values may be interpolated. Measured in watts.

has range
  float

### basin reserve volumedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#basinReserveVolume

Volume between operating and overflow levels in cooling tower basin. Usually measured in cubic metre (m3).

has range
  float

### blade actiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#bladeAction

Blade action.

has range
  string

### blade edgedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#bladeEdge

Blade edge.

has range
  string

### blade shapedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#bladeShape

Blade shape. Flat means triple V-groove.

has range
  string

### blade thicknessdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#bladeThickness

The thickness of the damper blade. Usually measured in millimeters (mm).

has range
  float

### body massdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#bodyMass

Overall body mass of the heater. Usually measured in kilograms (kg) or grams (g).

has range
  float

### capacity controldp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#capacityControl

FanCycling: Fan is cycled on and off to control duty. TwoSpeedFan: Fan is switched between low and high speed to control duty. VariableSpeedFan: Fan speed is varied to control duty. DampersControl: Dampers modulate the air flow to control duty. BypassValveControl: Bypass valve modulates the water flow to control duty. MultipleSeriesPumps: Turn on/off multiple series pump to control duty. TwoSpeedPump: Switch between high/low pump speed to control duty. VariableSpeedPump: vary pump speed to control duty.

has range
  string

### capacity control typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#capacityControlType

InletVane: Control by adjusting inlet vane. VariableSpeedDrive: Control by variable speed drive. BladePitchAngle: Control by adjusting blade pitch angle. TwoSpeed: Control by switch between high and low speed. DischargeDamper: Control by modulating discharge damper.

has range
  string

### capacity peopledp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#capacityPeople

capacity of the transportation element measured in numbers of person.

has range
  positive integer

### capacity weightdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#capacityWeight

Capacity of the transport element measured by weight. Usually measured in kilograms (kg) or grams (g).

has range
  float

### circuit typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#circuitType

OpenCircuit: Exposes water directly to the cooling atmosphere. CloseCircuit: The fluid is separated from the atmosphere by a heat exchanger. Wet: The air stream or the heat exchange surface is evaporatively cooled. Dry: No evaporation into the air stream. DryWet: A combination of a dry tower and a wet tower.

has range
  string

### close off ratingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#closeOffRating

Close off rating. Usually measured in Pascals (Pa, N/m2).

has range
  float

### coil lengthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#coilLength

Length of coil. Usually measured in millimeters (mm).

has range
  float

### coil widthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#coilWidth

Width of coil. Usually measured in millimeters (mm

has range
  float

### color appearancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#colorAppearance

In both the DIN and CIE standards, artificial light sources are classified in terms of their color appearance. To the human eye they all appear to be white the difference can only be detected by direct comparison. Visual performance is not directly affected by differences in color appearance.

has range
  string

### color rendering indexdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#colorRenderingIndex

The CRI indicates how well a light source renders eight standard colors compared to perfect reference lamp with the same color temperature. The CRI scale ranges from 1 to 100, with 100 representing perfect rendering properties.

has range
  integer

### color tempeaturedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#colorTempeature

The color temperature of any source of radiation is defined as the temperature (in Kelvin) of a black-body or Planckian radiator whose radiation has the same chromaticity as the source of radiation. Often the values are only approximate color temperatures as the black-body radiator cannot emit radiation of every chromaticity value. The color temperatures of the commonest artificial light sources range from less than 3000K (warm white) to 4000K (intermediate) and over 5000K (daylight). Usually measured in degrees Kelvin (K).

has range
  float

### compressor speeddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#compressorSpeed

Compressor speed. Usually measured in cycles/s.

has range
  float

### connection sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#connectionSize

The connection size of the to and from the pump. Usually measured in millimeters (mm).

has range
  float

### contributed luminous fluxdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#contributedLuminousFlux

Luminous flux is a photometric measure of radiant flux, i.e. the volume of light emitted from a light source. Luminous flux is measured either for the interior as a whole or for a part of the interior (partial luminous flux for a solid angle). All other photometric parameters are derivatives of luminous flux. Luminous flux is measured in lumens (lm). The luminous flux is given as a nominal value for each lamp. Usually measured in Lumen (lm, Candela Steradian).

has range
  float

### control strategydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#controlStrategy

FixedExitingWaterTemp: The capacity is controlled to maintain a fixed exiting water temperature. WetBulbTempReset: The set-point is reset based on the wet-bulb temperature.

has range
  string

### cover lengthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#coverLength

The length measured along the x-axis in the local coordinate system or the radius (in the case of a circular shape in plan) of the cover of the oil interceptor. Usually measured in millimeters (mm).

has range
  float

### cover widthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#coverWidth

The length measured along the x-axis in the local coordinate system of the cover of the oil interceptor. Usually measured in millimeters (mm).

has range
  float

### effective capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#effectiveCapacity

The total effective or actual volumetric capacity of the tank. Usually measured in cubic metre (m3).B3

has range
  float

### electric generator efficiencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#electricGeneratorEfficiency

the ratio of output capacity to intake capacity.

has range
  float

### electric motor efficiencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#electricMotorEfficiency

The ratio of output capacity to intake capacity.

has range
  float

### end shape typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#endShapeType

Defines the types of end shapes that can be used for preformed tanks. The convention for reading these enumerated values is that for a vertical cylinder, the first value is the base and the second is the top for a horizontal cylinder, the order of reading should be left to right. For a speherical tank, the value UNSET should be used.B5

has range
  string

### energy sourcedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#energySource

Enumeration defining the energy source or fuel combusted to generate heat if applicable. Note: hydronic heaters shall use UNSET, dual-use hydronic/electric heaters shall use ELECTRICITY.

has range
  string

### evaporation coolantdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#evaporationCoolant

The fluid used for the coolant in the evaporator.

has range
  string

### evaporation medium typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#evaporationMediumType

ColdLiquid: Evaporator is using liquid type of fluid to exchange heat with refrigerant. ColdAir: Evaporator is using air to exchange heat with refrigerant.

has range
  string

### external surface areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#externalSurfaceArea

External surface area (both primary and secondary area). Usually measured in square metre (m2).

has range
  float

### face areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#faceArea

Face area open to the airstream. Usually measured in square metre (m2).

has range
  float

### fail positiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#failPosition

Specifies the required fail-safe position of the actuator.

has range
  string

### final resistancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#finalResistance

Filter fluid resistance when replacement is required (i.e., Pressure drop at the maximum air flowrate across the filter when the filter needs replacement per ASHRAE Standard 52.1). Usually measured in Pascals (Pa, N/m2).

has range
  float

### finish colordp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#finishColor

Finish color for cooled beam.

has range
  string

### fire exitdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#fireExit

Indication whether this object is designed to serve as an exit in the case of fire (TRUE) or not (FALSE). Here whether the transport element (in case of e.g., a lift) is designed to serve as a fire exit, e.g., for fire escape purposes.

has range
  boolean

### first curvature radiusdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#firstCurvatureRadius

FirstCurvatureRadius should be defined as the base or left side radius of curvature value. Usually measured in millimeters (mm).

has range
  float

### flow arrangementdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#flowArrangement

CounterFlow: Air and water flow enter in different directions. CrossFlow: Air and water flow are perpendicular. ParallelFlow: air and water flow enter in same directions.

has range
  string

### flow coefficientdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#flowCoefficient

Flow coefficient (the quantity of fluid that passes through a fully open valve at unit pressure drop), typically expressed as the Kv or Cv value for the valve.

has range
  float

### flow rate rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#flowRateRange

Allowable range of volume of fluid being pumped against the resistance specified. Usually measured in kg/s.

has range
  real real range c

### flow resistance rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#flowResistanceRange

Allowable range of frictional resistance against which the fluid is being pumped. Usually measured in Pascals (Pa, N/m2).

has range
  real real range c

### fouling factordp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#foulingFactor

Fouling factor of the tubes in the tube bundle. Usually measured in m2 Kelvin/Watt.

has range
  float

### frame depthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#frameDepth

The length (or depth) of the damper frame. Usually measured in millimeters (mm).

has range
  float

### frame sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#frameSize

Designation of the frame size according to the named range of frame sizes designated at the place of use or according to a given standard.

has range
  string

### frame thicknessdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#frameThickness

The thickness of the damper frame material. Usually measured in millimeters (mm).

has range
  float

### frame typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#frameType

The type of frame used by the damper (e.g., Standard, Single Flange, Single Reversed Flange, Double Flange, etc.).

has range
  string

### has defrostdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasDefrost

has the heat exchanger has defrost function or not.

has range
  boolean

### has exterior insulationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasExteriorInsulation

TRUE if the silencer has exterior insulation. FALSE if it does not.

has range
  boolean

### has hot gas bypassdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasHotGasBypass

Whether or not hot gas bypass is provided for the compressor. TRUE = Yes, FALSE = No.

has range
  boolean

### has lockdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasLock

Indication of whether a switching device has a key operated lock (=TRUE) or not (= FALSE).

has range
  boolean

### has part windingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasPartWinding

Indication of whether the motor is single speed, i.e. has a single winding (= FALSE) or multi-speed i.e.has part winding (= TRUE) .

has range
  boolean

### has turbulatordp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hasTurbulator

TRUE if the tube has a turbulator, FALSE if it does not.

has range
  boolean

### heat exchange areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#heatExchangeArea

Heat exchange area. Usually measured in square metre (m2).

has range
  float

### heat transfer dimensiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#heatTransferDimension

Indicates how heat is transmitted according to the shape of the space heater.

has range
  string

### heat transfer mediumdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#heatTransferMedium

Enumeration defining the heat transfer medium if applicable.

has range
  string

### heat transfer surface areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#heatTransferSurfaceArea

Total heat transfer area of the vessel. Usually measured in square metre (m2).

has range
  float

### heat transfer type enumdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#heatTransferTypeEnum

Type of heat transfer between the two air streams.

has range
  string

### heightdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#height

Height of the vibration isolator before tha application of load. Usually measured in millimeters (mm).

has range
  float

### horizontal spacingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#horizontalSpacing

Horizontal spacing between tubes in the tube bundle. Usually measured in millimeters (mm).

has range
  float

### hydraulic diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#hydraulicDiameter

Hydraulic diameter. Usually measured in millimeters (mm).

has range
  float

### ideal capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#idealCapacity

Compressor capacity under ideal conditions. Usually measured in Watts (W, J/s).

has range
  float

### ideal shaft powerdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#idealShaftPower

Compressor shaft power under ideal conditions. Usually measured in Watts (W, J/s).

has range
  float

### imaginary impedance ratiodp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#imaginaryImpedanceRatio

The ratio between the imaginary part of the zero sequence impedance and the imaginary part of the positive impedance (i.e. imaginary part of the short-circuit voltage) of the transformer. Used for three-phase transformer which includes a N-conductor.

has range
  float

### impeller diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#impellerDiameter

Diameter of compressor impeller - used to scale performance of geometrically similar compressors. Usually measured in millimeters (mm).

has range
  float

### in line row spacingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#inLineRowSpacing

In-line tube row spacing. Usually measured in millimeters (mm).

has range
  float

### initial resistancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#initialResistance

Initial new filter fluid resistance (i.e., pressure drop at the maximum air flowrate across the filter when the filter is new per ASHRAE Standard 52.1). Usually measured in Pascals (Pa, N/m2).

has range
  float

### inlet connection sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#inletConnectionSize

Size of the inlet connection. Usually measured in millimeters (mm).

has range
  float

### inside diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#insideDiameter

Actual inner diameter of the tube in the tube bundle. Usually measured in millimeters (mm).

has range
  float

### integrated lighting typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#integratedLightingType

Integrated lighting in cooled beam.

has range
  string

### internal controldp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#internalControl

Internal modulation control.

has range
  string

### internal refrigerant volumedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#internalRefrigerantVolume

Internal volume of condenser (refrigerant side). Usually measured in cubic metre (m3).

has range
  float

### internal surface areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#internalSurfaceArea

Internal surface area. Usually measured in square metre (m2).

has range
  float

### internal water volumedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#internalWaterVolume

Internal volume of condenser (water side). Usually measured in cubic metre (m3).

has range
  float

### is externaldp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isExternal

Indication whether the element is designed for use in the exterior (TRUE) or not (FALSE). If (TRUE) it is an external element and faces the outside of the building.

has range
  boolean

### is free hangingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isFreeHanging

Is it free hanging type (not mounted in a false ceiling)?

has range
  boolean

### is guardeddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isGuarded

Indication of whether the motor enclosure is guarded (= TRUE) or not (= FALSE).

has range
  boolean

### is illuminateddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isIlluminated

An indication of whether there is an illuminated indicator to show that the switch is on (=TRUE) or not (= FALSE).

has range
  boolean

### is neutral primary terminal availabledp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isNeutralPrimaryTerminalAvailable

An indication of whether the neutral point of the primary winding is available as a terminal (=TRUE) or not (= FALSE).

has range
  boolean

### is neutral secondary terminal availabledp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isNeutralSecondaryTerminalAvailable

An indication of whether the neutral point of the secondary winding is available as a terminal (=TRUE) or not (= FALSE).

has range
  boolean

### is pluggable outletdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isPluggableOutlet

Indication of whether the outlet accepts a loose plug connection (= TRUE) or whether it is directly connected (= FALSE) or whether the form of connection has not yet been determined (= UNKNOWN).

has range
  boolean

### is water storage heaterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isWaterStorageHeater

This is used to identify if the boiler has storage capacity (TRUE). If FALSE, then there is no storage capacity built into the boiler, such as an instantaneous hot water heater.

has range
  boolean

### isolator compressibilitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isolatorCompressibility

The compressibility of the vibration isolator.

has range
  float

### isolator static deflectiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#isolatorStaticDeflection

Static deflection of the vibration isolator. Usually measured in millimeters (mm).

has range
  float

### lamp ballast typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#lampBallastType

The type of ballast used to stabilise gas discharge by limiting the current during operation and to deliver the necessary striking voltage for starting. Ballasts are needed to operate Discharge Lamps such as Fluorescent, Compact Fluorescent, High-pressure Mercury, Metal Halide and High-pressure Sodium Lamps. Magnetic ballasts are chokes which limit the current passing through a lamp connected in series on the principle of self-induction. The resultant current and power are decisive for the efficient operation of the lamp. A specially designed ballast is required for every type of lamp to comply with lamp rating in terms of Luminous Flux, Color Appearance and service life. The two types of magnetic ballasts for fluorescent lamps are KVG Conventional (EC-A series) and VVG Low-loss ballasts (EC-B series). Low-loss ballasts have a higher efficiency, which means reduced ballast losses and a lower thermal load. Electronic ballasts are used to run fluorescent lamps at high frequencies (approx. 35 - 40 kHz).

has range
  string

### lamp compensation typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#lampCompensationType

Identifies the form of compensation used for power factor correction and radio suppression.

has range
  string

### lamp maintenance factordp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#lampMaintenanceFactor

Non recoverable losses of luminous flux of a lamp due to lamp depreciation i.e. the decreasing of light output of a luminaire due to aging and dirt.

has range
  float

### leakage fully closeddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#leakageFullyClosed

Leakage when fully closed. Usually measured in m3/s.

has range
  float

### legenddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#legend

A text inscribed or applied to the switch as a legend to indicate purpose or function.

has range
  string

### lengthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#length

Length of the tubes in the tube bundle. Usually measured in millimeters (mm).

has range
  float

### lift elevation differencedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#liftElevationDifference

Elevation difference between cooling tower sump and the top of the tower. Usually measured in millimeters (mm).

has range
  float

### light emitter nominal powerdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#lightEmitterNominalPower

Light emitter nominal power. Usually measured in Watts (W, J/s).

has range
  float

### limiting terminal sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#limitingTerminalSize

The maximum terminal size capacity of the device. Usually measured in square metre (m2).

has range
  float

### locked rotor currentdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#lockedRotorCurrent

Input current when a motor armature is energized but not rotating. Usually measured in Ampere (A).

has range
  float

### manual overridedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#manualOverride

Identifies whether hand-operated operation is provided as an override (= TRUE) or not (= FALSE). Note that this value should be set to FALSE by default in the case of a Hand Operated Actuator.

has range
  boolean

### maximum air flow ratedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumAirFlowRate

Maximum allowable air flow rate. Usually measured in m3/s.

has range
  float

### maximum apparent powerdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumApparentPower

Maximum apparent power/capacity in VA (volt ampere). Usually measured in Watts (W, J/s).

has range
  float

### maximum part load ratiodp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumPartLoadRatio

Maximum part load ratio as a fraction of nominal capacity.

has range
  float

### maximum power outputdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumPowerOutput

The maximum output power rating of the engine. Usually measured in Watts (W, J/s).

has range
  float

### maximum supported weightdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumSupportedWeight

The maximum weight that can be carried by the vibration isolator. Usually measured in kilograms (kg) or grams (g).

has range
  float

### maximum working pressuredp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#maximumWorkingPressure

Maximum working pressure. Usually measured in Pascals (Pa, N/m2).

has range
  float

### mechanical operateddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#mechanicalOperated

Indication whether the element is operated machanically (TRUE) or not, i.e. manually (FALSE).

has range
  boolean

### media sourcedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#mediaSource

Indicates media sources and corresponding names of ports (IfcDistributionPort with FlowDirection=SINK and PredefinedType=AUDIOVISUAL) or aggregated audio/video components (IfcAudioVisualAppliance).

has range
  string

### minimun part load ratiodp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#minimunPartLoadRatio

Minimum part load ratio as a fraction of nominal capacity.

has range
  float

### motor drive typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#motorDriveType

Motor drive type: DIRECTDRIVE: Direct drive. BELTDRIVE: Belt drive. COUPLING: Coupling. OTHER: Other type of motor drive. UNKNOWN: Unknown motor drive type.

has range
  string

### motor enclosure typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#motorEnclosureType

A list of the available types of motor enclosure from which that required may be selected.

has range
  string

### net positive suction headdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#netPositiveSuctionHead

Minimum liquid pressure at the pump inlet to prevent cavitation. Usually measured in Pascals (Pa, N/m2).

has range
  float

### nominal air flow ratedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalAirFlowRate

Nominal air flow rate. Usually measured in m3/s.

has range
  float

### nominal body depthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalBodyDepth

Nominal or quoted =length, measured along the z-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).

has range
  float

### nominal body lengthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalBodyLength

Nominal or quoted length, measured along the x-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).

has range
  float

### nominal body widthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalBodyWidth

Nominal or quoted length, measured along the y-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).

has range
  float

### nominal capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalCapacity

Compressor nameplate capacity. Usually measured in Watts (W, J/s).

has range
  float

### nominal capcitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalCapcity

Nominal cooling tower capacity in terms of heat transfer rate of the cooling tower between air stream and water stream at nominal conditions. Usually measured in Watts (W, J/s).

has range
  float

### nominal condensing temperaturedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalCondensingTemperature

Chiller condensing temperature. Usually measured in degrees Kelvin (K).

has range
  float

### nominal cooling capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalCoolingCapacity

Nominal cooling capacity. Usually measured in Watts (W, J/s).

has range
  float

### nominal depthdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalDepth

The nominal depth of the tank. Note: Not required for a horizontal cylindrical tank. Usually measured in millimeters (mm).

has range
  float

### nominal diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalDiameter

Nominal diameter or width of the tubes in the tube bundle. Usually measured in millimeters (mm).

has range
  float

### nominal efficiencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalEfficiency

Nominal chiller efficiency under nominal conditions.

has range
  float

### nominal energy consumptiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalEnergyConsumption

Nominal fuel consumption rate required to produce the total boiler heat output. Usually measured in Watts (W, J/s).

has range
  float

### nominal evaporating temmperaturedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalEvaporatingTemmperature

Chiller evaporating temperature.Usually measured in degrees Kelvin (K).

has range
  float

### nominal filter face velocitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalFilterFaceVelocity

Filter face velocity. Usually measured in m/s.

has range
  float

### nominal flow ratedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalFlowRate

Nominal fluid flow rate through the filter. Usually measured in m3/s.

has range
  float

### nominal frequencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalFrequency

The nominal frequency of the supply. Usually measured in cycles/s or Hertz (Hz).

has range
  float

### nominal heat rejection ratedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalHeatRejectionRate

Sum of the refrigeration effect and the heat equivalent of the power input to the compressor. Usually measured in Watts (W, J/s).

has range
  float

### nominal heat transfer areadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalHeatTransferArea

Nominal heat transfer surface area associated with nominal overall heat transfer coefficient. Usually measured in square metre (m2).

has range
  float

### nominal heat transfer coefficientdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalHeatTransferCoefficient

Nominal overall heat transfer coefficient associated with nominal heat transfer area. Usually measured in Watts/m2 Kelvin.

has range
  float

### nominal heating capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalHeatingCapacity

Nominal heating capacity. Usually measured in Watts (W, J/s).

has range
  float

### nominal latent capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalLatentCapacity

Nominal latent capacity. Usually measured in Watts (W, J/s).

has range
  float

### nominal length or diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalLengthOrDiameter

The nominal length or, in the case of a vertical cylindrical tank, the nominal diameter of the tank. Usually measured in millimeters (mm).

has range
  float

### nominal media surface velocitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalMediaSurfaceVelocity

Average fluid velocity at the media surface. Usually measured in m/s.

has range
  float

### nominal moisture gaindp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalMoistureGain

Nominal rate of water vapor added into the airstream. Usually measured in kg/s.

has range
  float

### nominal part load ratiodp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalPartLoadRatio

Allowable part load ratio range.

has range
  real real range c

### nominal particle geometric mean diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalParticleGeometricMeanDiameter

Particle geometric mean diameter associated with nominal efficiency. Usually measured in millimeters (mm).

has range
  float

### nominal particle geometric standard deviationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalParticleGeometricStandardDeviation

Particle geometric standard deviation associated with nominal efficiency.

has range
  float

### nominal power consumptiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalPowerConsumption

Nominal total power consumption. Usually measured in Watts (W, J/s).

has range
  float

### nominal power ratedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalPowerRate

Nominal fan power rate.Usually measured in Watts (W, J/s).

has range
  float

### nominal pressure dropdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalPressureDrop

Total pressure drop across the filter. Usually measured in Pascals (Pa, N/m2).

has range
  float

### nominal return water temperature coolingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalReturnWaterTemperatureCooling

Nominal return water temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal return water temperature heatingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalReturnWaterTemperatureHeating

Nominal return water temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal rotation speeddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalRotationSpeed

Nominal fan wheel speed. Usually measured in cycles/s.

has range
  float

### nominal sensible capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSensibleCapacity

Nominal sensible capacity. Usually measured in Watts (W, J/s).

has range
  float

### nominal sorrounding humidity coolingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSorroundingHumidityCooling

Nominal surrounding humidity (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal sorrounding temperature coolingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSorroundingTemperatureCooling

Nominal surrounding temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal sorrounding temperature heatingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSorroundingTemperatureHeating

Nominal surrounding temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal static pressuredp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalStaticPressure

The static pressure within the air stream that the fan must overcome to insure designed circulation of air. Usually measured in Pascals (Pa, N/m2).

has range
  float

### nominal supply voltagedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSupplyVoltage

The nominal voltage of the supply. Usually measured in Volts (V, W/A).

has range
  float

### nominal supply voltage offsetdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSupplyVoltageOffset

The maximum and minimum allowed voltage of the supply e.g. boundaries of 380V/440V may be applied for a nominal voltage of 400V.

has range
  real real range c

### nominal supply water temperature coolingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSupplyWaterTemperatureCooling

Nominal supply water temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal supply water temperature heatingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalSupplyWaterTemperatureHeating

Nominal supply water temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).

has range
  float

### nominal total pressuredp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalTotalPressure

Nominal total pressure rise across the fan. Usually measured in Pascals (Pa, N/m2).

has range
  float

### nominal uadp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalUa

Nominal UA value.

has range
  float

### nominal water flow coolingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalWaterFlowCooling

Nominal water flow (refers to nominal cooling capacity). Usually measured in m3/s.

has range
  float

### nominal water flow heatingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalWaterFlowHeating

Nominal water flow (refers to nominal heating capacity). Usually measured in m3/s.

has range
  float

### nominal width or diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nominalWidthOrDiameter

The nominal width or, in the case of a horizontal cylindrical tank, the nominal diameter of the tank. Note: Not required for a vertical cylindrical tank. Usually measured in millimeters (mm).

has range
  float

### nomminal rotation speeddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#nomminalRotationSpeed

Pump rotational speed under nominal conditions. Usually measured in cycles/s.

has range
  float

### number of bladesdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfBlades

Number of blades.

has range
  integer

### number of cellsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfCells

Number of cells in one cooling tower unit.

has range
  integer

### number of circuitsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfCircuits

Number of parallel fluid tube circuits.

has range
  integer

### number of gangsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfGangs

Number of gangs/buttons on this switch.

has range
  integer

### number of panelsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfPanels

Number of panels.

has range
  integer

### number of rowsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfRows

Number of tube rows in the tube bundle assembly.

has range
  integer

### number of sectionsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOfSections

Number of sections used in the construction of the tank. Default is 1. Note: All sections assumed to be the same size.

has range
  integer

### number os socketsdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#numberOsSockets

The number of sockets that may be connected. In case of inconsistency, sockets defined on ports take precedence.

has range
  integer

### open pressure dropdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#openPressureDrop

Total pressure drop across damper. Usually measured in Pascals (Pa, N/m2).

has range
  float

### operating modedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operatingMode

Identifies the operating mode of the boiler.

has range
  string

### operating wightdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operatingWight

Operating weight of the tank including all of its contents. Usually measured in kilograms (kg) or grams (g).

has range
  float

### operationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operation

The operational mechanism for the damper operation.

has range
  string

### operation temperature rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operationTemperatureRange

Allowable operation ambient air temperature range. Usually measured in degrees Kelvin (K).

has range
  float
  real real range c

### operational riterialdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operationalRiterial

Time of operation at maximum operational ambient air temperature. Measured in seconds (s) or days (d) or other units of time.

has range
  float

### operational temperature rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#operationalTemperatureRange

Allowable operation ambient air temperature range. Usually measured in degrees Kelvin (K).

has range
  real real range c

### orientationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#orientation

The intended orientation for the damper as specified by the manufacturer.

has range
  string

### outlet connection sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#outletConnectionSize

Size of the outlet connection. Usually measured in millimeters (mm).

has range
  float

### outlet temperature rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#outletTemperatureRange

Allowable outlet temperature of either the water or the steam. Usually measured in degrees Kelvin (K).

has range
  real real range c

### output capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#outputCapacity

Total nominal heat output as listed by the manufacturer. Usually measured in Watts (W, J/s).

has range
  float

### outside diameterdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#outsideDiameter

Actual outside diameter of the tube in the tube bundle. Usually measured in millimeters (mm).

has range
  float

### pattern typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#patternType

Defines the types of pattern (or shape of a tank that may be specified.

has range
  string

### pipe connection enumdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#pipeConnectionEnum

The manner in which the pipe connection is made to the cooled beam.

has range
  string

### placement typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#placementType

Indicates the placement of the coil. FLOOR indicates an under floor heater (if coil type is WATERHEATINGCOIL or ELECTRICHEATINGCOIL), CEILING indicates a cooling ceiling (if coil type is WATERCOOLINGCOIL), UNIT indicates that the coil is part of a cooling or heating unit, like cooled beam, etc.

has range
  string

### power sourcedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#powerSource

Type of power driving the compressor.

has range
  string

### pressure ratingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#pressureRating

Nominal pressure rating of the boiler as rated by the agency having jurisdiction. Usually measured in Pascals (Pa, N/m2).

has range
  float

### primary air flow rate rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#primaryAirFlowRateRange

possible range of primary airflow that can be delivered. Usually measured in m3/s.

has range
  real real range c

### primary apparent powerdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#primaryApparentPower

The power in VA (volt ampere) that has been transformed and that runs into the transformer on the primary side. Usually measured in Watts (W, J/s).

has range
  float

### primary currentdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#primaryCurrent

The current that is going to be transformed and that runs into the transformer on the primary side. Usually measured in Ampere (A).

has range
  float

### primary frequencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#primaryFrequency

The frequency that is going to be transformed and that runs into the transformer on the primary side. Usually measured in cycles/s or Hertz (Hz).

has range
  float

### primary voltagedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#primaryVoltage

The voltage that is going to be transformed and that runs into the transformer on the primary side. Usually measured in Volts (V, W/A).

has range
  float

### read out typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#readOutType

Indication of the form that readout from the meter takes. In the case of a dial read out, this may comprise multiple dials that give a cumulative reading and/or a mechanical odometer.

has range
  string

### real impedance ratiodp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#realImpedanceRatio

The ratio between the real part of the zero sequence impedance and the real part of the positive impedance (i.e. real part of the short-circuit voltage) of the transformer. Used for three-phase transformer which includes a N-conductor.

has range
  float

### refrigerant classdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#refrigerantClass

Refrigerant class used by the compressor. CFC: Chlorofluorocarbons. HCFC: Hydrochlorofluorocarbons. HFC: Hydrofluorocarbons.

has range
  string

### remote readingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#remoteReading

Indicates whether the meter has a connection for remote reading through connection of a communication device (set TRUE) or not (set FALSE).

has range
  boolean

### roughnessdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#roughness

A measure of the vertical deviations of the surface.

has range
  string

### second curvature radiusdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondCurvatureRadius

SecondCurvatureRadius should be defined as the top or right side radius of curvature value. Usually measured in millimeters (mm).

has range
  float

### secondary air flow rate rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryAirFlowRateRange

possible range of secondary airflow that can be delivered. Usually measured in Pascals (Pa, N/m2).

has range
  real real range c

### secondary apparent powerdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryApparentPower

The power in VA (volt ampere) that has been transformed and is running out of the transformer on the secondary side. Usually measured in Watts (W, J/s).

has range
  float

### secondary currentdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryCurrent

The current that has been transformed and is running out of the transformer on the secondary side. Usually measured in Ampere (A).

has range
  float

### secondary current typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryCurrentType

A list of the secondary current types that can result from transformer output.

has range
  string

### secondary frequencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryFrequency

The frequency that has been transformed and is running out of the transformer on the secondary side. Usually measured in cycles/s or Hertz (Hz).

has range
  float

### secondary voltagedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#secondaryVoltage

The voltage that has been transformed and is running out of the transformer on the secondary side. Usually measured in Volts (V, W/A).

has range
  float

### shading device typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#shadingDeviceType

Specifies the type of shading device.

has range
  string

### short circuit voltageop back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#shortCircuitVoltage

A complex number that specifies the real and imaginary parts of the short-circuit voltage at rated current of a transformer given in %.

is also defined as
  object property

### sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#size

The size of the connection to the valve (or to each connection for faucets, mixing valves, etc.). Usually measured in millimeters (mm).

has range
  float

### solar reflectancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#solarReflectance

(Rsol): The ratio of incident solar radiation that is reflected by a shading system (also named _e). Note the following equation Asol + Rsol + Tsol = 1

has range
  float

### solar transmittancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#solarTransmittance

(Tsol) The ratio of incident solar radiation that directly passes through a shading system (also named _e). Note the following equation Asol + Rsol + Tsol = 1

has range
  float

### spectrumdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#spectrum

The spectrum of radiation describes its composition with regard to wavelength. Light, for example, as the portion of electromagnetic radiation that is visible to the human eye, is radiation with wavelengths in the range of approx. 380 to 780 nm (1 nm = 10 m). The corresponding range of colours varies from violet to indigo, blue, green, yellow, orange, and red. These colours form a continuous spectrum, in which the various spectral sectors merge into each other.

has range
  real real range c

### spray typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#sprayType

SprayFilled: Water is sprayed into airflow. SplashTypeFill: water cascades over successive rows of splash bars. FilmTypeFill: water flows in a thin layer over closely spaced sheets.

has range
  string

### staggered row spacingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#staggeredRowSpacing

Staggered tube row spacing. Usually measured in millimeters (mm).

has range
  float

### standarddp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#standard

the designation of the Standard applicable for the definition of the characteristics of the tripping_unit.

has range
  string

### start current factordp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#startCurrentFactor

IEC. Start current factor defines how large the peek starting current will become on the engine. StartCurrentFactor is multiplied to NominalCurrent and we get the start current.

has range
  float

### starting timedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#startingTime

The time (in s) needed for the motor to reach its rated speed with its driven equipment attached, starting from standstill and at the nominal voltage applied at its terminals.

has range
  float

### storage typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#storageType

Defines the general material category intended to be stored.

has range
  string

### switch functiondp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#switchFunction

Indicates types of switches which differs in functionality.

has range
  string

### te timedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#teTime

The maximum time (in s) at which the motor could run with locked rotor when the motor is used in an EX-environment. The time indicates that a protective device should trip before this time when the starting current of the motor is slowing through the device.

has range
  float

### temperature classificationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#temperatureClassification

Enumeration defining the temperature classification of the space heater surface temperature. low temperature - surface temperature is relatively low, usually heated by hot water or electricity. high temperature - surface temperature is relatively high, usually heated by gas or steam.

has range
  string

### temperature rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#temperatureRange

Allowable minimum and maximum temperature. Usually measured in degrees Kelvin (K).

has range
  real real range c

### temperature ratingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#temperatureRating

Temperature rating. Usually measured in degrees Kelvin (K).

has range
  float

### test pressuredp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#testPressure

The maximum pressure to which the valve has been subjected under test. Usually measured in Pascals (Pa, N/m2).

has range
  float

### thermal conductivitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#thermalConductivity

Fouling factor of the tubes in the tube bundle. Usually measured in m2 Kelvin/Watt.

has range
  float

### thermal efficiencydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#thermalEfficiency

Overall Thermal Efficiency is defined as gross energy output of the heat transfer device divided by the energy input.

has range
  float

### thermal mass heat capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#thermalMassHeatCapacity

Product of component mass and specific heat.

has range
  float

### thermal transmittancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#thermalTransmittance

IfcThermalTransmittanceMeasure is a measure of the rate at which energy is transmitted through a body. Usually measured in Watts/m2 Kelvin.

has range
  float

### transformer vector groupdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#transformerVectorGroup

List of the possible vector groups for the transformer from which that required may be set. Values in the enumeration list follow a standard international code where the first letter describes how the primary windings are connected, the second letter describes how the secondary windings are connected, and the numbers describe the rotation of voltages and currents from the primary to the secondary side in multiples of 30 degrees. D: means that the windings are delta-connected. Y: means that the windings are star-connected. Z: means that the windings are zig-zag connected (a special start-connected providing low reactance of the transformer). The connectivity is only relevant for three-phase transformers.

has range
  string

### valve mechanismdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#valveMechanism

The mechanism by which the valve function is achieved where: BALL: Valve that has a ported ball that can be turned relative to the body seat ports. BUTTERFLY: Valve in which a streamlined disc pivots about a diametric axis. CONFIGUREDGATE: Screwdown valve in which the closing gate is shaped in a configured manner to have a more precise control of pressure and flow change across the valve. GLAND: Valve with a tapered seating, in which a rotatable plug is retained by means of a gland and gland packing. GLOBE: Screwdown valve that has a spherical body. LUBRICATEDPLUG: Plug valve in which a lubricant is injected under pressure between the plug face and the body. NEEDLE: Valve for regulating the flow in or from a pipe, in which a slender cone moves along the axis of flow to close against a fixed conical seat. PARALLELSLIDE: Screwdown valve that has a machined plate that slides in formed grooves to form a seal. PLUG: Valve that has a ported plug that can be turned relative to the body seat ports. WEDGEGATE: Screwdown valve that has a wedge shaped plate fitting into tapered guides to form a seal.

has range
  string

### valve operationdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#valveOperation

The method of valve operation where: DROPWEIGHT: A valve that is closed by the action of a weighted lever being released, the weight normally being prevented from dropping by being held by a wire, the closure normally being made by the action of heat on a fusible link in the wire FLOAT: A valve that is opened and closed by the action of a float that rises and falls with water level. The float may be a ball attached to a lever or other mechanism HYDRAULIC: A valve that is opened and closed by hydraulic actuation LEVER: A valve that is opened and closed by the action of a lever rotating the gate within the valve. LOCKSHIELD: A valve that requires the use of a special lockshield key for opening and closing, the operating mechanism being protected by a shroud during normal operation. MOTORIZED: A valve that is opened and closed by the action of an electric motor on an actuator PNEUMATIC: A valve that is opened and closed by pneumatic actuation SOLENOID: A valve that is normally held open by a magnetic field in a coil acting on the gate but that is closed immediately if the electrical current generating the magnetic field is removed. SPRING: A valve that is normally held in position by the pressure of a spring on a plate but that may be caused to open if the pressure of the fluid is sufficient to overcome the spring pressure. THERMOSTATIC: A valve in which the ports are opened or closed to maintain a required predetermined temperature. WHEEL: A valve that is opened and closed by the action of a wheel moving the gate within the valve.

has range
  string

### valve patterndp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#valvePattern

The configuration of the ports of a valve according to either the linear route taken by a fluid flowing through the valve or by the number of ports where: SINGLEPORT: Valve that has a single entry port from the system that it serves, the exit port being to the surrounding environment. ANGLED_2_PORT: Valve in which the direction of flow is changed through 90 degrees. STRAIGHT_2_PORT: Valve in which the flow is straight through. STRAIGHT_3_PORT: Valve with three separate ports. CROSSOVER_4_PORT: Valve with 4 separate ports.

has range
  string

### ventilating pipe sizedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#ventilatingPipeSize

Size of the ventilating pipe(s). Usually measured in millimeters (mm).

has range
  float

### vertical spacingdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#verticalSpacing

Vertical spacing between tubes in the tube bundle.Usually measured in millimeters (mm).

has range
  float

### vibration transmissibilitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#vibrationTransmissibility

the vibration transmissibility percentage.

has range
  float

### visible light reflectancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#visibleLightReflectance

Fraction of the visible light that is reflected by the glazing at normal incidence. It is a value without unit.

has range
  float

### visible light transmittancedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#visibleLightTransmittance

Fraction of the visible light that passes the shading system at normal incidence. It is a value without unit.

has range
  float

### volumendp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#volumen

Total volume of fluid in the tubes and their headers. Usually measured in cubic metre (m3).

has range
  float

### water flow control system typedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#waterFlowControlSystemType

Factory fitted waterflow control system.

has range
  string

### water inlet temperature rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#waterInletTemperatureRange

Allowable water inlet temperature range. Usually measured in degrees Kelvin (K).

has range
  real real range c

### water pressure rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#waterPressureRange

Allowable water circuit working pressure range. Usually measured in Pascals (Pa, N/m2).

has range
  real real range c

### water requirementdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#waterRequirement

Make-up water requirement. Usually measured in m3/s.

has range
  float

### water storage capacitydp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#waterStorageCapacity

Water storage capacity. Usually measured in cubic metre (m3).

has range
  float

### weightdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#weight

The weight of the humidifier. Usually measured in kilograms (kg) or grams (g).

has range
  float

### working pressuredp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#workingPressure

The normally expected maximum working pressure of the valve. Usually measured in Pascals (Pa, N/m2).

has range
  float

### working pressure rangedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/def/bldg#workingPressureRange

Allowable minimum and maximum working pressure (relative to ambient pressure). Usually measured in Pascals (Pa, N/m2).

has range
  real real range c