#
#                          +---------+
#                          |         |
#                          |   SRC   |
#                          | 9.9.9.1 |
#                          |         |
#                          +---------+
#                               |eth-rt1 (.1)
#                               |
#                               |10.0.10.0/24
#                               |
#                               |eth-src (.2)
#                          +---------+                      .
#                          |         |                      .
#                          |   RT1   |eth-rt1-pce (???)     .
#                          | 1.1.1.1 +----------------------------------+
#                          |  16010  |                      .       ??? |
#                          +---------+                      .           |
#                               |eth-sw1                    .           |
#                               |                           .           |
#                               |                           .           |
#                               |                           .           |
#          +---------+          |          +---------+      .           |
#          |         |          |          |         |      .           |
#          |   RT2   |eth-sw1   |   eth-sw1|   RT3   |      .           |
#          | 2.2.2.2 +----------+----------+ 3.3.3.3 |      .           |
#          |  16020  |     10.0.1.0/24     |  16030  |      .           |
#          +---------+                     +---------+      .eth-pce-rt1|(???)
#     eth-rt4-1|  |eth-rt4-2          eth-rt5-1|  |eth-rt5-2.      +----+----+
#              |  |                            |  |         .      |         |
#   10.0.2.0/24|  |10.0.3.0/24      10.0.4.0/24|  |10.0.5.0/24     |   PCE   |
#              |  |                            |  |         .      |   ????  |
#     eth-rt2-1|  |eth-rt2-2          eth-rt3-1|  |eth-rt3-2.      |         |
#          +---------+                     +---------+      .      +----+----+
#          |         |                     |         |      .eth-pce-rt6|(???)
#          |   RT4   |     10.0.6.0/24     |   RT5   |      .           |
#          | 4.4.4.4 +---------------------+ 5.5.5.5 |      .           |
#          |  16040  |eth-rt5       eth-rt4|  16050  |      .           |
#          +---------+                     +---------+      .           |
#        eth-rt6|                                |eth-rt6   .           |
#               |                                |          .           |
#    10.0.7.0/24|                                |10.0.8.0/24           |
#               |          +---------+           |          .           |
#               +----------|         |-----------+          .           |
#                   eth-rt4|   RT6   |eth-rt5               .           |
#                          | 6.6.6.6 |eth-rt6-pce (????)    .      ???? |
#                          |  16060  +----------------------------------+
#                          +---------+                      .
#                               |eth-dst (.1)               .
#                               |                           .
#                               |10.0.11.0/24
#                               |
#                               |eth-rt6 (.2)
#                          +---------+
#                          |         |
#                          |   DST   |
#                          | 9.9.9.2 |
#                          |         |
#                          +---------+
#

---

routers:

  src:
    links:
      lo:
        ipv4: 9.9.9.1/32
        ipv6: 2001:db8:1066::1/128
        mpls: yes
      eth-rt1:
        peer: [rt1, eth-src]
        ipv4: 10.0.10.1/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
    shell: |
      ip route add 9.9.9.2/32 encap mpls 1111 via inet 10.0.10.2 src 9.9.9.1

  rt1:
    links:
      lo:
        ipv4: 1.1.1.1/32
        mpls: yes
      eth-sw1:
        peer: [sw1, sw1-rt1]
        ipv4: 10.0.1.1/24
        mpls: yes
      eth-src:
        peer: [src, eth-rt1]
        ipv4: 10.0.10.2/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      pathd:
        args: "-M pathd_pcep"
        config: |
          debug pathd pcep basic
          segment-routing
           traffic-eng
            mpls-te on
            policy color 1 endpoint 6.6.6.6
             name DEFAULT
             binding-sid 1111
             candidate-path preference 100 name RUNTIME dynamic
             !
            !
            pcep
             pce-config CONFIG
              source-address ip 1.1.1.1
             pce PCE
              address ip ${PCE_IP}
              config CONFIG
             pcc
              peer PCE
          !
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-sw1
           ip router isis 1
           ipv6 router isis 1
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0001.00
           is-type level-1
           redistribute ipv4 static level-1
           redistribute ipv4 connected level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 1.1.1.1/32 index 10 explicit-null
           segment-routing prefix 2001:db8:1000::1/128 index 11 explicit-null
          !
    shell: |
      ip route add 9.9.9.1/32 dev eth-src
      ip link add eth-rt1-pce type veth peer name eth-pce-rt1
      ip addr add ${RT1_PCE_INT_IF_IP}/24 dev eth-rt1-pce
      ip link set eth-pce-rt1 netns ${PCE_NETNS}
      ip -n ${PCE_NETNS} addr add ${RT1_PCE_EXT_IF_IP}/24 dev eth-pce-rt1
      ip link set eth-rt1-pce up
      ip -n ${PCE_NETNS} link set eth-pce-rt1 up
      ip route add ${RT1_PCE_EXT_IF_IP}/24 via ${RT1_PCE_INT_IF_IP} dev eth-rt1-pce src 1.1.1.1
      ip -n ${PCE_NETNS} route add ${RT1_PCE_INT_IF_IP}/32 via ${RT1_PCE_EXT_IF_IP} dev eth-pce-rt1
      ip -n ${PCE_NETNS} route add 1.1.1.1/32 via ${RT1_PCE_EXT_IF_IP} dev eth-pce-rt1

  rt2:
    links:
      lo:
        ipv4: 2.2.2.2/32
        ipv6: 2001:db8:1000::2/128
        mpls: yes
      eth-sw1:
        peer: [sw1, sw1-rt2]
        ipv4: 10.0.1.2/24
        mpls: yes
      eth-rt4-1:
        peer: [rt4, eth-rt2-1]
        ipv4: 10.0.2.2/24
        mpls: yes
      eth-rt4-2:
        peer: [rt4, eth-rt2-2]
        ipv4: 10.0.3.2/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-sw1
           ip router isis 1
           ipv6 router isis 1
           isis hello-multiplier 3
          !
          interface eth-rt4-1
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt4-2
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0002.00
           is-type level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 2.2.2.2/32 index 20 no-php-flag
           segment-routing prefix 2001:db8:1000::2/128 index 21 no-php-flag
          !

  rt3:
    links:
      lo:
        ipv4: 3.3.3.3/32
        ipv6: 2001:db8:1000::3/128
        mpls: yes
      eth-sw1:
        peer: [sw1, sw1-rt3]
        ipv4: 10.0.1.3/24
        mpls: yes
      eth-rt5-1:
        peer: [rt5, eth-rt3-1]
        ipv4: 10.0.4.3/24
        mpls: yes
      eth-rt5-2:
        peer: [rt5, eth-rt3-2]
        ipv4: 10.0.5.3/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-sw1
           ip router isis 1
           ipv6 router isis 1
           isis hello-multiplier 3
          !
          interface eth-rt5-1
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt5-2
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0003.00
           is-type level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 3.3.3.3/32 index 30 no-php-flag
           segment-routing prefix 2001:db8:1000::3/128 index 31 no-php-flag
          !

  rt4:
    links:
      lo:
        ipv4: 4.4.4.4/32
        ipv6: 2001:db8:1000::4/128
        mpls: yes
      eth-rt2-1:
        peer: [rt2, eth-rt4-1]
        ipv4: 10.0.2.4/24
        mpls: yes
      eth-rt2-2:
        peer: [rt2, eth-rt4-2]
        ipv4: 10.0.3.4/24
        mpls: yes
      eth-rt5:
        peer: [rt5, eth-rt4]
        ipv4: 10.0.6.4/24
        mpls: yes
      eth-rt6:
        peer: [rt6, eth-rt4]
        ipv4: 10.0.7.4/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-rt2-1
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt2-2
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt5
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt6
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0004.00
           is-type level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 4.4.4.4/32 index 40 no-php-flag
           segment-routing prefix 2001:db8:1000::4/128 index 41 no-php-flag
          !

  rt5:
    links:
      lo:
        ipv4: 5.5.5.5/32
        ipv6: 2001:db8:1000::5/128
        mpls: yes
      eth-rt3-1:
        peer: [rt3, eth-rt5-1]
        ipv4: 10.0.4.5/24
        mpls: yes
      eth-rt3-2:
        peer: [rt3, eth-rt5-2]
        ipv4: 10.0.5.5/24
        mpls: yes
      eth-rt4:
        peer: [rt4, eth-rt5]
        ipv4: 10.0.6.5/24
        mpls: yes
      eth-rt6:
        peer: [rt6, eth-rt5]
        ipv4: 10.0.8.5/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-rt3-1
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt3-2
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt4
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt6
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0005.00
           is-type level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 5.5.5.5/32 index 50 no-php-flag
           segment-routing prefix 2001:db8:1000::5/128 index 51 no-php-flag
          !

  rt6:
    links:
      lo:
        ipv4: 6.6.6.6/32
        ipv6: 2001:db8:1000::6/128
        mpls: yes
      eth-rt4:
        peer: [rt4, eth-rt6]
        ipv4: 10.0.7.6/24
        mpls: yes
      eth-rt5:
        peer: [rt5, eth-rt6]
        ipv4: 10.0.8.6/24
        mpls: yes
      eth-dst:
        peer: [dst, eth-rt6]
        ipv4: 10.0.11.1/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
      pathd:
        args: "-M pathd_pcep"
        config: |
          debug pathd pcep
          segment-routing
           traffic-eng
            policy color 1 endpoint 1.1.1.1
             name DEFAULT
             binding-sid 6666
             candidate-path preference 200 name RUNTIME dynamic
             !
            !
            pcep
             pce-config CONFIG
              source-address ip 6.6.6.6
             pce PCE
              address ip ${PCE_IP}
              config CONFIG
             pcc
              peer PCE
          !
      isisd:
        run: yes
        config: |
          interface lo
           ip router isis 1
           ipv6 router isis 1
           isis passive
          !
          interface eth-rt4
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          interface eth-rt5
           ip router isis 1
           ipv6 router isis 1
           isis network point-to-point
           isis hello-multiplier 3
          !
          router isis 1
           net 49.0000.0000.0000.0006.00
           is-type level-1
           redistribute ipv4 static level-1
           redistribute ipv4 connected level-1
           topology ipv6-unicast
           segment-routing on
           segment-routing global-block 16000 23999
           segment-routing node-msd 8
           segment-routing prefix 6.6.6.6/32 index 60 explicit-null
           segment-routing prefix 2001:db8:1000::6/128 index 61 explicit-null
          !
    shell: |
      ip route add 9.9.9.2/32 dev eth-dst
      ip link add eth-rt6-pce type veth peer name eth-pce-rt6
      ip addr add ${RT6_PCE_INT_IF_IP}/24 dev eth-rt6-pce
      ip link set eth-pce-rt6 netns ${PCE_NETNS}
      ip -n ${PCE_NETNS} addr add ${RT6_PCE_EXT_IF_IP}/24 dev eth-pce-rt6
      ip link set eth-rt6-pce up
      ip -n ${PCE_NETNS} link set eth-pce-rt6 up
      ip route add ${RT6_PCE_EXT_IF_IP}/24 via ${RT6_PCE_INT_IF_IP} dev eth-rt6-pce src 6.6.6.6
      ip -n ${PCE_NETNS} route add ${RT6_PCE_INT_IF_IP}/32 via ${RT6_PCE_EXT_IF_IP} dev eth-pce-rt6
      ip -n ${PCE_NETNS} route add 6.6.6.6/32 via ${RT6_PCE_EXT_IF_IP} dev eth-pce-rt6

  dst:
    links:
      lo:
        ipv4: 9.9.9.2/32
        ipv6: 2001:db8:1066::2/128
        mpls: yes
      eth-rt6:
        peer: [rt6, eth-dst]
        ipv4: 10.0.11.2/24
        mpls: yes
    frr:
      zebra:
        run: yes
        config:
    shell: |
      ip route add 9.9.9.1/32 encap mpls 6666 via inet 10.0.11.1

switches:
  sw1:
    links:
      sw1-rt1:
        peer: [rt1, rt1-sw1]
      sw1-rt2:
        peer: [rt2, rt2-sw1]
      sw1-rt3:
        peer: [rt3, rt3-sw1]

frr:
  #perf: yes
  #valgrind: yes
  base-configs:
    all: |
      hostname %(node)
      password 1
      log file %(logdir)/%(node)-%(daemon).log
      log commands
    zebra: |
      debug zebra kernel
      debug zebra packet
      debug zebra mpls
    isisd: |
      debug isis events
      debug isis route-events
      debug isis spf-events
      debug isis sr-events
      debug isis lsp-gen
