# MtsCapabilityInfoMtsAccessInfo

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**AccessId** | **int32** | Unique identifier for the access network connection | [optional] [default to null]
**AccessType** | **int32** | Numeric value (0-255) corresponding to specific type of access network as following: 0 &#x3D; Unknown 1 &#x3D; Any IEEE802.11-based WLAN technology 2 &#x3D; Any 3GPP-based Cellular technology 3 &#x3D; Any Fixed Access 11 &#x3D; IEEE802.11 a/b/g WLAN 12 &#x3D; IEEE 802.11 a/b/g/n WLAN 13 &#x3D; IEEE 802.11 a/b/g/n/ac WLAN 14 &#x3D; IEEE 802.11 a/b/g/n/ac/ax WLAN (Wi-Fi 6) 15 &#x3D; IEEE 802.11 b/g/n WLAN 31 &#x3D; 3GPP GERAN/UTRA (2G/3G) 32 &#x3D; 3GPP E-UTRA (4G/LTE) 33 &#x3D; 3GPP NR (5G) | [optional] [default to null]
**Metered** | **int32** | Numeric value (0-255) corresponding to the following: 0: the connection is not metered (see note) 1: the connection is metered 2: unknown  | [optional] [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)

