# NeighborReport

## Properties
Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**Bssid** | **string** | BSS Id of the Access Point that is being reported. | [default to null]
**BssidInfo** | **int32** | Additional information related to Access Point that is being reported such as AP reachability, security, key scope, Mobility Domain, HT/VHT capability and Fine Time Measurements. | [default to null]
**Channel** | **int32** | The channel currently used by this Access Point. | [default to null]
**OperatingClass** | **int32** | The channel set of the AP indicated by this BSSID. | [default to null]
**PhyType** | **int32** | PHY type of the AP indicated by this BSSID. It is an integer value coded according to the value of the dot11PHYType. | [default to null]

[[Back to Model list]](../README.md#documentation-for-models) [[Back to API list]](../README.md#documentation-for-api-endpoints) [[Back to README]](../README.md)


