## 4. Cross reference for example1 classes, properties and dataproperties

This section provides details for each class and property defined by example1.

## Classes

- Building
- Building space
- Compressor
- Measurement
- Spatial thing
- Unit of measure

### Buildingc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/data/bldg#Building

A building represents a structure that provides shelter for its occupants or contents and stands in one place. The building is also used to provide a basic element within the spatial structure hierarchy for the components of a building project (together with site, storey, and space).

has super-classes
  Spatial thing c
  location op only Spatial thing c
has members
  Computer Science Building 1 ni

### Building spacec back to ToC or Class ToC

IRI: http://saref.linkeddata.es/data/bldg#BuildingSpace

An entity used to define the physical spaces of the building. A building space contains devices or building objects.

has super-classes
  Spatial thing c
  isSpaceOf op only Building c or Building space c
has members
  Refrigeration store of Computer Science Building 1 ni

### Compressorc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/data/bldg#Compressor

A compressor is a device that compresses a fluid typically used in a refrigeration circuit.

has super-classes
  compressor speed op only Measurement c
  refrigerant class dp only string
  power source dp only string
  impeller diameter op only Measurement c
  has hot gas bypass dp only boolean
  ideal capacity op only Measurement c
  nominal capacity op only Measurement c
has members
  CompressorSIERRA02-0434C3 ni

### Measurementc back to ToC or Class ToC

IRI: http://saref.linkeddata.es/data/bldg#Measurement

Represents the measured value made over a property. It is also linked to the unit of measure in which the value is expressed and the timestamp of the measurement.

has super-classes
  is measured in op only Unit of measure c
  is measured in op exactly 1 Unit of measure c
  has value dp exactly 1
has members
  Compressor speed of compressor001 SIERRA02-0434C3 ni, Ideal capacity of compressor001 SIERRA02-0434C3 ni, Impeller diameter of compressor001 SIERRA02-0434C3 ni, Nominal capacity of compressor001 SIERRA02-0434C3 ni

### Spatial thingc back to ToC or Class ToC

IRI: http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing

is defined by
  http://www.w3.org/2003/01/geo/wgs84_pos#

Anything with spatial extent, i.e. size, shape, or position. e.g. people, places, bowling balls, as well as abstract areas like cubes.

has sub-classes
  Building c, Building space c
has members
  Location of Computer Science Building 1 ni, Location of compressor001 SIERRA02-0434C3 ni, LocationRefrigerationStoreComputerScienceBuilding1 ni

### Unit of measurec back to ToC or Class ToC

IRI: https://w3id.org/saref#UnitOfMeasure

is defined by
  https://w3id.org/saref#

The unit of measure is a standard for measurement of a quantity, such as a Property. For example, Power is a property and Watt is a unit of power that represents a definite predetermined power: when we say 10 Watt, we actually mean 10 times the definite predetermined power called "watt". Our definition is based on the definition of unit of measure in the Ontology of units of Measure (OM). We propose here a list of some units of measure that are relevant for the purpose of the Smart Appliances ontology, but this list can be extended.

has members
  cycles per second ni, inch international ni

## Object Properties

- compressor speed
- ideal capacity
- impeller diameter
- is contained in
- is measured in
- isSpaceOf
- location
- nominal capacity

### compressor speedop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#compressorSpeed

Compressor speed. Usually measured in cycles/s.

### ideal capacityop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#idealCapacity

Compressor capacity under ideal conditions. Usually measured in Watts (W, J/s).

### impeller diameterop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#impellerDiameter

Diameter of compressor impeller - used to scale performance of geometrically similar compressors. Usually measured in millimeters (mm).

### is contained inop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#isContainedIn

A relation between an object and the physical space in which it is located.

### is measured inop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#isMeasuredIn

A relation between a measurement and the unit of measure in which the measurement value is expressed.

### isSpaceOfop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#isSpaceOf

Relation between a building space and the building or building space it belongs to.

### locationop back to ToC or Object Property ToC

IRI: http://www.w3.org/2003/01/geo/wgs84_pos#location

is defined by
  http://www.w3.org/2003/01/geo/wgs84_pos#

The relation between something and the point, or other geometrical thing in space, where it is. For example, the realtionship between a radio tower and a Point with a given lat and long. Or a relationship between a park and its outline as a closed arc of points, or a road and its location as a arc (a sequence of points). Clearly in practice there will be limit to the accuracy of any such statement, but one would expect an accuracy appropriate for the size of the object and uses such as mapping .

### nominal capacityop back to ToC or Object Property ToC

IRI: http://saref.linkeddata.es/data/bldg#nominalCapacity

Nominal capacity. Usually measured in Watts (W, J/s).

## Data Properties

- has hot gas bypass
- has value
- power source
- refrigerant class

### has hot gas bypassdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/data/bldg#hasHotGasBypass

Whether or not hot gas bypass is provided for the compressor. TRUE = Yes, FALSE = No.

has range
  boolean

### has valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/saref#hasValue

is defined by
  https://w3id.org/saref#

A relationship defining the value of a certain property, e.g., energy or power

### power sourcedp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/data/bldg#powerSource

Type of power driving the compressor.

has range
  string

### refrigerant classdp back to ToC or Data Property ToC

IRI: http://saref.linkeddata.es/data/bldg#refrigerantClass

Refrigerant class used by the compressor. CFC: Chlorofluorocarbons. HCFC: Hydrochlorofluorocarbons. HFC: Hydrofluorocarbons.

has range
  string

## Named Individuals

- Compressor speed of compressor001 SIERRA02-0434C3
- CompressorSIERRA02-0434C3
- Computer Science Building 1
- cycles per second
- Ideal capacity of compressor001 SIERRA02-0434C3
- Impeller diameter of compressor001 SIERRA02-0434C3
- inch international
- Location of compressor001 SIERRA02-0434C3
- Location of Computer Science Building 1
- LocationRefrigerationStoreComputerScienceBuilding1
- Nominal capacity of compressor001 SIERRA02-0434C3
- Power of compressor 001 SIERRA02-0434C3
- Power profile of compressor 001 SIERRA02-0434C3
- Refrigeration store of Computer Science Building 1
- watt

### Compressor speed of compressor001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#CompressorSpeedCompressor001SIERRA02-0434C3

belongs to
  Measurement c
has facts
  has value dp "3.0"^^float
  is measured in op cycles per second

### CompressorSIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#Compressor001SIERRA02-0434C3

belongs to
  Compressor c
has facts
  refrigerant class dp "HFC"^^string
  power source dp "MotorDriven"^^string
  has manufacturer dp "SIEMENS"^^string
  has name dp "SIERRA 02-0434C3"^^string
  has hot gas bypass dp "false"^^boolean
  compressor speed op Compressor speed of compressor001 SIERRA02-0434C3
  ideal capacity op Ideal capacity of compressor001 SIERRA02-0434C3
  impeller diameter op Impeller diameter of compressor001 SIERRA02-0434C3
  location op Location of compressor001 SIERRA02-0434C3
  nominal capacity op Nominal capacity of compressor001 SIERRA02-0434C3
  exposes op Power profile of compressor 001 SIERRA02-0434C3
  is contained in op Refrigeration store of Computer Science Building 1

### Computer Science Building 1ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#ComputerScienceBuilding1

belongs to
  Building c
has facts
  location op Location of Computer Science Building 1

### cycles per secondni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#cyclesPerSecond

belongs to
  Unit of measure c

### Ideal capacity of compressor001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#IdealCapacityCompressor001SIERRA02-0434C3

belongs to
  Measurement c
has facts
  has value dp "1800.0"^^float
  is measured in op watt

### Impeller diameter of compressor001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#ImpellerDiameterCompressor001SIERRA02-0434C3

belongs to
  Measurement c
has facts
  has value dp "5.9"^^float
  is measured in op inch international

### inch internationalni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/inch-international

belongs to
  Unit of measure c

### Location of compressor001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#LocationCompressor001SIERRA02-0434C3

belongs to
  Spatial thing c
has facts
  longitude dp "-3.839203"^^decimal
  latitude dp "40.405155"^^decimal

### Location of Computer Science Building 1ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#LocationComputerScienceBuilding1

belongs to
  Spatial thing c
has facts
  longitude dp "-3.839349"^^decimal
  latitude dp "40.405013"^^decimal

### LocationRefrigerationStoreComputerScienceBuilding1ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#LocationRefrigerationStoreComputerScienceBuilding1

belongs to
  Spatial thing c
has facts
  longitude dp "-3.839209"^^decimal
  latitude dp "40.405152"^^decimal

### Nominal capacity of compressor001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#NominalCapacityCompressor001SIERRA02-0434C3

belongs to
  Measurement c
has facts
  has value dp "680.0"^^float
  is measured in op watt

### Power of compressor 001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#PowerCompressor001SIERRA02-0434C3

belongs to
  power c
has facts
  has value dp "902.0"^^float
  is measured in op watt

### Power profile of compressor 001 SIERRA02-0434C3ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#PowerProfileCompressor001SIERRA02-0434C3

belongs to
  power profile c
has facts
  has consumption op Power of compressor 001 SIERRA02-0434C3

### Refrigeration store of Computer Science Building 1ni back to ToC or Named Individual ToC

IRI: http://saref.linkeddata.es/data/bldg#RefrigerationStoreComputerScienceBuilding1

belongs to
  Building space c
has facts
  isSpaceOf op Computer Science Building 1
  location op LocationRefrigerationStoreComputerScienceBuilding1

### wattni back to ToC or Named Individual ToC

IRI: http://www.wurvoc.org/vocabularies/om-1.8/watt

belongs to
  power unit c