## Cross reference for SAREF extension for industry and manufacturing domain classes, properties and dataproperties back to ToC

This section provides details for each class and property defined by SAREF extension for industry and manufacturing domain.

### Classes

- Actual measurement
- Area
- Batch
- Expected measurement
- Factory
- GTIN12ID
- GTIN13ID
- GTIN14ID
- GTIN18ID
- Identifier
- IRDI
- Item
- Item Batch
- Item category
- Material Batch
- Material category
- Measurement
- Production equipment category
- Production equipment function
- ProductionEquipment
- Site
- Size
- UUID
- Work center

### Actual measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ActualMeasurement

Describes whether the measurement is actually measured during the production process. Disjoint with ExpectedMeasurement.

has super-classes
  Measurement c
is disjoint with
  Expected measurement c

### Areac back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Area

A subclass of s4bldg:BuildingSpace used to define the physical spaces of the building. According to IEC 62264, areas are physical, geographical or logical groupings of resources determined by the site. A site can be divided in areas, whereas areas contain work centers.s.

has super-classes
  building space c
is disjoint with
  Site c, Work center c

### Batchc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Batch

A uniform collection of tangible objects or Lot. This can either be a collection of produced items (i.e. the outflow of products) or a collection of raw material or required material (i.e. the inflow of products). It is assumed that the objects in a batch are similar and thus have shared attributes. Note that this definition is broader than the definition in IEC 61512, which defines a batch as the material that is being produced (whereas in SAREF4INMA a batch can be items or materials).

has super-classes
  feature of interest c, thing c
has sub-classes
  Item Batch c, Material Batch c

### Expected measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ExpectedMeasurement

Describes whether the measurement is expected (i.e., planned before the production process). Disjoint with ActualMeasurement.

has super-classes
  Measurement c
is disjoint with
  Actual measurement c

### Factoryc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Factory

A subclass of s4bldg:Building specialized for the purpose of SAREF4INMA, a factory represents one or more organizations sharing a definit mission, goals and objectives which provides an output such as a product (definition taken from IEC 62264). A factory can be divided in one or multiple sites.

has super-classes
  building c

### GTIN12IDc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#GTIN12ID

GTIN-12 (UPC-A) is a 12-digit number used primarily in North America

has super-classes
  Identifier c
is in range of
  has GTIN12ID op

### GTIN13IDc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#GTIN13ID

GTIN-13 (EAN/UCC-13) is a 13-digit number used predominately outside of North America

has super-classes
  Identifier c
is in range of
  has GTIN13ID op

### GTIN14IDc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#GTIN14ID

GTIN-14 (EAN/UCC-14 or ITF-14 or also known as ITF Symbol, SCC-14, DUN-14, UPC Case Code, UPC Shipping Container Code, UCC Code 128, EAN Code 128) is a 14-digit number used to identify trade items at various packaging levels.

has super-classes
  Identifier c
is in range of
  has GTIN14ID op

### GTIN18IDc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#GTIN8ID

GTIN-8 (EAN/UCC-8) is an 8-digit number used predominately outside of North America.

has super-classes
  Identifier c
is in range of
  has GTIN8ID op

### Identifierc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ID

A unique identifier.

has super-classes
  concept scheme c
has sub-classes
  GTIN12ID c, GTIN13ID c, GTIN14ID c, GTIN18ID c, IRDI c, UUID c
is in range of
  has identifier op

### IRDIc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#IRDI

International Registration Data Identifier (IRDI) is based on the international standards ISO/IEC 11179-6, ISO 29002 and ISO 6532 and used in eCl@ss and the Asset Administration Shell as unique identifier.

has super-classes
  Identifier c
is in range of
  has IRDI op

### Itemc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Item

A tangible object which can be unique identified, for example, with a GTIN in the form of a barcode/QR/RFID tag. An item product can be the result of the organization's production process (i.e. outflow of objects/goods) or can be uniquely identifiable material (i.e. inflow of objects/supplies). Each item is part of exactly one ItemBatch, whereas each ItemBatch contains only Items which have similar properties. An item can consists of multiple Batches and other Items (i.e. subassemblies).

has super-classes
  feature of interest c

### Item Batchc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ItemBatch

A uniform collection of tangible objects which are relevant for the prodcution process. The ItemBatch consists of a set of objects with similar properties (e.g. a certain type of sensors or metal sheets). The difference between ItemBatch and MaterialBatch is that individual items can be traced in a ItemBatch, whereas this is not possible in a MaterialBatch, meaning that, for example, it is possible to trace the individual metal sheet used in a ItemBatch. This implies that the objects in an ItemBatch have an unique identifier (e.g. a GTIN code in the form of a barcode/QR-code or RFID tag).

has super-classes
  Batch c

### Item categoryc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ItemCategory

An ItemCategory describes a single type of item in terms of its static properties. Each ItemCategory can have multiple related ItemBatches, which all contain individual Items. The essential properties of each Item in all ItemBatches are the same. However, each batch might use different MaterialBatches and/or different ProductionEquipment. Therefore, small deviations between batches might occur, while the essential properties of all Items related to an ItemCategory are similar.

has super-classes

### Material Batchc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#MaterialBatch

A uniform collection of tangible raw material which are relevant for the prodcution process. The MaterialBatch can consists of a set of objects with similar properties (e.g. a certain type of screws) or a stock of homogeen material (e.g. oil, water). The difference between MaterialBatch and ItemBatch is that individual items cannot be traced in a MaterialBatch, whereas this is possible in an ItemBatch, meaning that, for example, it is not possible to trace the individual screw used in a MaterialBatch.

has super-classes
  Batch c

### Material categoryc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#MaterialCategory

A MaterialCategory describes a category of material in terms of its static properties. Examples are: a certain category of steel or plastic. Each MaterialCategory can have multiple related MaterialBatches, which represent the physical material. The essential properties of the material in all MaterialBatches are the same. However, each batch might use different MaterialBatches and/or different ProductionEquipment. Therefore, small deviations between batches might occur, while the essential properties of the material related to an MaterialCategory are similar.

has super-classes

### Measurementc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Measurement

A subclass of saref:Measurement that represents the measured value made over a property. It is also linked to the unit of measure in which the value is expressed and the timestamp of the measurement. The saref4imna:Measurement can be linked to individual Batches or Items. Moreover, the Measurement can be an ExpectedMeasurement (i.e. the value which is planned) or the ActualMeasurement (i.e. the value measured during production), which enables to check for deviations between the planned and actual values.

has super-classes
  measurement c
has sub-classes
  Actual measurement c, Expected measurement c

### Production equipment categoryc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ProductionEquipmentCategory

A ProductionEquipmentCategory represents a certain type of production equipment, which is generally static over time. More concretely, the ProductionEquipmentCategory represents a certain model and brand of a production equipment. Each ProductionEquipmentCategory can have multiple related ProductionEquipment, which represent the actual individual machines. Moreover, each ItemCategory can be produced by multiple ProductionEquipmentCategories.

has super-classes

### Production equipment functionc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ProductionEquipmentFunction

has super-classes
  function c, thing c

### ProductionEquipmentc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#ProductionEquipment

A production equipment is a specialization of a saref:Device and s4bldg:PhysicalObject that can produce items in a manufacturing process. This class represents an individual production equipment device and includes their specification in terms of functions, states and services. Different types of machines can be defined under this class as needed, for example, LaserCuttingMachine (i.e., a type of production equipment to cut steel material), MillingMachine (i.e., to drill holes in steel material), MouldingMachine (i.e., to mold liquid material, such as iron or plastic, and let it harden in a certain shape), WeldingMachine (i.e., join parts of material, such as steel, together), etc.

has super-classes
  device c, physical object c
has sub-classes
  Work center c

### Sitec back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Site

A subclass of s4bldg:BuildingSpace used to define the physical spaces of the building. According to IEC 62264, sites are identified physical, geographical, and/or logical component groupings of a manufacturing enterprise. A factory can be divided in sites, whereas sites can be divided areas

has super-classes
  building space c
is disjoint with
  Area c, Work center c

### Sizec back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#Size

The amount of certain objects in a collection (e.g., size of a material batch).

has super-classes
  property c

### UUIDc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#UUID

A universally unique identifier (UUID) is a 128-bit number used to identify items and is also known as: globally unique identifier (GUID). In its canonical textual representation, the sixteen octets of a UUID are represented as 32 hexadecimal (base 16) digits, displayed in five groups separated by hyphens, in the form 8-4-4-4-12 for a total of 36 characters (32 alphanumeric characters and four hyphens). UUID are documented in ISO/IEC 11578:1996 "Information technology – Open Systems Interconnection – Remote Procedure Call (RPC)" and in ITU-T Rec. X.667 | ISO/IEC 9834-8:2005.

has super-classes
  Identifier c
is in range of
  has UUID op

### Work centerc back to ToC or Class ToC

IRI: https://w3id.org/def/saref4inma#WorkCenter

A subclass of s4inma:ProductionEquipment (and therefore of s4bld:PhysicalObject). It is an equipment element under an area in a role-based equipment hierarchy that performs production, storage or material movement (definition taken from IEC 62264). An Area contains work centers.

has super-classes
  ProductionEquipment c
is disjoint with
  Area c, Site c

### Object Properties

- belongs to category
- consists of batch
- consists of item
- creates
- has feature of interest
- has GTIN12ID
- has GTIN13ID
- has GTIN14ID
- has GTIN8ID
- has identifier
- has IRDI
- has size
- has state
- has update
- has UUID
- is category of
- is created in
- is feature of interest of
- is produced by
- needs equipment
- produces

### belongs to categoryop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#belongsToCategory

Link between an entity and its category

is inverse of
  is category of op

### consists of batchop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#consistsOfBatch

A relation to express that a batch can recursively consists of other batches

### consists of itemop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#consistsOfItem

A relation to express that an item can recursively consists of other Items

### createsop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#creates

A relation between a production process (e.g., Batch) that creates one or more tangible objects (e.g., Items)

is inverse of
  is created in op

### has feature of interestop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasFeatureOfInterest

is inverse of
  is feature of interest of op

### has GTIN12ID op back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN12ID

has super-properties
  has identifier op
has range
  GTIN12ID c

### has GTIN13IDop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN13ID

has super-properties
  has identifier op
has range
  GTIN13ID c

### has GTIN14IDop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN14ID

has super-properties
  has identifier op
has range
  GTIN14ID c

### has GTIN8IDop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN8ID

has super-properties
  has identifier op
has range
  GTIN18ID c

### has identifierop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasIdentifier

link between an entity and its unique identifier

has sub-properties
  has GTIN12ID op, has GTIN13ID op, has GTIN14ID op, has GTIN8ID op, has IRDI op, has UUID op
has range
  Identifier c

### has IRDIop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasIRDI

has super-properties
  has identifier op
has range
  IRDI c

### has sizeop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasSize

A relationship to count the amount of certain objects in a collection (e.g., size of a material batch)

### has stateop back to ToC or Object Property ToC

IRI: https://w3id.org/saref#hasState

### has updateop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasUpdate

The newer version of a ItemCategory.

### has UUIDop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#hasUUID

has super-properties
  has identifier op
has range
  UUID c

### is category ofop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#isCategoryOf

is inverse of
  belongs to category op

### is created inop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#isCreatedIn

An Item is created in an ItemBatch.

is inverse of
  creates op

### is feature of interest ofop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#isFeatureOfInterestOf

is inverse of
  has feature of interest op

### is produced byop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#isProducedBy

Items are produced using certain types of ProductionEquipmentCategories, for example: welding machines or laser cutting machines.

is inverse of
  produces op

### needs equipmentop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#needsEquipment

A relationship indicating that an entity needs a particular equipment to be produced

### producesop back to ToC or Object Property ToC

IRI: https://w3id.org/def/saref4inma#produces

ProductionEquipmentCategory, such as welding machines or laser cutting machines, produce certain categories of items (inverse of s4inma:isProducedBy)

is inverse of
  is produced by op

### Data Properties

- has certificate
- has g t i n8 i d value
- has GTIN12ID value
- has GTIN13ID value
- has GTIN14ID
- has identifier value
- has IRDI
- has model number
- has serial number
- has UUID value
- has version

### has certificatedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasCertificate

The MaterialBatch can contain material quality certificates, for example a NEN 10204:2004 3.1 steel certificate.

has range
  string

### has g t i n8 i d valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN8IDValue

has super-properties
  has identifier value dp
has range
  string

### has GTIN12ID valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN12IDValue

has super-properties
  has identifier value dp
has range
  string

### has GTIN13ID valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN13IDValue

has super-properties
  has identifier value dp
has range
  string

### has GTIN14IDdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasGTIN14IDValue

has super-properties
  has identifier value dp
has range
  string

### has identifier valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasIDValue

A relation to express the value of an indentifier as a string (it can be used as alternative to or in combination with the s4inma:hasIdentifier object property

has sub-properties
  has GTIN12ID value dp, has GTIN13ID value dp, has GTIN14ID dp, has IRDI dp, has UUID value dp, has g t i n8 i d value dp
has range
  string

### has IRDIdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasIRDIValue

has super-properties
  has identifier value dp
has range
  string

### has model numberdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasModelNumber

A relation to express the model number of a certain object (item, product, equipment, etc.)

### has serial numberdp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasSerialNumber

A relation to describe the serial number of a certain Item, which is unique per Item.

### has UUID valuedp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasUUIDValue

has super-properties
  has identifier value dp
has range
  string

### has versiondp back to ToC or Data Property ToC

IRI: https://w3id.org/def/saref4inma#hasVersion

An item has a certain revision or version number, whereas a higher number indicates a newer version.

## Legend back to ToC

c: Classes
op: Object Properties
dp: Data Properties
ni: Named Individuals