<?xml version="1.0"?>
<rdf:RDF xmlns="https://w3id.org/def/saref4bldg#"
     xml:base="https://w3id.org/def/saref4bldg"
     xmlns:rdf="http://www.w3.org/1999/02/22-rdf-syntax-ns#"
     xmlns:terms="http://purl.org/dc/terms/"
     xmlns:owl="http://www.w3.org/2002/07/owl#"
     xmlns:xml="http://www.w3.org/XML/1998/namespace"
     xmlns:xsd="http://www.w3.org/2001/XMLSchema#"
     xmlns:rdfs="http://www.w3.org/2000/01/rdf-schema#"
     xmlns:vann="http://purl.org/vocab/vann/"
     xmlns:prov="http://www.w3.org/ns/prov#"
     xmlns:dc="http://purl.org/dc/elements/1.1/">
    <owl:Ontology rdf:about="https://w3id.org/def/saref4bldg">
        <owl:versionIRI rdf:resource="https://w3id.org/def/v1/saref4bldg"/>
        <dc:description xml:lang="en">This ontology extends the SAREF ontology for the building domain by defining building devices and how they are located in a building. This extension is based on the ISO 16739:2013 Industry Foundation Classes (IFC) standard for data sharing in the construction and facility management industries. The descriptions of the classes and properties extracted from IFC have been taken from the IFC documentation.</dc:description>
        <dc:publisher rdf:resource="http://www.oeg-upm.net/"/>
        <dc:title xml:lang="en">SAREF extension for building devices</dc:title>
        <terms:creator rdf:resource="http://purl.org/net/mpoveda"/>
        <terms:creator rdf:resource="http://www.garcia-castro.com/foaf.rdf#me"/>
        <terms:license rdf:resource="http://purl.org/NET/rdflicense/cc-by4.0"/>
        <vann:preferredNamespacePrefix rdf:datatype="http://www.w3.org/2001/XMLSchema#string">s4bldg</vann:preferredNamespacePrefix>
        <vann:preferredNamespaceUri rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/def/saref4bldg#</vann:preferredNamespaceUri>
        <owl:versionInfo rdf:datatype="http://www.w3.org/2001/XMLSchema#string">1.0</owl:versionInfo>
    </owl:Ontology>
    


    <!-- 
    ///////////////////////////////////////////////////////////////////////////////////////
    //
    // Annotation properties
    //
    ///////////////////////////////////////////////////////////////////////////////////////
     -->


    


    <!-- http://purl.org/dc/terms/creator -->


    <owl:AnnotationProperty rdf:about="http://purl.org/dc/terms/creator"/>
    


    <!-- http://purl.org/dc/terms/dateCopyrighted -->


    <owl:AnnotationProperty rdf:about="http://purl.org/dc/terms/dateCopyrighted"/>
    


    <!-- http://purl.org/dc/terms/rightsHolder -->


    <owl:AnnotationProperty rdf:about="http://purl.org/dc/terms/rightsHolder"/>
    


    <!-- http://purl.org/vocab/vann/preferredNamespacePrefix -->


    <owl:AnnotationProperty rdf:about="http://purl.org/vocab/vann/preferredNamespacePrefix"/>
    


    <!-- http://purl.org/vocab/vann/preferredNamespaceUri -->


    <owl:AnnotationProperty rdf:about="http://purl.org/vocab/vann/preferredNamespaceUri"/>
    


    <!-- http://www.w3.org/ns/prov#hadPrimarySource -->


    <owl:AnnotationProperty rdf:about="http://www.w3.org/ns/prov#hadPrimarySource"/>
    


    <!-- 
    ///////////////////////////////////////////////////////////////////////////////////////
    //
    // Datatypes
    //
    ///////////////////////////////////////////////////////////////////////////////////////
     -->


    


    <!-- http://www.w3.org/2001/XMLSchema#duration -->


    <rdfs:Datatype rdf:about="http://www.w3.org/2001/XMLSchema#duration"/>
    


    <!-- 
    ///////////////////////////////////////////////////////////////////////////////////////
    //
    // Object Properties
    //
    ///////////////////////////////////////////////////////////////////////////////////////
     -->


    


    <!-- http://www.w3.org/2003/01/geo/wgs84_pos#location -->


    <owl:ObjectProperty rdf:about="http://www.w3.org/2003/01/geo/wgs84_pos#location">
        <rdfs:comment xml:lang="en">The relation between something and the point,  or other geometrical thing in space, where it is.  For example, the realtionship between a radio tower and a Point with a given lat and long. Or a relationship between a park and its outline as a closed arc of points, or a road and its location as a arc (a sequence of points). Clearly in practice there will be limit to the accuracy of any such statement, but one would expect an accuracy appropriate for the size of the object and uses such as mapping .</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#"/>
        <rdfs:label xml:lang="en">location</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#airFlowRateMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#airFlowRateMax">
        <rdfs:comment xml:lang="en">Maximum allowable air flow rate. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">air flow rate range max</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#airFlowRateMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#airFlowRateMin">
        <rdfs:comment xml:lang="en">Minimum allowable air flow rate. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">air flow rate range min</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#ambientDesignDryBulbTemperature -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#ambientDesignDryBulbTemperature">
        <rdfs:comment xml:lang="en">Ambient design dry bulb temperature used for selecting the cooling tower. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">ambient design dry bulb temperature</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#ambientDesignWetBulbTemperature -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#ambientDesignWetBulbTemperature">
        <rdfs:comment xml:lang="en">Ambient design wet bulb temperature used for selecting the cooling tower. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">ambient design wet bulb temperature</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#apparentPowerMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#apparentPowerMax">
        <rdfs:comment xml:lang="en">Maximum apparent power/capacity in VA (volt ampere). Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">maximum apparent power</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#audioVolume -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#audioVolume">
        <rdfs:comment xml:lang="en">Indicates discrete audio volume levels and corresponding sound power offsets, if applicable. Missing values may be interpolated. Measured in watts.</rdfs:comment>
        <rdfs:label xml:lang="en">audio volume</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#basinReserveVolume -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#basinReserveVolume">
        <rdfs:comment xml:lang="en">Volume between operating and overflow levels in cooling tower basin. Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">basin reserve volume</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#bladeThickness -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#bladeThickness">
        <rdfs:comment xml:lang="en">The thickness of the damper blade. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">blade thickness</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#bodyMass -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#bodyMass">
        <rdfs:comment xml:lang="en">Overall body mass of the heater. Usually measured in kilograms (kg) or grams (g).</rdfs:comment>
        <rdfs:label xml:lang="en">body mass</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#capacityWeight -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#capacityWeight">
        <rdfs:comment xml:lang="en">Capacity of the transport element measured by weight. Usually measured in kilograms (kg) or grams (g).</rdfs:comment>
        <rdfs:label xml:lang="en">capacity weight</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#closeOffRating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#closeOffRating">
        <rdfs:comment xml:lang="en">Close off rating. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">close off rating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#coilLength -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#coilLength">
        <rdfs:comment xml:lang="en">Length of coil. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">coil length</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#coilWidth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#coilWidth">
        <rdfs:comment xml:lang="en">Width of coil. Usually measured in millimeters (mm</rdfs:comment>
        <rdfs:label xml:lang="en">coil width</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#colorTemperature -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#colorTemperature">
        <rdfs:comment xml:lang="en">The color temperature of any source of radiation is defined as the temperature (in Kelvin) of a black-body or Planckian radiator whose radiation has the same chromaticity as the source of radiation. Often the values are only approximate color temperatures as the black-body radiator cannot emit radiation of every chromaticity value. The color temperatures of the commonest artificial light sources range from less than 3000K (warm white) to 4000K (intermediate) and over 5000K (daylight). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">color temperature</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#compressorSpeed -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#compressorSpeed">
        <rdfs:comment xml:lang="en">Compressor speed. Usually measured in cycles/s.</rdfs:comment>
        <rdfs:label xml:lang="en">compressor speed</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#connectionSize -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#connectionSize">
        <rdfs:comment xml:lang="en">The connection size of the to and from the pump. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">connection size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#contains -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#contains">
        <owl:inverseOf rdf:resource="https://w3id.org/def/saref4bldg#isContainedIn"/>
        <rdf:type rdf:resource="http://www.w3.org/2002/07/owl#TransitiveProperty"/>
        <rdfs:comment xml:lang="en">A relation between a physical space and the objects located in such space.</rdfs:comment>
        <rdfs:label xml:lang="en">contains</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#contributedLuminousFlux -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#contributedLuminousFlux">
        <rdfs:comment xml:lang="en">Luminous flux is a photometric measure of radiant flux, i.e. the volume of light emitted from a light source. Luminous flux is measured either for the interior as a whole or for a part of the interior (partial luminous flux for a solid angle). All other photometric parameters are derivatives of luminous flux. Luminous flux is measured in lumens (lm). The luminous flux is given as a nominal value for each lamp. Usually measured in Lumen (lm, Candela Steradian).</rdfs:comment>
        <rdfs:label xml:lang="en">contributed luminous flux</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#coverLength -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#coverLength">
        <rdfs:comment xml:lang="en">The length measured along the x-axis in the local coordinate system or the radius (in the case of a circular shape in plan) of the cover of the oil interceptor. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">cover length</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#coverWidth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#coverWidth">
        <rdfs:comment xml:lang="en">The length measured along the x-axis in the local coordinate system of the cover of the oil interceptor. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">cover width</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#effectiveCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#effectiveCapacity">
        <rdfs:comment xml:lang="en">The total effective or actual volumetric capacity of the tank. Usually measured in cubic metre (m3).B3</rdfs:comment>
        <rdfs:label xml:lang="en">effective capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#electricGeneratorEfficiency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#electricGeneratorEfficiency">
        <rdfs:comment xml:lang="en">The ratio of output capacity to intake capacity.</rdfs:comment>
        <rdfs:label xml:lang="en">electric generator efficiency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#electricMotorEfficiency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#electricMotorEfficiency">
        <rdfs:comment xml:lang="en">The ratio of output capacity to intake capacity.</rdfs:comment>
        <rdfs:label xml:lang="en">electric motor efficiency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#externalSurfaceArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#externalSurfaceArea">
        <rdfs:comment xml:lang="en">External surface area (both primary and secondary area). Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">external surface area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#faceArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#faceArea">
        <rdfs:comment xml:lang="en">Face area open to the airstream. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">face area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#finalResistance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#finalResistance">
        <rdfs:comment xml:lang="en">Filter fluid resistance when replacement is required (i.e., Pressure drop at the maximum air flowrate across the filter when the filter needs replacement per ASHRAE Standard 52.1). Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">final resistance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#firstCurvatureRadius -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#firstCurvatureRadius">
        <rdfs:comment xml:lang="en">FirstCurvatureRadius should be defined as the base or left side radius of curvature value. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">first curvature radius</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#flowCoefficient -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#flowCoefficient">
        <rdfs:comment xml:lang="en">Flow coefficient (the quantity of fluid that passes through a fully open valve at unit pressure drop), typically expressed as the Kv or Cv value for the valve.</rdfs:comment>
        <rdfs:label xml:lang="en">flow coefficient</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#flowResistanceMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#flowResistanceMax">
        <rdfs:comment xml:lang="en">Allowable range of frictional resistance against which the fluid is being pumped. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">flow resistance range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#flowResistanceMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#flowResistanceMin">
        <rdfs:comment xml:lang="en">Allowable range of frictional resistance against which the fluid is being pumped. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">flow resistance range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#fluidFlowRateMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#fluidFlowRateMax">
        <rdfs:comment xml:lang="en">Possible range of fluid flowrate that can be delivered. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">fluid flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#fluidFlowRateMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#fluidFlowRateMin">
        <rdfs:comment xml:lang="en">Possible range of fluid flowrate that can be delivered. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">fluid flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#foulingFactor -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#foulingFactor">
        <rdfs:comment xml:lang="en">Fouling factor of the tubes in the tube bundle. Usually measured in m2 Kelvin/Watt.</rdfs:comment>
        <rdfs:label xml:lang="en">fouling factor</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#frameDepth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#frameDepth">
        <rdfs:comment xml:lang="en">The length (or depth) of the damper frame. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">frame depth</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#frameThickness -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#frameThickness">
        <rdfs:comment xml:lang="en">The thickness of the damper frame material. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">frame thickness</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasSpace -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#hasSpace">
        <owl:inverseOf rdf:resource="https://w3id.org/def/saref4bldg#isSpaceOf"/>
        <rdf:type rdf:resource="http://www.w3.org/2002/07/owl#TransitiveProperty"/>
        <rdfs:comment xml:lang="en">Relation between a building or a building space and the spaces it can be divided into.</rdfs:comment>
        <rdfs:label xml:lang="en">has space</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#heatExchangeArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#heatExchangeArea">
        <rdfs:comment xml:lang="en">Heat exchange area. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">heat exchange area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#heatTransferSurfaceArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#heatTransferSurfaceArea">
        <rdfs:comment xml:lang="en">Total heat transfer area of the vessel. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">heat transfer surface area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#height -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#height">
        <rdfs:comment xml:lang="en">Height of the vibration isolator before tha application of load. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">height</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#horizontalSpacing -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#horizontalSpacing">
        <rdfs:comment xml:lang="en">Horizontal spacing between tubes in the tube bundle. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">horizontal spacing</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hydraulicDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#hydraulicDiameter">
        <rdfs:comment xml:lang="en">Hydraulic diameter. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">hydraulic diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#idealCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#idealCapacity">
        <rdfs:comment xml:lang="en">Compressor capacity under ideal conditions. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">ideal capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#idealShaftPower -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#idealShaftPower">
        <rdfs:comment xml:lang="en">Compressor shaft power under ideal conditions. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">ideal shaft power</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#imaginaryImpedanceRatio -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#imaginaryImpedanceRatio">
        <rdfs:comment xml:lang="en">The ratio between the imaginary part of the zero sequence impedance and the imaginary part of the positive impedance (i.e. imaginary part of the short-circuit voltage) of the transformer. Used for three-phase transformer which includes a N-conductor.</rdfs:comment>
        <rdfs:label xml:lang="en">imaginary impedance ratio</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#impellerDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#impellerDiameter">
        <rdfs:comment xml:lang="en">Diameter of compressor impeller - used to scale performance of geometrically similar compressors. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">impeller diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#inLineRowSpacing -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#inLineRowSpacing">
        <rdfs:comment xml:lang="en">In-line tube row spacing. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">in line row spacing</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#initialResistance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#initialResistance">
        <rdfs:comment xml:lang="en">Initial new filter fluid resistance (i.e., pressure drop at the maximum air flowrate across the filter when the filter is new per ASHRAE Standard 52.1). Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">initial resistance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#inletConnectionSize -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#inletConnectionSize">
        <rdfs:comment xml:lang="en">Size of the inlet connection. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">inlet connection size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#insideDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#insideDiameter">
        <rdfs:comment xml:lang="en">Actual inner diameter of the tube in the tube bundle. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">inside diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#internalRefrigerantVolume -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#internalRefrigerantVolume">
        <rdfs:comment xml:lang="en">Internal volume of evaporator (refrigerant side). Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">internal refrigerant volume</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#internalSurfaceArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#internalSurfaceArea">
        <rdfs:comment xml:lang="en">Internal surface area. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">internal surface area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#internalWaterVolume -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#internalWaterVolume">
        <rdfs:comment xml:lang="en">Internal volume of evaporator (water side). Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">internal water volume</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isContainedIn -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#isContainedIn">
        <rdf:type rdf:resource="http://www.w3.org/2002/07/owl#TransitiveProperty"/>
        <rdfs:comment xml:lang="en">A relation between an object and the physical space in which it is located.</rdfs:comment>
        <rdfs:label xml:lang="en">is contained in</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isSpaceOf -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#isSpaceOf">
        <rdf:type rdf:resource="http://www.w3.org/2002/07/owl#TransitiveProperty"/>
        <rdfs:comment xml:lang="en">Relation between a building space and the building or building space it belongs to.</rdfs:comment>
        <rdfs:label xml:lang="en">isSpaceOf</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isolatorCompressibility -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#isolatorCompressibility">
        <rdfs:comment xml:lang="en">The compressibility of the vibration isolator.</rdfs:comment>
        <rdfs:label xml:lang="en">isolator compressibility</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isolatorStaticDeflection -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#isolatorStaticDeflection">
        <rdfs:comment xml:lang="en">Static deflection of the vibration isolator. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">isolator static deflection</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#lampMaintenanceFactor -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#lampMaintenanceFactor">
        <rdfs:comment xml:lang="en">Non recoverable losses of luminous flux of a lamp due to lamp depreciation i.e. the decreasing of light output of a luminaire due to aging and dirt.</rdfs:comment>
        <rdfs:label xml:lang="en">lamp maintenance factor</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#leakageFullyClosed -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#leakageFullyClosed">
        <rdfs:comment xml:lang="en">Leakage when fully closed. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">leakage fully closed</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#length -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#length">
        <rdfs:comment xml:lang="en">The finished length of the device. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">length</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#liftElevationDifference -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#liftElevationDifference">
        <rdfs:comment xml:lang="en">Elevation difference between cooling tower sump and the top of the tower. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">lift elevation difference</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#lightEmitterNominalPower -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#lightEmitterNominalPower">
        <rdfs:comment xml:lang="en">Light emitter nominal power. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">light emitter nominal power</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#limitingTerminalSize -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#limitingTerminalSize">
        <rdfs:comment xml:lang="en">The maximum terminal size capacity of the device. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">limiting terminal size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#lockedRotorCurrent -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#lockedRotorCurrent">
        <rdfs:comment xml:lang="en">Input current when a motor armature is energized but not rotating. Usually measured in Ampere (A).</rdfs:comment>
        <rdfs:label xml:lang="en">locked rotor current</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#netPositiveSuctionHead -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#netPositiveSuctionHead">
        <rdfs:comment xml:lang="en">Minimum liquid pressure at the pump inlet to prevent cavitation. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">net positive suction head</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalAirFlowRate -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalAirFlowRate">
        <rdfs:comment xml:lang="en">Nominal rate of air flow. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal air flow rate</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalBodyDepth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalBodyDepth">
        <rdfs:comment xml:lang="en">Nominal or quoted =length, measured along the z-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal body depth</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalBodyLength -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalBodyLength">
        <rdfs:comment xml:lang="en">Nominal or quoted length, measured along the x-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal body length</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalBodyWidth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalBodyWidth">
        <rdfs:comment xml:lang="en">Nominal or quoted length, measured along the y-axis of the local coordinate system of the object, of the body of the object. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal body width</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalCapacity">
        <rdfs:comment xml:lang="en">Nominal capacity. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalCondensingTemperature -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalCondensingTemperature">
        <rdfs:comment xml:lang="en">Chiller condensing temperature. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal condensing temperature</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalCoolingCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalCoolingCapacity">
        <rdfs:comment xml:lang="en">Nominal cooling capacity. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal cooling capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalDepth -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalDepth">
        <rdfs:comment xml:lang="en">The nominal depth of the tank. Note: Not required for a horizontal cylindrical tank. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal depth</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalDiameter">
        <rdfs:comment xml:lang="en">Nominal diameter or width of the tubes in the tube bundle. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalEfficiency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalEfficiency">
        <rdfs:comment xml:lang="en">Nominal chiller efficiency under nominal conditions. </rdfs:comment>
        <rdfs:label xml:lang="en">nominal efficiency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalEnergyConsumption -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalEnergyConsumption">
        <rdfs:comment xml:lang="en">Nominal fuel consumption rate required to produce the total boiler heat output. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal energy consumption</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalEvaporatingTemmperature -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalEvaporatingTemmperature">
        <rdfs:comment xml:lang="en">Chiller evaporating temperature.Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal evaporating temmperature</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalFilterFaceVelocity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalFilterFaceVelocity">
        <rdfs:comment xml:lang="en">Filter face velocity. Usually measured in m/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal filter face velocity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalFlowRate -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalFlowRate">
        <rdfs:comment xml:lang="en">Nominal fluid flow rate through the filter. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal flow rate</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalFrequency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalFrequency">
        <rdfs:comment xml:lang="en">The nominal frequency of the supply. Usually measured in cycles/s or Hertz (Hz).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal frequency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalHeatRejectionRate -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalHeatRejectionRate">
        <rdfs:comment xml:lang="en">Sum of the refrigeration effect and the heat equivalent of the power input to the compressor. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal heat rejection rate</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalHeatTransferArea -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalHeatTransferArea">
        <rdfs:comment xml:lang="en">Nominal heat transfer surface area associated with nominal overall heat transfer coefficient. Usually measured in square metre (m2).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal heat transfer area</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalHeatTransferCoefficient -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalHeatTransferCoefficient">
        <rdfs:comment xml:lang="en">Nominal overall heat transfer coefficient associated with nominal heat transfer area. Usually measured in Watts/m2 Kelvin.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal heat transfer coefficient</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalHeatingCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalHeatingCapacity">
        <rdfs:comment xml:lang="en">Nominal heating capacity. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal heating capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalLatentCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalLatentCapacity">
        <rdfs:comment xml:lang="en">Nominal latent capacity. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal latent capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalLengthOrDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalLengthOrDiameter">
        <rdfs:comment xml:lang="en">The nominal length or, in the case of a vertical cylindrical tank, the nominal diameter of the tank. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal length or diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalMediaSurfaceVelocity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalMediaSurfaceVelocity">
        <rdfs:comment xml:lang="en">Average fluid velocity at the media surface. Usually measured in m/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal media surface velocity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalMoistureGain -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalMoistureGain">
        <rdfs:comment xml:lang="en">Nominal rate of water vapor added into the airstream. Usually measured in kg/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal moisture gain</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalPartLoadRatio -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalPartLoadRatio">
        <rdfs:comment xml:lang="en">Allowable part load ratio range.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal part load ratio</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalParticleGeometricMeanDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalParticleGeometricMeanDiameter">
        <rdfs:comment xml:lang="en">Particle geometric mean diameter associated with nominal efficiency. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal particle geometric mean diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalParticleGeometricStandardDeviation -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalParticleGeometricStandardDeviation">
        <rdfs:comment xml:lang="en">Particle geometric standard deviation associated with nominal efficiency. </rdfs:comment>
        <rdfs:label xml:lang="en">nominal particle geometric standard deviation</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalPowerConsumption -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalPowerConsumption">
        <rdfs:comment xml:lang="en">Nominal total power consumption. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal power consumption</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalPowerRate -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalPowerRate">
        <rdfs:comment xml:lang="en">Nominal fan power rate.Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal power rate</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalPressureDrop -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalPressureDrop">
        <rdfs:comment xml:lang="en">Total pressure drop across the filter. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal pressure drop</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureCooling -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureCooling">
        <rdfs:comment xml:lang="en">Nominal return water temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal return water temperature cooling</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureHeating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureHeating">
        <rdfs:comment xml:lang="en">Nominal return water temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal return water temperature heating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalRotationSpeed -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalRotationSpeed">
        <rdfs:comment xml:lang="en">Nominal fan wheel speed. Usually measured in cycles/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal rotation speed</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSensibleCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSensibleCapacity">
        <rdfs:comment xml:lang="en">Nominal sensible capacity. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal sensible capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSorroundingHumidityCooling -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSorroundingHumidityCooling">
        <rdfs:comment xml:lang="en">Nominal surrounding humidity (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal sorrounding humidity cooling</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureCooling -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureCooling">
        <rdfs:comment xml:lang="en">Nominal surrounding temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal sorrounding temperature cooling</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureHeating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureHeating">
        <rdfs:comment xml:lang="en">Nominal surrounding temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal sorrounding temperature heating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalStaticPressure -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalStaticPressure">
        <rdfs:comment xml:lang="en">The static pressure within the air stream that the fan must overcome to insure designed circulation of air. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal static pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSupplyVoltage -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSupplyVoltage">
        <rdfs:comment xml:lang="en">The nominal voltage of the supply. Usually measured in Volts (V, W/A).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal supply voltage</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSupplyVoltageMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSupplyVoltageMax">
        <rdfs:comment xml:lang="en">The maximum and minimum allowed voltage of the supply e.g. boundaries of 380V/440V may be applied for a nominal voltage of 400V.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal supply voltage offset</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSupplyVoltageMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSupplyVoltageMin">
        <rdfs:comment xml:lang="en">The maximum and minimum allowed voltage of the supply e.g. boundaries of 380V/440V may be applied for a nominal voltage of 400V.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal supply voltage offset</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureCooling -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureCooling">
        <rdfs:comment xml:lang="en">Nominal supply water temperature (refers to nominal cooling capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal supply water temperature cooling</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureHeating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureHeating">
        <rdfs:comment xml:lang="en">Nominal supply water temperature (refers to nominal heating capacity). Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal supply water temperature heating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalTotalPressure -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalTotalPressure">
        <rdfs:comment xml:lang="en">Nominal total pressure rise across the fan. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal total pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalUa -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalUa">
        <rdfs:comment xml:lang="en">Nominal UA value.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal ua</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalVolumetricCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalVolumetricCapacity">
        <rdfs:comment xml:lang="en">The total nominal or design volumetric capacity of the tank. Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal volumetric capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalWaterFlowCooling -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalWaterFlowCooling">
        <rdfs:comment xml:lang="en">Nominal water flow (refers to nominal cooling capacity). Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal water flow cooling</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalWaterFlowHeating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalWaterFlowHeating">
        <rdfs:comment xml:lang="en">Nominal water flow (refers to nominal heating capacity). Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nominal water flow heating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nominalWidthOrDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nominalWidthOrDiameter">
        <rdfs:comment xml:lang="en">The nominal width or, in the case of a horizontal cylindrical tank, the nominal diameter of the tank. Note: Not required for a vertical cylindrical tank. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">nominal width or diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#nomminalRotationSpeed -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#nomminalRotationSpeed">
        <rdfs:comment xml:lang="en">Pump rotational speed under nominal conditions. Usually measured in cycles/s.</rdfs:comment>
        <rdfs:label xml:lang="en">nomminal rotation speed</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#openPressureDrop -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#openPressureDrop">
        <rdfs:comment xml:lang="en">Total pressure drop across damper. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">open pressure drop</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operatingWight -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#operatingWight">
        <rdfs:comment xml:lang="en">Operating weight of the tank including all of its contents. Usually measured in kilograms (kg) or grams (g).</rdfs:comment>
        <rdfs:label xml:lang="en">operating wight</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operationTemperatureMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#operationTemperatureMax">
        <rdfs:comment xml:lang="en">Allowable operation ambient (air, fluid) temperature range. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">operation temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operationTemperatureMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#operationTemperatureMin">
        <rdfs:comment xml:lang="en">Allowable operation ambient (air, fluid) temperature range. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">operation temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operationalRiterial -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#operationalRiterial">
        <rdfs:comment xml:lang="en">Time of operation at maximum operational ambient air temperature. Measured in seconds (s) or days (d) or other units of time.</rdfs:comment>
        <rdfs:label xml:lang="en">operational riterial</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#outletConnectionSize -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#outletConnectionSize">
        <rdfs:comment xml:lang="en">Size of the outlet connection. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">outlet connection size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#outletTemperatureMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#outletTemperatureMax">
        <rdfs:comment xml:lang="en">Allowable outlet temperature of either the water or the steam. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">outlet temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#outletTemperatureMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#outletTemperatureMin">
        <rdfs:comment xml:lang="en">Allowable outlet temperature of either the water or the steam. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">outlet temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#outputCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#outputCapacity">
        <rdfs:comment xml:lang="en">Total nominal heat output as listed by the manufacturer. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">output capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#outsideDiameter -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#outsideDiameter">
        <rdfs:comment xml:lang="en">Actual outside diameter of the tube in the tube bundle. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">outside diameter</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#partLoadRatioMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#partLoadRatioMax">
        <rdfs:comment xml:lang="en">Maximum part load ratio as a fraction of nominal capacity.</rdfs:comment>
        <rdfs:label xml:lang="en">maximum part load ratio</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#partLoadRatioMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#partLoadRatioMin">
        <rdfs:comment xml:lang="en">Minimum part load ratio as a fraction of nominal capacity.</rdfs:comment>
        <rdfs:label xml:lang="en">minimum part load ratio</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#powerOutputMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#powerOutputMax">
        <rdfs:comment xml:lang="en">The maximum output power rating of the engine. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">maximum power output</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#pressureRating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#pressureRating">
        <rdfs:comment xml:lang="en">Nominal pressure rating of the boiler as rated by the agency having jurisdiction. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">pressure rating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryAirFlowRateMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryAirFlowRateMax">
        <rdfs:comment xml:lang="en">Maximum primary airflow that can be delivered. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">primary air flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryAirFlowRateMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryAirFlowRateMin">
        <rdfs:comment xml:lang="en">Minimum primary airflow that can be delivered. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">primary air flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryApparentPower -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryApparentPower">
        <rdfs:comment xml:lang="en">The power in VA (volt ampere) that has been transformed and that runs into the transformer on the primary side. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">primary apparent power</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryCurrent -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryCurrent">
        <rdfs:comment xml:lang="en">The current that is going to be transformed and that runs into the transformer on the primary side. Usually measured in Ampere (A).</rdfs:comment>
        <rdfs:label xml:lang="en">primary current</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryFrequency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryFrequency">
        <rdfs:comment xml:lang="en">The frequency that is going to be transformed and that runs into the transformer on the primary side. Usually measured in cycles/s or Hertz (Hz).</rdfs:comment>
        <rdfs:label xml:lang="en">primary frequency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#primaryVoltage -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#primaryVoltage">
        <rdfs:comment xml:lang="en">The voltage that is going to be transformed and that runs into the transformer on the primary side. Usually measured in Volts (V, W/A).</rdfs:comment>
        <rdfs:label xml:lang="en">primary voltage</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#pumpFlowRateMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#pumpFlowRateMax">
        <rdfs:comment xml:lang="en">Allowable range of volume of fluid being pumped against the resistance specified. Usually measured in kg/s.</rdfs:comment>
        <rdfs:label xml:lang="en">pump flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#pumpFlowRateMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#pumpFlowRateMin">
        <rdfs:comment xml:lang="en">Allowable range of volume of fluid being pumped against the resistance specified. Usually measured in kg/s.</rdfs:comment>
        <rdfs:label xml:lang="en">pump flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#realImpedanceRatio -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#realImpedanceRatio">
        <rdfs:comment xml:lang="en">The ratio between the real part of the zero sequence impedance and the real part of the positive impedance (i.e. real part of the short-circuit voltage) of the transformer. Used for three-phase transformer which includes a N-conductor.</rdfs:comment>
        <rdfs:label xml:lang="en">real impedance ratio</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondCurvatureRadius -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondCurvatureRadius">
        <rdfs:comment xml:lang="en">SecondCurvatureRadius should be defined as the top or right side radius of curvature value. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">second curvature radius</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryAirFlowRateMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryAirFlowRateMax">
        <rdfs:comment xml:lang="en">Maximum secondary airflow that can be delivered. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary air flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryAirFlowRateMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryAirFlowRateMin">
        <rdfs:comment xml:lang="en">Maximum secondary airflow that can be delivered. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary air flow rate range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryApparentPower -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryApparentPower">
        <rdfs:comment xml:lang="en">The power in VA (volt ampere) that has been transformed and is running out of the transformer on the secondary side. Usually measured in Watts (W, J/s).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary apparent power</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryCurrent -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryCurrent">
        <rdfs:comment xml:lang="en">The current that has been transformed and is running out of the transformer on the secondary side. Usually measured in Ampere (A).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary current</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryFrequency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryFrequency">
        <rdfs:comment xml:lang="en">The frequency that has been transformed and is running out of the transformer on the secondary side. Usually measured in cycles/s or Hertz (Hz).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary frequency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryVoltage -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryVoltage">
        <rdfs:comment xml:lang="en">The voltage that has been transformed and is running out of the transformer on the secondary side. Usually measured in Volts (V, W/A).</rdfs:comment>
        <rdfs:label xml:lang="en">secondary voltage</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#shortCircuitVoltage -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#shortCircuitVoltage">
        <rdfs:comment xml:lang="en">A complex number that specifies the real and imaginary parts of the short-circuit voltage at rated current of a transformer given in %.</rdfs:comment>
        <rdfs:label xml:lang="en">short circuit voltage</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#size -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#size">
        <rdfs:comment xml:lang="en">The size of the connection to the valve (or to each connection for faucets, mixing valves, etc.). Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#solarReflectance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#solarReflectance">
        <rdfs:comment xml:lang="en">(Rsol): The ratio of incident solar radiation that is reflected by a shading system (also named _e). Note the following equation Asol + Rsol + Tsol = 1</rdfs:comment>
        <rdfs:label xml:lang="en">solar reflectance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#solarTransmittance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#solarTransmittance">
        <rdfs:comment xml:lang="en">(Tsol) The ratio of incident solar radiation that directly passes through a shading system (also named _e). Note the following equation Asol + Rsol + Tsol = 1</rdfs:comment>
        <rdfs:label xml:lang="en">solar transmittance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#spectrumMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#spectrumMax">
        <rdfs:comment xml:lang="en">The spectrum of radiation describes its composition with regard to wavelength. Light, for example, as the portion of electromagnetic radiation that is visible to the human eye, is radiation with wavelengths in the range of approx. 380 to 780 nm (1 nm = 10 m). The corresponding range of colours varies from violet to indigo, blue, green, yellow, orange, and red. These colours form a continuous spectrum, in which the various spectral sectors merge into each other.</rdfs:comment>
        <rdfs:label xml:lang="en">maximum spectrum</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#spectrumMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#spectrumMin">
        <rdfs:comment xml:lang="en">The spectrum of radiation describes its composition with regard to wavelength. Light, for example, as the portion of electromagnetic radiation that is visible to the human eye, is radiation with wavelengths in the range of approx. 380 to 780 nm (1 nm = 10 m). The corresponding range of colours varies from violet to indigo, blue, green, yellow, orange, and red. These colours form a continuous spectrum, in which the various spectral sectors merge into each other.</rdfs:comment>
        <rdfs:label xml:lang="en">minimum spectrum</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#staggeredRowSpacing -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#staggeredRowSpacing">
        <rdfs:comment xml:lang="en">Staggered tube row spacing. Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">staggered row spacing</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#startCurrentFactor -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#startCurrentFactor">
        <rdfs:comment xml:lang="en">IEC. Start current factor defines how large the peek starting current will become on the engine. StartCurrentFactor is multiplied to NominalCurrent and we get the start current.</rdfs:comment>
        <rdfs:label xml:lang="en">start current factor</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#startingTime -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#startingTime">
        <rdfs:comment xml:lang="en">The time (in s) needed for the motor to reach its rated speed with its driven equipment attached, starting from standstill and at the nominal voltage applied at its terminals.</rdfs:comment>
        <rdfs:label xml:lang="en">starting time</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#supportedWeightMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#supportedWeightMax">
        <rdfs:comment xml:lang="en">The maximum weight that can be carried by the vibration isolator. Usually measured in kilograms (kg) or grams (g).</rdfs:comment>
        <rdfs:label xml:lang="en">maximum supported weight</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#teTime -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#teTime">
        <rdfs:comment xml:lang="en">The maximum time (in s) at which the motor could run with locked rotor when the motor is used in an EX-environment. The time indicates that a protective device should trip before this time when the starting current of the motor is slowing through the device.</rdfs:comment>
        <rdfs:label xml:lang="en">te time</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#temperatureRating -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#temperatureRating">
        <rdfs:comment xml:lang="en">Temperature rating. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">temperature rating</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#testPressure -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#testPressure">
        <rdfs:comment xml:lang="en">The maximum pressure to which the valve has been subjected under test. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">test pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#thermalConductivity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#thermalConductivity">
        <rdfs:comment xml:lang="en">Fouling factor of the tubes in the tube bundle. Usually measured in m2 Kelvin/Watt.</rdfs:comment>
        <rdfs:label xml:lang="en">thermal conductivity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#thermalEfficiency -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#thermalEfficiency">
        <rdfs:comment xml:lang="en">Overall Thermal Efficiency is defined as gross energy output of the heat transfer device divided by the energy input.</rdfs:comment>
        <rdfs:label xml:lang="en">thermal efficiency</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#thermalMassHeatCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#thermalMassHeatCapacity">
        <rdfs:comment xml:lang="en">Product of component mass and specific heat.</rdfs:comment>
        <rdfs:label xml:lang="en">thermal mass heat capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#thermalTransmittance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#thermalTransmittance">
        <rdfs:comment xml:lang="en">Rate at which energy is transmitted through a body. Usually measured in Watts/m2 Kelvin.</rdfs:comment>
        <rdfs:label xml:lang="en">thermal transmittance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#ventilatingPipeSize -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#ventilatingPipeSize">
        <rdfs:comment xml:lang="en">Size of the ventilating pipe(s). Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">ventilating pipe size</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#verticalSpacing -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#verticalSpacing">
        <rdfs:comment xml:lang="en">Vertical spacing between tubes in the tube bundle.Usually measured in millimeters (mm).</rdfs:comment>
        <rdfs:label xml:lang="en">vertical spacing</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#vibrationTransmissibility -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#vibrationTransmissibility">
        <rdfs:comment xml:lang="en">The vibration transmissibility percentage.</rdfs:comment>
        <rdfs:label xml:lang="en">vibration transmissibility</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#visibleLightReflectance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#visibleLightReflectance">
        <rdfs:comment xml:lang="en">Fraction of the visible light that is reflected by the glazing at normal incidence. It is a value without unit.</rdfs:comment>
        <rdfs:label xml:lang="en">visible light reflectance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#visibleLightTransmittance -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#visibleLightTransmittance">
        <rdfs:comment xml:lang="en">Fraction of the visible light that passes the shading system at normal incidence. It is a value without unit.</rdfs:comment>
        <rdfs:label xml:lang="en">visible light transmittance</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#volumen -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#volumen">
        <rdfs:comment xml:lang="en">Total volume of fluid in the tubes and their headers. Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">volumen</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterInletTemperatureMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterInletTemperatureMax">
        <rdfs:comment xml:lang="en">Allowable water inlet temperature range. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">water inlet temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterInletTemperatureMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterInletTemperatureMin">
        <rdfs:comment xml:lang="en">Allowable water inlet temperature range. Usually measured in degrees Kelvin (K).</rdfs:comment>
        <rdfs:label xml:lang="en">water inlet temperature range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterPressureMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterPressureMax">
        <rdfs:comment xml:lang="en">Allowable water circuit working pressure range. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">water pressure range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterPressureMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterPressureMin">
        <rdfs:comment xml:lang="en">Allowable water circuit working pressure range. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">water pressure range</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterRequirement -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterRequirement">
        <rdfs:comment xml:lang="en">Make-up water requirement. Usually measured in m3/s.</rdfs:comment>
        <rdfs:label xml:lang="en">water requirement</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterStorageCapacity -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#waterStorageCapacity">
        <rdfs:comment xml:lang="en">Water storage capacity. Usually measured in cubic metre (m3).</rdfs:comment>
        <rdfs:label xml:lang="en">water storage capacity</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#weight -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#weight">
        <rdfs:comment xml:lang="en">The weight of the device. Usually measured in kilograms (kg) or grams (g).</rdfs:comment>
        <rdfs:label xml:lang="en">weight</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#workingPressure -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#workingPressure">
        <rdfs:comment xml:lang="en">The normally expected maximum working pressure of the valve. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">working pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#workingPressureMax -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#workingPressureMax">
        <rdfs:comment xml:lang="en">Maximum working pressure. Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">maximum working pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/def/saref4bldg#workingPressureMin -->


    <owl:ObjectProperty rdf:about="https://w3id.org/def/saref4bldg#workingPressureMin">
        <rdfs:comment xml:lang="en">Allowable minimum working pressure (relative to ambient pressure). Usually measured in Pascals (Pa, N/m2).</rdfs:comment>
        <rdfs:label xml:lang="en">minimum working pressure</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/saref#isMeasuredIn -->


    <owl:ObjectProperty rdf:about="https://w3id.org/saref#isMeasuredIn">
        <rdfs:comment xml:lang="en">A relation between a measurement and the unit of measure in which the measurement value is expressed.</rdfs:comment>
        <rdfs:isDefinedBy rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/saref#</rdfs:isDefinedBy>
        <rdfs:label xml:lang="en">is measured in</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- https://w3id.org/saref#relatesToProperty -->


    <owl:ObjectProperty rdf:about="https://w3id.org/saref#relatesToProperty">
        <rdfs:comment xml:lang="en">A relation between a measurement and the property such measurement is about.</rdfs:comment>
        <rdfs:isDefinedBy rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/saref#</rdfs:isDefinedBy>
        <rdfs:label xml:lang="en">relates to property</rdfs:label>
    </owl:ObjectProperty>
    


    <!-- 
    ///////////////////////////////////////////////////////////////////////////////////////
    //
    // Data properties
    //
    ///////////////////////////////////////////////////////////////////////////////////////
     -->


    


    <!-- https://w3id.org/def/saref4bldg#accessType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#accessType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Defines the types of access (or cover) to a tank that may be specified. Note that covers are generally specified for rectangular tanks. For cylindrical tanks, access will normally be via a manhole.</rdfs:comment>
        <rdfs:label xml:lang="en">access type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#application -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#application">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Humidifier application. Fixed: Humidifier installed in a ducted flow distribution system. Portable: Humidifier is not installed in a ducted flow distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">application</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#arrangement -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#arrangement">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Defines the basic flow arrangements for the heat exchanger: COUNTERFLOW: Counterflow heat exchanger arrangement. CROSSFLOW: Crossflow heat exchanger arrangement. PARALLELFLOW: Parallel flow heat exchanger arrangement. MULTIPASS: Multipass flow heat exchanger arrangement. OTHER: Other type of heat exchanger flow arrangement not defined above.</rdfs:comment>
        <rdfs:label xml:lang="en">arrangement</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#bladeAction -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#bladeAction">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Blade action.</rdfs:comment>
        <rdfs:label xml:lang="en">blade action</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#bladeEdge -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#bladeEdge">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Blade edge.</rdfs:comment>
        <rdfs:label xml:lang="en">blade edge</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#bladeShape -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#bladeShape">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Blade shape. Flat means triple V-groove.</rdfs:comment>
        <rdfs:label xml:lang="en">blade shape</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#capacityControl -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#capacityControl">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">FanCycling: Fan is cycled on and off to control duty. TwoSpeedFan: Fan is switched between low and high speed to control duty. VariableSpeedFan: Fan speed is varied to control duty. DampersControl: Dampers modulate the air flow to control duty. BypassValveControl: Bypass valve modulates the water flow to control duty. MultipleSeriesPumps: Turn on/off multiple series pump to control duty. TwoSpeedPump: Switch between high/low pump speed to control duty. VariableSpeedPump: vary pump speed to control duty.</rdfs:comment>
        <rdfs:label xml:lang="en">capacity control</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#capacityControlType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#capacityControlType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">InletVane: Control by adjusting inlet vane. VariableSpeedDrive: Control by variable speed drive. BladePitchAngle: Control by adjusting blade pitch angle. TwoSpeed: Control by switch between high and low speed. DischargeDamper: Control by modulating discharge damper.</rdfs:comment>
        <rdfs:label xml:lang="en">capacity control type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#capacityPeople -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#capacityPeople">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#nonNegativeInteger"/>
        <rdfs:comment xml:lang="en">Capacity of the transportation element measured in numbers of person.</rdfs:comment>
        <rdfs:label xml:lang="en">capacity people</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#circuitType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#circuitType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">OpenCircuit: Exposes water directly to the cooling atmosphere. CloseCircuit: The fluid is separated from the atmosphere by a heat exchanger. Wet: The air stream or the heat exchange surface is evaporatively cooled. Dry: No evaporation into the air stream. DryWet: A combination of a dry tower and a wet tower.</rdfs:comment>
        <rdfs:label xml:lang="en">circuit type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#colorAppearance -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#colorAppearance">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">In both the DIN and CIE standards, artificial light sources are classified in terms of their color appearance. To the human eye they all appear to be white the difference can only be detected by direct comparison. Visual performance is not directly affected by differences in color appearance.</rdfs:comment>
        <rdfs:label xml:lang="en">color appearance</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#colorRenderingIndex -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#colorRenderingIndex">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">The CRI indicates how well a light source renders eight standard colors compared to perfect reference lamp with the same color temperature. The CRI scale ranges from 1 to 100, with 100 representing perfect rendering properties.</rdfs:comment>
        <rdfs:label xml:lang="en">color rendering index</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#controlStrategy -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#controlStrategy">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">FixedExitingWaterTemp: The capacity is controlled to maintain a fixed exiting water temperature. WetBulbTempReset: The set-point is reset based on the wet-bulb temperature.</rdfs:comment>
        <rdfs:label xml:lang="en">control strategy</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#endShapeType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#endShapeType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Defines the types of end shapes that can be used for preformed tanks. The convention for reading these enumerated values is that for a vertical cylinder, the first value is the base and the second is the top for a horizontal cylinder, the order of reading should be left to right. For a speherical tank, the value UNSET should be used.B5</rdfs:comment>
        <rdfs:label xml:lang="en">end shape type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#energySource -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#energySource">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Enumeration defining the energy source or fuel cumbusted to generate heat.</rdfs:comment>
        <rdfs:comment xml:lang="en">The source of energy.</rdfs:comment>
        <rdfs:label xml:lang="en">energy source</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#evaporationCoolant -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#evaporationCoolant">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The fluid used for the coolant in the evaporator.</rdfs:comment>
        <rdfs:label xml:lang="en">evaporation coolant</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#evaporationMediumType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#evaporationMediumType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">ColdLiquid: Evaporator is using liquid type of fluid to exchange heat with refrigerant. ColdAir: Evaporator is using air to exchange heat with refrigerant.</rdfs:comment>
        <rdfs:label xml:lang="en">evaporation medium type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#failPosition -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#failPosition">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Specifies the required fail-safe position of the actuator.</rdfs:comment>
        <rdfs:label xml:lang="en">fail position</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#finishColor -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#finishColor">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Finish color for cooled beam.</rdfs:comment>
        <rdfs:label xml:lang="en">finish color</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#fireExit -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#fireExit">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication whether this object is designed to serve as an exit in the case of fire (TRUE) or not (FALSE). Here whether the transport element (in case of e.g., a lift) is designed to serve as a fire exit, e.g., for fire escape purposes.</rdfs:comment>
        <rdfs:label xml:lang="en">fire exit</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#flowArrangement -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#flowArrangement">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">CounterFlow: Air and water flow enter in different directions. CrossFlow: Air and water flow are perpendicular. ParallelFlow: air and water flow enter in same directions.</rdfs:comment>
        <rdfs:label xml:lang="en">flow arrangement</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#frameSize -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#frameSize">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Designation of the frame size according to the named range of frame sizes designated at the place of use or according to a given standard.</rdfs:comment>
        <rdfs:label xml:lang="en">frame size</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#frameType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#frameType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The type of frame used by the damper (e.g., Standard, Single Flange, Single Reversed Flange, Double Flange, etc.).</rdfs:comment>
        <rdfs:label xml:lang="en">frame type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasDefrost -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasDefrost">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Whether the heat exchanger has defrost function or not.</rdfs:comment>
        <rdfs:label xml:lang="en">has defrost</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasExteriorInsulation -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasExteriorInsulation">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">TRUE if the silencer has exterior insulation. FALSE if it does not.</rdfs:comment>
        <rdfs:label xml:lang="en">has exterior insulation</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasHotGasBypass -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasHotGasBypass">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Whether or not hot gas bypass is provided for the compressor. TRUE = Yes, FALSE = No.</rdfs:comment>
        <rdfs:label xml:lang="en">has hot gas bypass</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasLock -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasLock">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication of whether a switching device has a key operated lock (=TRUE) or not (= FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">has lock</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasPartWinding -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasPartWinding">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication of whether the motor is single speed, i.e. has a single winding (= FALSE) or multi-speed i.e.has part winding (= TRUE) .</rdfs:comment>
        <rdfs:label xml:lang="en">has part winding</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#hasTurbulator -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#hasTurbulator">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">TRUE if the tube has a turbulator, FALSE if it does not.</rdfs:comment>
        <rdfs:label xml:lang="en">has turbulator</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#heatTransferDimension -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#heatTransferDimension">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Indicates how heat is transmitted according to the shape of the space heater.</rdfs:comment>
        <rdfs:label xml:lang="en">heat transfer dimension</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#heatTransferMedium -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#heatTransferMedium">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Enumeration defining the heat transfer medium if applicable.</rdfs:comment>
        <rdfs:label xml:lang="en">heat transfer medium</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#heatTransferTypeEnum -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#heatTransferTypeEnum">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Type of heat transfer between the two air streams.</rdfs:comment>
        <rdfs:label xml:lang="en">heat transfer type enum</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#integratedLightingType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#integratedLightingType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Integrated lighting in cooled beam.</rdfs:comment>
        <rdfs:label xml:lang="en">integrated lighting type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#internalControl -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#internalControl">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Internal modulation control.</rdfs:comment>
        <rdfs:label xml:lang="en">internal control</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isExternal -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isExternal">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication whether the element is designed for use in the exterior (TRUE) or not (FALSE). If (TRUE) it is an external element and faces the outside of the building.</rdfs:comment>
        <rdfs:label xml:lang="en">is external</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isFreeHanging -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isFreeHanging">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Is it free hanging type (not mounted in a false ceiling)?</rdfs:comment>
        <rdfs:label xml:lang="en">is free hanging</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isGuarded -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isGuarded">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication of whether the motor enclosure is guarded (= TRUE) or not (= FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">is guarded</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isIlluminated -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isIlluminated">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">An indication of whether there is an illuminated indicator to show that the switch is on (=TRUE) or not (= FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">is illuminated</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isNeutralPrimaryTerminalAvailable -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isNeutralPrimaryTerminalAvailable">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">An indication of whether the neutral point of the primary winding is available as a terminal (=TRUE) or not (= FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">is neutral primary terminal available</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isNeutralSecondaryTerminalAvailable -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isNeutralSecondaryTerminalAvailable">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">An indication of whether the neutral point of the secondary winding is available as a terminal (=TRUE) or not (= FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">is neutral secondary terminal available</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isPluggableOutlet -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isPluggableOutlet">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication of whether the outlet accepts a loose plug connection (= TRUE) or whether it is directly connected (= FALSE) or whether the form of connection has not yet been determined (= UNKNOWN).</rdfs:comment>
        <rdfs:label xml:lang="en">is pluggable outlet</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#isWaterStorageHeater -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#isWaterStorageHeater">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">This is used to identify if the boiler has storage capacity (TRUE). If FALSE, then there is no storage capacity built into the boiler, such as an instantaneous hot water heater.</rdfs:comment>
        <rdfs:label xml:lang="en">is water storage heater</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#lampBallastType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#lampBallastType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The type of ballast used to stabilise gas discharge by limiting the current during operation and to deliver the necessary striking voltage for starting. Ballasts are needed to operate Discharge Lamps such as Fluorescent, Compact Fluorescent, High-pressure Mercury, Metal Halide and High-pressure Sodium Lamps. Magnetic ballasts are chokes which limit the current passing through a lamp connected in series on the principle of self-induction. The resultant current and power are decisive for the efficient operation of the lamp. A specially designed ballast is required for every type of lamp to comply with lamp rating in terms of Luminous Flux, Color Appearance and service life. The two types of magnetic ballasts for fluorescent lamps are KVG Conventional (EC-A series) and VVG Low-loss ballasts (EC-B series). Low-loss ballasts have a higher efficiency, which means reduced ballast losses and a lower thermal load. Electronic ballasts are used to run fluorescent lamps at high frequencies (approx. 35 - 40 kHz).</rdfs:comment>
        <rdfs:label xml:lang="en">lamp ballast type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#lampCompensationType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#lampCompensationType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Identifies the form of compensation used for power factor correction and radio suppression.</rdfs:comment>
        <rdfs:label xml:lang="en">lamp compensation type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#legend -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#legend">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">A text inscribed or applied to the switch as a legend to indicate purpose or function.</rdfs:comment>
        <rdfs:label xml:lang="en">legend</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#manualOverride -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#manualOverride">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Identifies whether hand-operated operation is provided as an override (= TRUE) or not (= FALSE). Note that this value should be set to FALSE by default in the case of a Hand Operated Actuator.</rdfs:comment>
        <rdfs:label xml:lang="en">manual override</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#mechanicalOperated -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#mechanicalOperated">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indication whether the element is operated machanically (TRUE) or not, i.e. manually (FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">mechanical operated</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#mediaSource -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#mediaSource">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Indicates media sources and corresponding names of ports (DistributionPort with FlowDirection=SINK and PredefinedType=AUDIOVISUAL) or aggregated audio/video components (AudioVisualAppliance).</rdfs:comment>
        <rdfs:label xml:lang="en">media source</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#motorDriveType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#motorDriveType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Motor drive type: DIRECTDRIVE: Direct drive. BELTDRIVE: Belt drive. COUPLING: Coupling. OTHER: Other type of motor drive. UNKNOWN: Unknown motor drive type. </rdfs:comment>
        <rdfs:label xml:lang="en">motor drive type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#motorEnclosureType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#motorEnclosureType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">A list of the available types of motor enclosure from which that required may be selected.</rdfs:comment>
        <rdfs:label xml:lang="en">motor enclosure type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfBlades -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfBlades">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of blades.</rdfs:comment>
        <rdfs:label xml:lang="en">number of blades</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfCells -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfCells">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of cells in one cooling tower unit.</rdfs:comment>
        <rdfs:label xml:lang="en">number of cells</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfCircuits -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfCircuits">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of parallel fluid tube circuits.</rdfs:comment>
        <rdfs:label xml:lang="en">number of circuits</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfGangs -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfGangs">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of gangs/buttons on this switch.</rdfs:comment>
        <rdfs:label xml:lang="en">number of gangs</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfPanels -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfPanels">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of panels.</rdfs:comment>
        <rdfs:label xml:lang="en">number of panels</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfRows -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfRows">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of tube rows in the tube bundle assembly.</rdfs:comment>
        <rdfs:label xml:lang="en">number of rows</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOfSections -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOfSections">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">Number of sections used.</rdfs:comment>
        <rdfs:label xml:lang="en">number of sections</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#numberOsSockets -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#numberOsSockets">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
        <rdfs:comment xml:lang="en">The number of sockets that may be connected. In case of inconsistency, sockets defined on ports take precedence.</rdfs:comment>
        <rdfs:label xml:lang="en">number os sockets</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operatingMode -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#operatingMode">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Identifies the operating mode of the boiler.</rdfs:comment>
        <rdfs:label xml:lang="en">operating mode</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#operation -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#operation">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The operational mechanism for the damper operation.</rdfs:comment>
        <rdfs:label xml:lang="en">operation</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#orientation -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#orientation">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The intended orientation for the damper as specified by the manufacturer.</rdfs:comment>
        <rdfs:label xml:lang="en">orientation</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#patternType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#patternType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Defines the types of pattern (or shape of a tank that may be specified.</rdfs:comment>
        <rdfs:label xml:lang="en">pattern type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#pipeConnectionEnum -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#pipeConnectionEnum">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The manner in which the pipe connection is made to the cooled beam.</rdfs:comment>
        <rdfs:label xml:lang="en">pipe connection enum</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#placementType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#placementType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Indicates how the device is designed to be placed.</rdfs:comment>
        <rdfs:label xml:lang="en">placement type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#powerSource -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#powerSource">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Type of power driving the compressor.</rdfs:comment>
        <rdfs:label xml:lang="en">power source</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#readOutType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#readOutType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Indication of the form that readout from the meter takes. In the case of a dial read out, this may comprise multiple dials that give a cumulative reading and/or a mechanical odometer.</rdfs:comment>
        <rdfs:label xml:lang="en">read out type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#refrigerantClass -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#refrigerantClass">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Refrigerant class used by the compressor. CFC: Chlorofluorocarbons. HCFC: Hydrochlorofluorocarbons. HFC: Hydrofluorocarbons.</rdfs:comment>
        <rdfs:label xml:lang="en">refrigerant class</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#remoteReading -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#remoteReading">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
        <rdfs:comment xml:lang="en">Indicates whether the meter has a connection for remote reading through connection of a communication device (set TRUE) or not (set FALSE).</rdfs:comment>
        <rdfs:label xml:lang="en">remote reading</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#roughness -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#roughness">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">A measure of the vertical deviations of the surface.</rdfs:comment>
        <rdfs:label xml:lang="en">roughness</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#secondaryCurrentType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#secondaryCurrentType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">A list of the secondary current types that can result from transformer output.</rdfs:comment>
        <rdfs:label xml:lang="en">secondary current type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#shadingDeviceType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#shadingDeviceType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Specifies the type of shading device.</rdfs:comment>
        <rdfs:label xml:lang="en">shading device type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#sprayType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#sprayType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">SprayFilled: Water is sprayed into airflow. SplashTypeFill: water cascades over successive rows of splash bars. FilmTypeFill: water flows in a thin layer over closely spaced sheets.</rdfs:comment>
        <rdfs:label xml:lang="en">spray type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#standard -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#standard">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The designation of the standard applicable for the definition of the characteristics of the unit.</rdfs:comment>
        <rdfs:label xml:lang="en">standard</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#storageType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#storageType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Defines the general material category intended to be stored.</rdfs:comment>
        <rdfs:label xml:lang="en">storage type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#switchFunction -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#switchFunction">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Indicates types of switches which differs in functionality.</rdfs:comment>
        <rdfs:label xml:lang="en">switch function</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#temperatureClassification -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#temperatureClassification">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Enumeration defining the temperature classification of the space heater surface temperature. low temperature - surface temperature is relatively low, usually heated by hot water or electricity. high temperature - surface temperature is relatively high, usually heated by gas or steam.</rdfs:comment>
        <rdfs:label xml:lang="en">temperature classification</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#transformerVectorGroup -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#transformerVectorGroup">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">List of the possible vector groups for the transformer from which that required may be set. Values in the enumeration list follow a standard international code where the first letter describes how the primary windings are connected, the second letter describes how the secondary windings are connected, and the numbers describe the rotation of voltages and currents from the primary to the secondary side in multiples of 30 degrees. D: means that the windings are delta-connected. Y: means that the windings are star-connected. Z: means that the windings are zig-zag connected (a special start-connected providing low reactance of the transformer). The connectivity is only relevant for three-phase transformers.</rdfs:comment>
        <rdfs:label xml:lang="en">transformer vector group</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#valveMechanism -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#valveMechanism">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The mechanism by which the valve function is achieved where: BALL: Valve that has a ported ball that can be turned relative to the body seat ports. BUTTERFLY: Valve in which a streamlined disc pivots about a diametric axis. CONFIGUREDGATE: Screwdown valve in which the closing gate is shaped in a configured manner to have a more precise control of pressure and flow change across the valve. GLAND: Valve with a tapered seating, in which a rotatable plug is retained by means of a gland and gland packing. GLOBE: Screwdown valve that has a spherical body. LUBRICATEDPLUG: Plug valve in which a lubricant is injected under pressure between the plug face and the body. NEEDLE: Valve for regulating the flow in or from a pipe, in which a slender cone moves along the axis of flow to close against a fixed conical seat. PARALLELSLIDE: Screwdown valve that has a machined plate that slides in formed grooves to form a seal. PLUG: Valve that has a ported plug that can be turned relative to the body seat ports. WEDGEGATE: Screwdown valve that has a wedge shaped plate fitting into tapered guides to form a seal.</rdfs:comment>
        <rdfs:label xml:lang="en">valve mechanism</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#valveOperation -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#valveOperation">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The method of valve operation where: DROPWEIGHT: A valve that is closed by the action of a weighted lever being released, the weight normally being prevented from dropping by being held by a wire, the closure normally being made by the action of heat on a fusible link in the wire FLOAT: A valve that is opened and closed by the action of a float that rises and falls with water level. The float may be a ball attached to a lever or other mechanism HYDRAULIC: A valve that is opened and closed by hydraulic actuation LEVER: A valve that is opened and closed by the action of a lever rotating the gate within the valve. LOCKSHIELD: A valve that requires the use of a special lockshield key for opening and closing, the operating mechanism being protected by a shroud during normal operation. MOTORIZED: A valve that is opened and closed by the action of an electric motor on an actuator PNEUMATIC: A valve that is opened and closed by pneumatic actuation SOLENOID: A valve that is normally held open by a magnetic field in a coil acting on the gate but that is closed immediately if the electrical current generating the magnetic field is removed. SPRING: A valve that is normally held in position by the pressure of a spring on a plate but that may be caused to open if the pressure of the fluid is sufficient to overcome the spring pressure. THERMOSTATIC: A valve in which the ports are opened or closed to maintain a required predetermined temperature. WHEEL: A valve that is opened and closed by the action of a wheel moving the gate within the valve.</rdfs:comment>
        <rdfs:label xml:lang="en">valve operation</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#valvePattern -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#valvePattern">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">The configuration of the ports of a valve according to either the linear route taken by a fluid flowing through the valve or by the number of ports where: SINGLEPORT: Valve that has a single entry port from the system that it serves, the exit port being to the surrounding environment. ANGLED_2_PORT: Valve in which the direction of flow is changed through 90 degrees. STRAIGHT_2_PORT: Valve in which the flow is straight through. STRAIGHT_3_PORT: Valve with three separate ports. CROSSOVER_4_PORT: Valve with 4 separate ports.</rdfs:comment>
        <rdfs:label xml:lang="en">valve pattern</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/def/saref4bldg#waterFlowControlSystemType -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/def/saref4bldg#waterFlowControlSystemType">
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
        <rdfs:comment xml:lang="en">Factory fitted waterflow control system.</rdfs:comment>
        <rdfs:label xml:lang="en">water flow control system type</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/saref#hasTimestamp -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/saref#hasTimestamp">
        <rdf:type rdf:resource="http://www.w3.org/2002/07/owl#FunctionalProperty"/>
        <rdfs:range rdf:resource="http://www.w3.org/2001/XMLSchema#dateTime"/>
        <rdfs:comment xml:lang="en">A relationship stating the timestamp of an entity (e.g. a measurement).</rdfs:comment>
        <rdfs:isDefinedBy rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/saref#</rdfs:isDefinedBy>
        <rdfs:label xml:lang="en">has timestamp</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- https://w3id.org/saref#hasValue -->


    <owl:DatatypeProperty rdf:about="https://w3id.org/saref#hasValue">
        <rdfs:comment xml:lang="en">A relationship defining the value of a certain property, e.g., energy or power</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="https://w3id.org/saref#"/>
        <rdfs:label xml:lang="en">has value</rdfs:label>
    </owl:DatatypeProperty>
    


    <!-- 
    ///////////////////////////////////////////////////////////////////////////////////////
    //
    // Classes
    //
    ///////////////////////////////////////////////////////////////////////////////////////
     -->


    


    <!-- http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing -->


    <owl:Class rdf:about="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing">
        <owl:disjointWith rdf:resource="https://w3id.org/saref#Measurement"/>
        <owl:disjointWith rdf:resource="https://w3id.org/saref#Property"/>
        <owl:disjointWith rdf:resource="https://w3id.org/saref#UnitOfMeasure"/>
        <rdfs:comment xml:lang="en">Anything with spatial extent, i.e. size, shape, or position. e.g. people, places, bowling balls, as well as abstract areas like cubes.</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#"/>
        <rdfs:label xml:lang="en">Spatial thing</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Actuator -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Actuator">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:subClassOf rdf:resource="https://w3id.org/saref#Actuator"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#failPosition"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#manualOverride"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An actuator is a mechanical device for moving or controlling a mechanism or system. An actuator takes energy, usually created by air, electricity, or liquid, and converts that into some kind of motion.</rdfs:comment>
        <rdfs:label xml:lang="en">Actuator</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcActuator</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifcactuator.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_actuatortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#AirToAirHeatRecovery -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#AirToAirHeatRecovery">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryAirFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryAirFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryAirFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryAirFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasDefrost"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#heatTransferTypeEnum"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An air-to-air heat recovery device employs a counter-flow heat exchanger between inbound and outbound air flow. It is typically used to transfer heat from warmer air in one chamber to cooler air in the second chamber (i.e., typically used to recover heat from the conditioned air being exhausted and the outside air being supplied to a building), resulting in energy savings from reduced heating (or cooling) requirements.</rdfs:comment>
        <rdfs:label xml:lang="en">Air to air heat recovery</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcAirToAirHeatRecovery</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcairtoairheatrecovery.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_airtoairheatrecoverytypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Alarm -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Alarm">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:comment xml:lang="en">An alarm is a device that signals the existence of a condition or situation that is outside the boundaries of normal expectation or that activates such a device.

Alarms include the provision of break glass buttons and manual pull boxes that are used to activate alarms.</rdfs:comment>
        <rdfs:label xml:lang="en">Alarm</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcAlarm</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifcalarm.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_alarmtypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#AudioVisualAppliance -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#AudioVisualAppliance">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#audioVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#mediaSource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An audio-visual appliance is a device that displays, captures, transmits, or receives audio or video.

Audio-visual appliances may be fixed in place or may be able to be moved from one space to another. They may require an electrical supply that may be supplied either by an electrical circuit or provided from a local battery source. Audio-visual appliances may be connected to data circuits including specialist circuits for audio visual purposes only.</rdfs:comment>
        <rdfs:label xml:lang="en">Audio visual appliance</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcAudioVisualApplicance</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcaudiovisualappliance.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_audiovisualappliancetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Boiler -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Boiler">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#heatTransferSurfaceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalEnergyConsumption"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalPartLoadRatio"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#outletTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#outletTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#pressureRating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterInletTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterInletTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterStorageCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#energySource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isWaterStorageHeater"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operatingMode"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A boiler is a closed, pressure-rated vessel in which water or other fluid is heated using an energy source such as natural gas, heating oil, or electricity. The fluid in the vessel is then circulated out of the boiler for use in various processes or heating applications.</rdfs:comment>
        <rdfs:label xml:lang="en">Boiler</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcBoiler</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcboiler.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_boilertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Building -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Building">
        <rdfs:subClassOf rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#location"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasSpace"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/def/saref4bldg#BuildingSpace"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A building represents a structure that provides shelter for its occupants or contents and stands in one place. The building is also used to provide a basic element within the spatial structure hierarchy for the components of a building project (together with site, storey, and space).</rdfs:comment>
        <rdfs:label xml:lang="en">Building</rdfs:label>
        <rdfs:seeAlso rdf:resource="https://w3id.org/ifc/IFC4_ADD1#IfcBuilding"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcproductextension/lexical/ifcbuilding.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#BuildingDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#BuildingDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#BuildingObject"/>
        <rdfs:subClassOf rdf:resource="https://w3id.org/saref#Device"/>
        <rdfs:comment xml:lang="en">A tangible object designed to accomplish a particular task in a building.</rdfs:comment>
        <rdfs:label xml:lang="en">Building device</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#BuildingObject -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#BuildingObject">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#PhysicalObject"/>
        <rdfs:comment xml:lang="en">An object in the building that can be controlled by devices, such as a door or a window that can be automatically opened or closed by an actuator.  (Definition taken from SAREF 1.0)</rdfs:comment>
        <rdfs:label xml:lang="en">Building object</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#BuildingSpace -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#BuildingSpace">
        <rdfs:subClassOf rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#contains"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/def/saref4bldg#PhysicalObject"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasSpace"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/def/saref4bldg#BuildingSpace"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isSpaceOf"/>
                <owl:allValuesFrom>
                    <owl:Class>
                        <owl:unionOf rdf:parseType="Collection">
                            <rdf:Description rdf:about="https://w3id.org/def/saref4bldg#Building"/>
                            <rdf:Description rdf:about="https://w3id.org/def/saref4bldg#BuildingSpace"/>
                        </owl:unionOf>
                    </owl:Class>
                </owl:allValuesFrom>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An entity used to define the physical spaces of the building. A building space contains devices or building objects.</rdfs:comment>
        <rdfs:label xml:lang="en">Building space</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Burner -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Burner">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#energySource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A burner is a device that converts fuel into heat through combustion. It includes gas, oil, and wood burners.</rdfs:comment>
        <rdfs:label xml:lang="en">Burner</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcBurner</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcburner.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_burnertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Chiller -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Chiller">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalCondensingTemperature"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalEfficiency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalEvaporatingTemmperature"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatRejectionRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalPowerConsumption"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A chiller is a device used to remove heat from a liquid via a vapor-compression or absorption refrigeration cycle to cool a fluid, typically water or a mixture of water and glycol. The chilled fluid is then used to cool and dehumidify air in a building.</rdfs:comment>
        <rdfs:label xml:lang="en">Chiller</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcChiller</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcchiller.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_chillertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Coil -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Coil">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#airFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#airFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalLatentCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSensibleCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalUa"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#placementType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A coil is a device used to provide heat transfer between non-mixing media. A common example is a cooling coil, which utilizes a finned coil in which circulates chilled water, antifreeze, or refrigerant that is used to remove heat from air moving across the surface of the coil. A coil may be used either for heating or cooling purposes by placing a series of tubes (the coil) carrying a heating or cooling fluid into an airstream. The coil may be constructed from tubes bundled in a serpentine form or from finned tubes that give a extended heat transfer surface.

Coils may also be used for non-airflow cases such as embedded in a floor slab.</rdfs:comment>
        <rdfs:label xml:lang="en">Coil</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCoil</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifccoil.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_coiltypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#CommunicationAppliance -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#CommunicationAppliance">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:comment xml:lang="en">A communications appliance transmits and receives electronic or digital information as data or sound.

Communication appliances may be fixed in place or may be able to be moved from one space to another. Communication appliances require an electrical supply that may be supplied either by an electrical circuit or provided from a local battery source.</rdfs:comment>
        <rdfs:label xml:lang="en">Communication appliance</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCommunicationAppliance</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifccommunicationsappliance.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_communicationsappliancetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Compressor -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Compressor">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowMovingDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#compressorSpeed"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#idealCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#idealShaftPower"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#impellerDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#partLoadRatioMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#partLoadRatioMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasHotGasBypass"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#powerSource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#refrigerantClass"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A compressor is a device that compresses a fluid typically used in a refrigeration circuit.</rdfs:comment>
        <rdfs:label xml:lang="en">Compressor</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCompressor</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifccompressor.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_compressortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Condenser -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Condenser">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#externalSurfaceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalRefrigerantVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalSurfaceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalWaterVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatTransferArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatTransferCoefficient"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#refrigerantClass"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A condenser is a device that is used to dissipate heat, typically by condensing a substance such as a refrigerant from its gaseous to its liquid state.</rdfs:comment>
        <rdfs:label xml:lang="en">Condenser</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCondenser</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifccondenser.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_condensertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Controller -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Controller">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:comment xml:lang="en">A controller is a device that monitors inputs and controls outputs within a building automation system.

A controller may be physical (having placement within a spatial structure) or logical (a software interface or aggregated within a programmable physical controller).</rdfs:comment>
        <rdfs:label xml:lang="en">Controller</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcController</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifccontroller.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_controllertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#CooledBeam -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#CooledBeam">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#coilLength"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#coilWidth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalCoolingCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatingCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureCooling"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalReturnWaterTemperatureHeating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSorroundingHumidityCooling"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureCooling"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSorroundingTemperatureHeating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureCooling"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSupplyWaterTemperatureHeating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalWaterFlowCooling"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalWaterFlowHeating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterPressureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterPressureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#finishColor"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#integratedLightingType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isFreeHanging"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#pipeConnectionEnum"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterFlowControlSystemType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A cooled beam (or chilled beam) is a device typically used to cool air by circulating a fluid such as chilled water through exposed finned tubes above a space. Typically mounted overhead near or within a ceiling, the cooled beam uses convection to cool the space below it by acting as a heat sink for the naturally rising warm air of the space. Once cooled, the air naturally drops back to the floor where the cycle begins again.</rdfs:comment>
        <rdfs:label xml:lang="en">Cooled beam</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCooledBeam</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifccooledbeam.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_cooledbeamtypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#CoolingTower -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#CoolingTower">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#ambientDesignDryBulbTemperature"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#ambientDesignWetBulbTemperature"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#basinReserveVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#liftElevationDifference"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterRequirement"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#capacityControl"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#circuitType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#controlStrategy"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#flowArrangement"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfCells"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#sprayType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A cooling tower is a device which rejects heat to ambient air by circulating a fluid such as water through it to reduce its temperature by partial evaporation.</rdfs:comment>
        <rdfs:label xml:lang="en">Cooling tower</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcCoolingTower</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifccoolingtower.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_coolingtowertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Damper -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Damper">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#airFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#bladeThickness"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#closeOffRating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#faceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#frameDepth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#frameThickness"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#leakageFullyClosed"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalAirFlowRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#openPressureDrop"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#temperatureRating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#workingPressureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#bladeAction"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#bladeEdge"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#bladeShape"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#frameType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfBlades"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operation"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#orientation"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A damper typically participates in an HVAC duct distribution system and is used to control or modulate the flow of air.</rdfs:comment>
        <rdfs:label xml:lang="en">Damper</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcDamper</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcdamper.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_dampertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#DistributionControlDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#DistributionControlDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionDevice"/>
        <rdfs:comment xml:lang="en">Represents devices of a building automation control system that are used to impart control over elements of a distribution system. (Definition adapated from http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcdistributioncontrolelement.htm)</rdfs:comment>
        <rdfs:label xml:lang="en">Distribution control device</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#DistributionDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#DistributionDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#BuildingDevice"/>
        <rdfs:comment xml:lang="en">Generalization of all devices that participate in a distribution system. (Definition adapated from http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcproductextension/lexical/ifcdistributionelement.htm)</rdfs:comment>
        <rdfs:label xml:lang="en">Distribution device</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#DistributionFlowDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#DistributionFlowDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionDevice"/>
        <rdfs:comment xml:lang="en">Represents devices of a distribution system that facilitate the distribution of energy or matter, such as air, water or power. (Definition adapated from http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcdistributionflowelement.htm)</rdfs:comment>
        <rdfs:label xml:lang="en">DistributionFlowDevice</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#DuctSilencer -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#DuctSilencer">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTreatmentDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#airFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#airFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hydraulicDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#length"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#weight"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#workingPressureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#workingPressureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasExteriorInsulation"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A duct silencer is a device that is typically installed inside a duct distribution system for the purpose of reducing the noise levels from air movement, fan noise, etc. in the adjacent space or downstream of the duct silencer device.</rdfs:comment>
        <rdfs:label xml:lang="en">Duct silencer</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcDuctSilencer</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcductsilencer.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_ductsilencertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ElectricAppliance -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ElectricAppliance">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:comment xml:lang="en">An electric appliance is a device intended for consumer usage that is powered by electricity.

Electric appliances may be fixed in place or may be able to be moved from one space to another. Electric appliances require an electrical supply that may be supplied either by an electrical circuit or provided from a local battery source.</rdfs:comment>
        <rdfs:label xml:lang="en">Electric appliance</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcElectricAppliance</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcelectricappliance.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_electricappliancetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ElectricFlowStorageDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ElectricFlowStorageDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowStorageDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalFrequency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSupplyVoltage"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalSupplyVoltageMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An electric flow storage device is a device in which electrical energy is stored and from which energy may be progressively released.</rdfs:comment>
        <rdfs:label xml:lang="en">Electric flow storage device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcElectricFlowStorageDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcelectricflowstoragedevice.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_electricflowstoragedevicetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ElectricGenerator -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ElectricGenerator">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#electricGeneratorEfficiency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#powerOutputMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#startCurrentFactor"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An electric generator is an engine that is a machine for converting mechanical energy into electrical energy.</rdfs:comment>
        <rdfs:label xml:lang="en">Electric generator</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcElectricGenerator</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcelectricgenerator.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_electricgeneratortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ElectricMotor -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ElectricMotor">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#electricMotorEfficiency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#lockedRotorCurrent"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#powerOutputMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#startCurrentFactor"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#startingTime"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#teTime"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#frameSize"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasPartWinding"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isGuarded"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#motorEnclosureType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An electric motor is an engine that is a machine for converting electrical energy into mechanical energy.</rdfs:comment>
        <rdfs:label xml:lang="en">Electric motor</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcElectricMotor</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcelectricmotor.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_electricmotortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ElectricTimeControl -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ElectricTimeControl">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:comment xml:lang="en">An electric time control is a device that applies control to the provision or flow of electrical energy over time.</rdfs:comment>
        <rdfs:label xml:lang="en">Electric time control</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcElectricTimeControl</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcelectrictimecontrol.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_electrictimecontroltypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#EnergyConversionDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#EnergyConversionDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element EnergyConversionDevice defines the occurrence of a device used to perform energy conversion or heat transfer and typically participates in a flow distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">Energy conversion device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcEnergyConversionDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcenergyconversiondevice.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Engine -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Engine">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#energySource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An engine is a device that converts fuel into mechanical energy through combustion.</rdfs:comment>
        <rdfs:label xml:lang="en">Engine</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcEngine</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcengine.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_enginetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#EvaporativeCooler -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#EvaporativeCooler">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#heatExchangeArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterRequirement"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#flowArrangement"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An evaporative cooler is a device that cools air by saturating it with water vapor.</rdfs:comment>
        <rdfs:label xml:lang="en">Evaporative cooler</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcEvaporativeCooler</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcevaporativecooler.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_evaporativecoolertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Evaporator -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Evaporator">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#externalSurfaceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalRefrigerantVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalSurfaceArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalWaterVolume"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatTransferArea"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalHeatTransferCoefficient"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#evaporationCoolant"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#evaporationMediumType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#refrigerantClass"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An evaporator is a device in which a liquid refrigerent is vaporized and absorbs heat from the surrounding fluid.</rdfs:comment>
        <rdfs:label xml:lang="en">Evaporator</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcEvaporator</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcevaporator.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_evaporatortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Fan -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Fan">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowMovingDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalAirFlowRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalPowerRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalRotationSpeed"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalStaticPressure"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalTotalPressure"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationalRiterial"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#capacityControlType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#motorDriveType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A fan is a device which imparts mechanical work on a gas. A typical usage of a fan is to induce airflow in a building services air distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">Fan</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFan</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcfan.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_fantypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Filter -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Filter">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTreatmentDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#finalResistance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#fluidFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#fluidFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#initialResistance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalFilterFaceVelocity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalFlowRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalMediaSurfaceVelocity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalParticleGeometricMeanDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalParticleGeometricStandardDeviation"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalPressureDrop"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#weight"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A filter is an apparatus used to remove particulate or gaseous matter from fluids and gases.</rdfs:comment>
        <rdfs:label xml:lang="en">Filter</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFilter</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcfilter.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_filtertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FireSuppressionTerminal -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FireSuppressionTerminal">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:comment xml:lang="en">A fire suppression terminal has the purpose of delivering a fluid (gas or liquid) that will suppress a fire.

A fire suppression terminal provides for all forms of sprinkler, spreader and other form of terminal that is connected to a pipework system and intended to act in the role of suppressing a fire.</rdfs:comment>
        <rdfs:label xml:lang="en">Fire suppression terminal</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFireSuppressionTerminal</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/lexical/ifcfiresuppressionterminal.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/pset/pset_firesuppressionterminaltypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowController -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowController">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element FlowController defines the occurrence of elements of a distribution system that are used to regulate flow through a distribution system. Examples include dampers, valves, switches, and relays.</rdfs:comment>
        <rdfs:label xml:lang="en">Flow controller</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowController</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcflowcontroller.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowInstrument -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowInstrument">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:comment xml:lang="en">A flow instrument reads and displays the value of a particular property of a system at a point, or displays the difference in the value of a property between two points.

Instrumentation is typically for the purpose of determining the value of the property at a point in time. It is not the purpose of an instrument to record or integrate the values over time (although they may be connected to recording devices that do perform such a function). This entity provides for all forms of mechanical flow instrument (thermometers, pressure gauges etc.) and electrical flow instruments (ammeters, voltmeters etc.)</rdfs:comment>
        <rdfs:label xml:lang="en">Flow instrument</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowInstrument</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifcflowinstrument.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_flowinstrumenttypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowMeter -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowMeter">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#readOutType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#remoteReading"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A flow meter is a device that is used to measure the flow rate in a system.</rdfs:comment>
        <rdfs:label xml:lang="en">Flow meter</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowMeter</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcflowmeter.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_flowmetertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowMovingDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowMovingDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element FlowMovingDevice defines the occurrence of an apparatus used to distribute, circulate or perform conveyance of fluids, including liquids and gases (such as a pump or fan), and typically participates in a flow distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">Flow moving device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowMovingDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcflowmovingdevice.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowStorageDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowStorageDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element FlowStorageDevice defines the occurrence of a device that participates in a distribution system and is used for temporary storage (such as a tank).</rdfs:comment>
        <rdfs:label xml:lang="en">Flow storage device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowStorageDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcflowstoragedevice.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowTerminal -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowTerminal">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element FlowTerminal defines the occurrence of a permanently attached element that acts as a terminus or beginning of a distribution system (such as an air outlet, drain, water closet, or sink). A terminal is typically a point at which a system interfaces with an external environment.</rdfs:comment>
        <rdfs:label xml:lang="en">Flow terminal</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowTerminal</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcflowterminal.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#FlowTreatmentDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#FlowTreatmentDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionFlowDevice"/>
        <rdfs:comment xml:lang="en">The distribution flow element FlowTreatmentDevice defines the occurrence of a device typically used to remove unwanted matter from a fluid, either liquid or gas, and typically participates in a flow distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">Flow treatment device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcFlowTreatmentDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgserviceelements/lexical/ifcflowtreatmentdevice.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#HeatExchanger -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#HeatExchanger">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#arrangement"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A heat exchanger is a device used to provide heat transfer between non-mixing media such as plate and shell and tube heat exchangers. HeatExchanger is commonly used on water-side distribution systems to recover energy from a liquid to another liquid (typically water-based), whereas AirToAirHeatRecovery is commonly used on air-side distribution systems to recover energy from a gas to a gas (usually air).</rdfs:comment>
        <rdfs:label xml:lang="en">Heat exchanger</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcHeatExchanger</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcheatexchanger.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_heatexchangertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Humidifier -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Humidifier">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalAirFlowRate"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalMoistureGain"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#waterRequirement"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#weight"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#application"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#internalControl"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A humidifier is a device that adds moisture into the air.</rdfs:comment>
        <rdfs:label xml:lang="en">Humidifier</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcHumidifier</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifchumidifier.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_humidifiertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Interceptor -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Interceptor">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTreatmentDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#coverLength"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#coverWidth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#inletConnectionSize"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalBodyDepth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalBodyLength"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalBodyWidth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#outletConnectionSize"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#ventilatingPipeSize"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An interceptor is a device designed and installed in order to separate and retain deleterious, hazardous or undesirable matter while permitting normal sewage or liquids to discharge into a collection system by gravity.</rdfs:comment>
        <rdfs:label xml:lang="en">Interceptor</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcInterceptor</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/lexical/ifcinterceptor.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/pset/pset_interceptortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Lamp -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Lamp">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#colorTemperature"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#contributedLuminousFlux"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#lampMaintenanceFactor"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#lightEmitterNominalPower"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#spectrumMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#spectrumMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#colorAppearance"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#colorRenderingIndex"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#lampBallastType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#lampCompensationType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A lamp is an artificial light source such as a light bulb or tube.</rdfs:comment>
        <rdfs:label xml:lang="en">Lamp</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcLamp</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifclamp.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_lamptypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#MedicalDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#MedicalDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:comment xml:lang="en">A medical device is attached to a medical piping system and operates upon medical gases to perform a specific function. Medical gases include medical air, medical vacuum, oxygen, carbon dioxide, nitrogen, and nitrous oxide.</rdfs:comment>
        <rdfs:label xml:lang="en">Medical device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcMedicalDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcmedicaldevice.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_medicaldevicetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Outlet -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Outlet">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isPluggableOutlet"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOsSockets"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">An outlet is a device installed at a point to receive one or more inserted plugs for electrical power or communications.

Power outlets are commonly connected within a junction box; data outlets may be directly connected to a wall. For power outlets sharing the same circuit within a junction box, the ports should indicate the logical wiring relationship to the enclosing junction box, even though they may be physically connected to a cable going to another outlet, switch, or fixture.</rdfs:comment>
        <rdfs:label xml:lang="en">Outlet</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcOutlet</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcoutlet.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_outlettypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#PhysicalObject -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#PhysicalObject">
        <rdfs:subClassOf rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#location"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2003/01/geo/wgs84_pos#SpatialThing"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#contains"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/def/saref4bldg#PhysicalObject"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isContainedIn"/>
                <owl:allValuesFrom>
                    <owl:Class>
                        <owl:unionOf rdf:parseType="Collection">
                            <rdf:Description rdf:about="https://w3id.org/def/saref4bldg#BuildingSpace"/>
                            <rdf:Description rdf:about="https://w3id.org/def/saref4bldg#PhysicalObject"/>
                        </owl:unionOf>
                    </owl:Class>
                </owl:allValuesFrom>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">Any Object that has a proper space region.  (Definition extracted from DUL ontology)</rdfs:comment>
        <rdfs:label xml:lang="en">Physical object</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ProtectiveDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ProtectiveDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:comment xml:lang="en">A protective device breaks an electrical circuit when a stated electric current that passes through it is exceeded.

A protective device provides protection against electrical current only (not as a general protective device). It may be used to represent the complete set of elements including both the tripping unit and the breaking unit that provide the protection. This may be particularly useful at earlier stages of design where the approach to breaking the electrical supply may be determined but the method of tripping may not. Alternatively, this entity may be used to specifically represent the breaking unit alone (in which case the tripping unit will also be specifically identified). This entity is specific to dedicated protective devices and excludes electrical outlets that may have circuit protection.</rdfs:comment>
        <rdfs:label xml:lang="en">Protective device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcProtectiveDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcprotectivedevice.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_protectivedevicetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ProtectiveDeviceTrippingUnit -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ProtectiveDeviceTrippingUnit">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#limitingTerminalSize"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#standard"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A protective device tripping unit breaks an electrical circuit at a separate breaking unit when a stated electric current that passes through the unit is exceeded.</rdfs:comment>
        <rdfs:label xml:lang="en">Protective device tripping unit</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcProtectiveDeviceTrippingUnit</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcprotectivedevicetrippingunit.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_protectivedevicetrippingunittypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Pump -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Pump">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowMovingDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#connectionSize"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#flowResistanceMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#flowResistanceMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#netPositiveSuctionHead"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nomminalRotationSpeed"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operationTemperatureMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#pumpFlowRateMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#pumpFlowRateMin"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A pump is a device which imparts mechanical work on fluids or slurries to move them through a channel or pipeline. A typical use of a pump is to circulate chilled water or heating hot water in a building services distribution system.</rdfs:comment>
        <rdfs:label xml:lang="en">Pump</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcPump</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcpump.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_pumptypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#SanitaryTerminal -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#SanitaryTerminal">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:comment xml:lang="en">A sanitary terminal is a fixed appliance or terminal usually supplied with water and used for drinking, cleaning or foul water disposal or that is an item of equipment directly used with such an appliance or terminal.</rdfs:comment>
        <rdfs:label xml:lang="en">Sanitary terminal</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcSanitaryTerminal</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/lexical/ifcsanitaryterminal.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcplumbingfireprotectiondomain/pset/pset_sanitaryterminaltypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Sensor -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Sensor">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:subClassOf rdf:resource="https://w3id.org/saref#Sensor"/>
        <rdfs:comment xml:lang="en">A sensor is a device that measures a physical quantity and converts it into a signal which can be read by an observer or by an instrument.</rdfs:comment>
        <rdfs:label xml:lang="en">Sensor</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcSensor</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifcsensor.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_sensortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#ShadingDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#ShadingDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#BuildingDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#solarReflectance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#solarTransmittance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#thermalTransmittance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#visibleLightReflectance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#visibleLightTransmittance"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isExternal"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#mechanicalOperated"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#roughness"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#shadingDeviceType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">Shading devices are purpose built devices to protect from the sunlight, from natural light, or screening them from view. Shading devices can form part of the facade or can be mounted inside the building, they can be fixed or operable.</rdfs:comment>
        <rdfs:label xml:lang="en">Shading device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcShadingDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgelements/lexical/ifcshadingdevice.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcsharedbldgelements/pset/pset_shadingdevicecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#SolarDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#SolarDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:comment xml:lang="en">A solar device converts solar radiation into other energy such as electric current or thermal energy.</rdfs:comment>
        <rdfs:label xml:lang="en">Solar device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcSolarDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcsolardevicetypeenum.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_solardevicetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#SpaceHeater -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#SpaceHeater">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowTerminal"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#bodyMass"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#outputCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#thermalEfficiency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#thermalMassHeatCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#energySource"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#heatTransferDimension"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#heatTransferMedium"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfPanels"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfSections"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#placementType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#temperatureClassification"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">Space heaters utilize a combination of radiation and/or natural convection using a heating source such as electricity, steam or hot water to heat a limited space or area. Examples of space heaters include radiators, convectors, baseboard and finned-tube heaters.

UnitaryEquipment should be used for packaged units supporting a combination of heating, cooling, and/or dehumidification; Coil should be used for coil-based floor heating.</rdfs:comment>
        <rdfs:label xml:lang="en">Space heater</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcSpaceHeater</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcspaceheater.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_spaceheatertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#SwitchingDevice -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#SwitchingDevice">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasLock"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isIlluminated"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#legend"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfGangs"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#switchFunction"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A switch is used in a cable distribution system (electrical circuit) to control or modulate the flow of electricity.

Switches include those used for electrical power, communications, audio-visual, or other distribution system types as determined by the available ports.</rdfs:comment>
        <rdfs:label xml:lang="en">Switching device</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcSwitchingDevice</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifcswitchingdevice.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_switchingdevicetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Tank -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Tank">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowStorageDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#effectiveCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#firstCurvatureRadius"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalDepth"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalLengthOrDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalVolumetricCapacity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalWidthOrDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#operatingWight"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondCurvatureRadius"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#accessType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#endShapeType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfSections"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#patternType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#storageType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A tank is a vessel or container in which a fluid or gas is stored for later use.</rdfs:comment>
        <rdfs:label xml:lang="en">Tank</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcTank</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifctank.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_tanktypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Transformer -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Transformer">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#apparentPowerMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#imaginaryImpedanceRatio"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryApparentPower"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryCurrent"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryFrequency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#primaryVoltage"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#realImpedanceRatio"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryApparentPower"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryCurrent"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryFrequency"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryVoltage"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isNeutralPrimaryTerminalAvailable"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isNeutralSecondaryTerminalAvailable"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#secondaryCurrentType"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#transformerVectorGroup"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A transformer is an inductive stationary device that transfers electrical energy from one circuit to another.

Transformer is used to transform electric power; conversion of electric signals for other purposes is handled at other entities: Controller converts arbitrary signals, AudioVisualAppliance converts signals for audio or video streams, and CommunicationsAppliance converts signals for data or other communications usage.</rdfs:comment>
        <rdfs:label xml:lang="en">Transformer</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcTransformer</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/lexical/ifctransformer.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcelectricaldomain/pset/pset_transformertypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#TransportElement -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#TransportElement">
        <rdfs:subClassOf rdf:resource="https://w3id.org/saref#Device"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#capacityWeight"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#capacityPeople"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#positiveInteger"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#fireExit"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A transport element is a generalization of all transport related objects that move people, animals or goods within a building or building complex. The TransportElement defines the occurrence of a transport element. </rdfs:comment>
        <rdfs:label xml:lang="en">Transport element</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcTransportElement</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcproductextension/lexical/ifctransportelement.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcproductextension/pset/pset_transportelementcommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#TubeBundle -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#TubeBundle">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#EnergyConversionDevice"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#foulingFactor"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#horizontalSpacing"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#inLineRowSpacing"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#insideDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#length"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#nominalDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#outsideDiameter"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#staggeredRowSpacing"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#thermalConductivity"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#verticalSpacing"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#volumen"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#hasTurbulator"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#boolean"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfCircuits"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#numberOfRows"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#integer"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A tube bundle is a device consisting of tubes and bundles of tubes used for heat transfer and contained typically within other energy conversion devices, such as a chiller or coil.</rdfs:comment>
        <rdfs:label xml:lang="en">Tube bundle</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcTubeBundle</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifctubebundle.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_tubebundletypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#UnitaryControlElement -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#UnitaryControlElement">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#DistributionControlDevice"/>
        <rdfs:comment xml:lang="en">A unitary control element combines a number of control components into a single product, such as a thermostat or humidistat.

A unitary control element provides a housing for an aggregation of control or electrical distribution elements that, in combination, perform a singular (unitary) purpose. Each item in the aggregation may have its own geometric representation and location.</rdfs:comment>
        <rdfs:label xml:lang="en">Unitary control element</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcUnitaryControlElement</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/lexical/ifcunitarycontrolelement.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifcbuildingcontrolsdomain/pset/pset_unitarycontrolelementtypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#Valve -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#Valve">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#FlowController"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#closeOffRating"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#flowCoefficient"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#size"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#testPressure"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#workingPressure"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#valveMechanism"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#valveOperation"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#valvePattern"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#string"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A valve is used in a building services piping distribution system to control or modulate the flow of the fluid.</rdfs:comment>
        <rdfs:label xml:lang="en">Valve</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcValve</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcvalve.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_valvetypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/def/saref4bldg#VibrationIsolator -->


    <owl:Class rdf:about="https://w3id.org/def/saref4bldg#VibrationIsolator">
        <rdfs:subClassOf rdf:resource="https://w3id.org/saref#Device"/>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#height"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isolatorCompressibility"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#isolatorStaticDeflection"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#supportedWeightMax"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/def/saref4bldg#vibrationTransmissibility"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Measurement"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:comment xml:lang="en">A vibration isolator is a device used to minimize the effects of vibration transmissibility in a building.</rdfs:comment>
        <rdfs:label xml:lang="en">Vibration isolator</rdfs:label>
        <rdfs:seeAlso rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/ifc/IFC4_ADD1#IfcVibrationIsolator</rdfs:seeAlso>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/lexical/ifcvibrationisolator.htm"/>
        <prov:hadPrimarySource rdf:resource="http://www.buildingsmart-tech.org/ifc/IFC4/Add1/html/schema/ifchvacdomain/pset/pset_vibrationisolatortypecommon.htm"/>
    </owl:Class>
    


    <!-- https://w3id.org/saref#Actuator -->


    <owl:Class rdf:about="https://w3id.org/saref#Actuator">
        <rdfs:comment xml:lang="en">A device responsible for moving or controlling a mechanism or system</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="https://w3id.org/saref#"/>
        <rdfs:label xml:lang="en">Actuator</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/saref#Device -->


    <owl:Class rdf:about="https://w3id.org/saref#Device">
        <rdfs:subClassOf rdf:resource="https://w3id.org/def/saref4bldg#PhysicalObject"/>
        <rdfs:comment xml:lang="en">A tangible object designed to accomplish a particular task in households, common public buildings or offices. In order to accomplish this task, the device performs one or more functions. For example, a washing machine is designed to wash (task) and to accomplish this task it performs the start and stop function.</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="https://w3id.org/saref#"/>
        <rdfs:label xml:lang="en">Device</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/saref#Measurement -->


    <owl:Class rdf:about="https://w3id.org/saref#Measurement">
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#isMeasuredIn"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#UnitOfMeasure"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#relatesToProperty"/>
                <owl:allValuesFrom rdf:resource="https://w3id.org/saref#Property"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#isMeasuredIn"/>
                <owl:qualifiedCardinality rdf:datatype="http://www.w3.org/2001/XMLSchema#nonNegativeInteger">1</owl:qualifiedCardinality>
                <owl:onClass rdf:resource="https://w3id.org/saref#UnitOfMeasure"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#relatesToProperty"/>
                <owl:qualifiedCardinality rdf:datatype="http://www.w3.org/2001/XMLSchema#nonNegativeInteger">1</owl:qualifiedCardinality>
                <owl:onClass rdf:resource="https://w3id.org/saref#Property"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#hasTimestamp"/>
                <owl:allValuesFrom rdf:resource="http://www.w3.org/2001/XMLSchema#dateTime"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <rdfs:subClassOf>
            <owl:Restriction>
                <owl:onProperty rdf:resource="https://w3id.org/saref#hasValue"/>
                <owl:qualifiedCardinality rdf:datatype="http://www.w3.org/2001/XMLSchema#nonNegativeInteger">1</owl:qualifiedCardinality>
                <owl:onDataRange rdf:resource="http://www.w3.org/2001/XMLSchema#float"/>
            </owl:Restriction>
        </rdfs:subClassOf>
        <owl:disjointWith rdf:resource="https://w3id.org/saref#Property"/>
        <owl:disjointWith rdf:resource="https://w3id.org/saref#UnitOfMeasure"/>
        <rdfs:comment xml:lang="en">Represents the measured value made over a property. It is also linked to the unit of measure in which the value is expressed and the timestamp of the measurement.</rdfs:comment>
        <rdfs:isDefinedBy rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/saref#</rdfs:isDefinedBy>
        <rdfs:label xml:lang="en">Measurement</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/saref#Property -->


    <owl:Class rdf:about="https://w3id.org/saref#Property">
        <owl:disjointWith rdf:resource="https://w3id.org/saref#UnitOfMeasure"/>
        <rdfs:comment xml:lang="en">An aspect of an entity that can be observable by a sensor.</rdfs:comment>
        <rdfs:isDefinedBy rdf:datatype="http://www.w3.org/2001/XMLSchema#string">https://w3id.org/saref#</rdfs:isDefinedBy>
        <rdfs:label xml:lang="en">Property</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/saref#Sensor -->


    <owl:Class rdf:about="https://w3id.org/saref#Sensor">
        <rdfs:comment xml:lang="en">A device that detects and responds to events or changes in the physical environment such as light, motion, or temperature changes.
A device that has category saref:Sensor and performs a saref:SensingFunction.</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="https://w3id.org/saref#"/>
        <rdfs:label xml:lang="en">Sensor</rdfs:label>
    </owl:Class>
    


    <!-- https://w3id.org/saref#UnitOfMeasure -->


    <owl:Class rdf:about="https://w3id.org/saref#UnitOfMeasure">
        <rdfs:comment xml:lang="en">The unit of measure is a standard for measurement of a quantity, such as a Property. For example,  Power is a property and Watt is a unit of power that represents a definite predetermined power: when we say 10 Watt, we actually mean 10 times the definite predetermined power called &quot;watt&quot;. Our definition is based on the definition of unit of measure in the Ontology of units of Measure (OM). We propose here a list of some units of measure that are relevant for the purpose of the Smart Appliances ontology, but this list can be extended.</rdfs:comment>
        <rdfs:isDefinedBy rdf:resource="https://w3id.org/saref#"/>
        <rdfs:label xml:lang="en">Unit of measure</rdfs:label>
    </owl:Class>
</rdf:RDF>



<!-- Generated by the OWL API (version 5.1.0) https://github.com/owlcs/owlapi/ -->


