Package generated_from_e_line_examples_provider_bridge_json {
    Type String
    Type TODO_RESOLVE_REFERENCED
    Use "e-line-examples-provider-bridge.json" as SOURCE_MAPPING
    Type JSON_String
    Structure JSON_e_line_examples_provider_bridge_json (
        JSON_ieee802_dot1q_bridge_bridges ieee802_dot1q_bridge_bridges,
        JSON_ietf_interfaces_interfaces ietf_interfaces_interfaces
    )
    Structure JSON_ieee802_dot1q_bridge_bridges (
        JSON_bridge bridge
    )
    Collection JSON_bridge of JSON_bridge_item
    Structure JSON_bridge_item (
        JSON_String name,
        JSON_String address,
        JSON_String bridge_type,
        JSON_component ^component
    )
    Collection JSON_component of JSON_component_item
    Structure JSON_component_item (
        JSON_String name,
        JSON_String id,
        JSON_String type,
        JSON_bridge_port bridge_port,
        JSON_filtering_database filtering_database,
        JSON_bridge_vlan bridge_vlan
    )
    Collection JSON_bridge_port of JSON_String
    Structure JSON_filtering_database (
        JSON_vlan_registration_entry vlan_registration_entry
    )
    Collection JSON_vlan_registration_entry of JSON_vlan_registration_entry_item
    Structure JSON_vlan_registration_entry_item (
        JSON_String database_id,
        JSON_String vids,
        JSON_String entry_type,
        JSON_port_map port_map
    )
    Collection JSON_port_map of JSON_port_map_item
    Structure JSON_port_map_item (
        JSON_String port_ref,
        JSON_static_vlan_registration_entries static_vlan_registration_entries
    )
    Structure JSON_static_vlan_registration_entries (
        JSON_String vlan_transmitted
    )
    Structure JSON_bridge_vlan (
        JSON_vlan vlan
    )
    Collection JSON_vlan of JSON_vlan_item
    Structure JSON_vlan_item (
        JSON_String vid,
        JSON_String name,
        JSON_untagged_ports untagged_ports,
        JSON_egress_ports egress_ports
    )
    Collection JSON_untagged_ports of JSON_String
    Collection JSON_egress_ports of JSON_String
    Structure JSON_ietf_interfaces_interfaces (
        JSON_interface interface
    )
    Collection JSON_interface of JSON_interface_item
    Structure JSON_interface_item (
        JSON_String name,
        JSON_String type,
        JSON_String oper_status,
        JSON_statistics statistics,
        JSON_ieee802_dot1q_bridge_bridge_port ieee802_dot1q_bridge_bridge_port
    )
    Structure JSON_statistics (
        JSON_String discontinuity_time
    )
    Structure JSON_ieee802_dot1q_bridge_bridge_port (
        JSON_String bridge_name,
        JSON_String component_name,
        JSON_String port_type,
        JSON_String pvid,
        JSON_String acceptable_frame,
        JSON_String enable_ingress_filtering,
        JSON_String port_number,
        JSON_ieee802_dot1q_pb_cvid_registration ieee802_dot1q_pb_cvid_registration,
        JSON_String enable_vid_translation_table,
        JSON_String enable_egress_vid_translation_table,
        JSON_vid_translations vid_translations
    )
    Collection JSON_ieee802_dot1q_pb_cvid_registration of JSON_ieee802_dot1q_pb_cvid_registration_item
    Structure JSON_ieee802_dot1q_pb_cvid_registration_item (
        JSON_String cvid,
        JSON_String svid,
        JSON_String untagged_pep,
        JSON_String untagged_cep
    )
    Collection JSON_vid_translations of JSON_vid_translations_item
    Structure JSON_vid_translations_item (
        JSON_String local_vid,
        JSON_String relay_vid
    )
    JSON_e_line_examples_provider_bridge_json JSON_instance (
        ieee802_dot1q_bridge_bridges = (
            bridge = [
                (
                    name = "ne1",
                    address = "10-10-10-10-10-10",
                    bridge_type = "ieee802-dot1q-bridge:provider-edge-bridge",
                    ^component = [
                        (
                            name = "sv0",
                            id = "0",
                            type = "ieee802-dot1q-bridge:s-vlan-component",
                            bridge_port = [
                                "eth3",
                                "eth4",
                                "eth5"
                            ],
                            filtering_database = (
                                vlan_registration_entry = [
                                    (
                                        database_id = "1",
                                        vids = "200",
                                        entry_type = "static",
                                        port_map = [
                                            (
                                                port_ref = "1",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "untagged"
                                                )
                                            ),
                                            (
                                                port_ref = "5",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "tagged"
                                                )
                                            )
                                        ]
                                    ),
                                    (
                                        database_id = "1",
                                        vids = "300",
                                        entry_type = "static",
                                        port_map = [
                                            (
                                                port_ref = "2",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "untagged"
                                                )
                                            ),
                                            (
                                                port_ref = "5",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "tagged"
                                                )
                                            )
                                        ]
                                    ),
                                    (
                                        database_id = "1",
                                        vids = "400",
                                        entry_type = "static",
                                        port_map = [
                                            (
                                                port_ref = "3",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "untagged"
                                                )
                                            ),
                                            (
                                                port_ref = "5",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "tagged"
                                                )
                                            )
                                        ]
                                    ),
                                    (
                                        database_id = "1",
                                        vids = "500",
                                        entry_type = "static",
                                        port_map = [
                                            (
                                                port_ref = "4",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "tagged"
                                                )
                                            ),
                                            (
                                                port_ref = "5",
                                                static_vlan_registration_entries = (
                                                    vlan_transmitted = "tagged"
                                                )
                                            )
                                        ]
                                    )
                                ]
                            ),
                            bridge_vlan = (
                                vlan = [
                                    (
                                        vid = "200",
                                        name = "E-Line 200",
                                        untagged_ports = [
                                            "eth1"
                                        ],
                                        egress_ports = [
                                            "eth1",
                                            "eth5"
                                        ]
                                    ),
                                    (
                                        vid = "300",
                                        name = "E-Line 300",
                                        untagged_ports = [
                                            "eth2"
                                        ],
                                        egress_ports = [
                                            "eth2",
                                            "eth5"
                                        ]
                                    ),
                                    (
                                        vid = "400",
                                        name = "E-Line 400",
                                        untagged_ports = [
                                            "eth3"
                                        ],
                                        egress_ports = [
                                            "eth3",
                                            "eth5"
                                        ]
                                    ),
                                    (
                                        vid = "500",
                                        name = "E-Line 500",
                                        egress_ports = [
                                            "eth4",
                                            "eth5"
                                        ]
                                    )
                                ]
                            )
                        ),
                        (
                            name = "cv1",
                            id = "1",
                            type = "ieee802-dot1q-bridge:c-vlan-component",
                            bridge_port = [
                                "eth1"
                            ]
                        ),
                        (
                            name = "cv2",
                            id = "2",
                            type = "ieee802-dot1q-bridge:c-vlan-component",
                            bridge_port = [
                                "eth2"
                            ]
                        )
                    ]
                )
            ]
        ),
        ietf_interfaces_interfaces = (
            interface = [
                (
                    name = "eth1",
                    type = "iana-if-type:ethernetCsmacd",
                    oper_status = "up",
                    statistics = (
                        discontinuity_time = "2022-03-23T11:00:00+02:00"
                    ),
                    ieee802_dot1q_bridge_bridge_port = (
                        bridge_name = "ne1",
                        component_name = "cv1",
                        port_type = "ieee802-dot1q-bridge:customer-edge-port",
                        pvid = "1",
                        acceptable_frame = "admit-only-VLAN-tagged-frames",
                        enable_ingress_filtering = "true",
                        port_number = "1",
                        ieee802_dot1q_pb_cvid_registration = [
                            (
                                cvid = "100",
                                svid = "200",
                                untagged_pep = "false",
                                untagged_cep = "false"
                            )
                        ]
                    )
                ),
                (
                    name = "eth2",
                    type = "iana-if-type:ethernetCsmacd",
                    oper_status = "up",
                    statistics = (
                        discontinuity_time = "2022-03-23T11:00:00+02:00"
                    ),
                    ieee802_dot1q_bridge_bridge_port = (
                        bridge_name = "ne1",
                        component_name = "cv2",
                        port_type = "ieee802-dot1q-bridge:customer-edge-port",
                        pvid = "1",
                        acceptable_frame = "admit-only-untagged-and-priority-tagged",
                        enable_ingress_filtering = "true",
                        port_number = "2",
                        ieee802_dot1q_pb_cvid_registration = [
                            (
                                cvid = "1",
                                svid = "300",
                                untagged_pep = "true",
                                untagged_cep = "true"
                            )
                        ]
                    )
                ),
                (
                    name = "eth3",
                    type = "iana-if-type:ethernetCsmacd",
                    oper_status = "up",
                    statistics = (
                        discontinuity_time = "2022-03-23T11:00:00+02:00"
                    ),
                    ieee802_dot1q_bridge_bridge_port = (
                        bridge_name = "ne1",
                        component_name = "sv0",
                        port_type = "ieee802-dot1q-bridge:customer-network-port",
                        pvid = "400",
                        acceptable_frame = "admit-only-untagged-and-priority-tagged",
                        enable_ingress_filtering = "true",
                        port_number = "3"
                    )
                ),
                (
                    name = "eth4",
                    type = "iana-if-type:ethernetCsmacd",
                    oper_status = "up",
                    statistics = (
                        discontinuity_time = "2022-03-23T11:00:00+02:00"
                    ),
                    ieee802_dot1q_bridge_bridge_port = (
                        bridge_name = "ne1",
                        component_name = "sv0",
                        port_type = "ieee802-dot1q-bridge:customer-network-port",
                        pvid = "1",
                        acceptable_frame = "admit-only-VLAN-tagged-frames",
                        enable_ingress_filtering = "true",
                        port_number = "4",
                        enable_vid_translation_table = "true",
                        enable_egress_vid_translation_table = "false",
                        vid_translations = [
                            (
                                local_vid = "100",
                                relay_vid = "500"
                            )
                        ]
                    )
                ),
                (
                    name = "eth5",
                    type = "iana-if-type:ethernetCsmacd",
                    oper_status = "up",
                    statistics = (
                        discontinuity_time = "2022-03-23T11:00:00+02:00"
                    ),
                    ieee802_dot1q_bridge_bridge_port = (
                        bridge_name = "ne1",
                        component_name = "sv0",
                        port_type = "ieee802-dot1q-bridge:provider-network-port",
                        pvid = "1",
                        acceptable_frame = "admit-only-VLAN-tagged-frames",
                        enable_ingress_filtering = "true",
                        port_number = "5"
                    )
                )
            ]
        )
    )
    Map JSON_e_line_examples_provider_bridge_json to "JSON" in SOURCE_MAPPING as JSON_SOURCE_MAPPING {
        ieee802_dot1q_bridge_bridges -> "ieee802-dot1q-bridge:bridges",
        ietf_interfaces_interfaces -> "ietf-interfaces:interfaces"
    }
    Map JSON_ieee802_dot1q_bridge_bridges to "JSON.ieee802-dot1q-bridge:bridges" in SOURCE_MAPPING as JSON_ieee802_dot1q_bridge_bridges_SOURCE_MAPPING {
        bridge -> "bridge"
    }
    Map JSON_bridge_item to "JSON.bridge.item" in SOURCE_MAPPING as JSON_bridge_item_SOURCE_MAPPING {
        name -> "name",
        address -> "address",
        bridge_type -> "bridge-type",
        ^component -> "component"
    }
    Map JSON_component_item to "JSON.component.item" in SOURCE_MAPPING as JSON_component_item_SOURCE_MAPPING {
        name -> "name",
        id -> "id",
        type -> "type",
        bridge_port -> "bridge-port",
        filtering_database -> "filtering-database",
        bridge_vlan -> "bridge-vlan"
    }
    Map JSON_filtering_database to "JSON.filtering-database" in SOURCE_MAPPING as JSON_filtering_database_SOURCE_MAPPING {
        vlan_registration_entry -> "vlan-registration-entry"
    }
    Map JSON_vlan_registration_entry_item to "JSON.vlan-registration-entry.item" in SOURCE_MAPPING as JSON_vlan_registration_entry_item_SOURCE_MAPPING {
        database_id -> "database-id",
        vids -> "vids",
        entry_type -> "entry-type",
        port_map -> "port-map"
    }
    Map JSON_port_map_item to "JSON.port-map.item" in SOURCE_MAPPING as JSON_port_map_item_SOURCE_MAPPING {
        port_ref -> "port-ref",
        static_vlan_registration_entries -> "static-vlan-registration-entries"
    }
    Map JSON_static_vlan_registration_entries to "JSON.static-vlan-registration-entries" in SOURCE_MAPPING as JSON_static_vlan_registration_entries_SOURCE_MAPPING {
        vlan_transmitted -> "vlan-transmitted"
    }
    Map JSON_bridge_vlan to "JSON.bridge-vlan" in SOURCE_MAPPING as JSON_bridge_vlan_SOURCE_MAPPING {
        vlan -> "vlan"
    }
    Map JSON_vlan_item to "JSON.vlan.item" in SOURCE_MAPPING as JSON_vlan_item_SOURCE_MAPPING {
        vid -> "vid",
        name -> "name",
        untagged_ports -> "untagged-ports",
        egress_ports -> "egress-ports"
    }
    Map JSON_ietf_interfaces_interfaces to "JSON.ietf-interfaces:interfaces" in SOURCE_MAPPING as JSON_ietf_interfaces_interfaces_SOURCE_MAPPING {
        interface -> "interface"
    }
    Map JSON_interface_item to "JSON.interface.item" in SOURCE_MAPPING as JSON_interface_item_SOURCE_MAPPING {
        name -> "name",
        type -> "type",
        oper_status -> "oper-status",
        statistics -> "statistics",
        ieee802_dot1q_bridge_bridge_port -> "ieee802-dot1q-bridge:bridge-port"
    }
    Map JSON_statistics to "JSON.statistics" in SOURCE_MAPPING as JSON_statistics_SOURCE_MAPPING {
        discontinuity_time -> "discontinuity-time"
    }
    Map JSON_ieee802_dot1q_bridge_bridge_port to "JSON.ieee802-dot1q-bridge:bridge-port" in SOURCE_MAPPING as JSON_ieee802_dot1q_bridge_bridge_port_SOURCE_MAPPING {
        bridge_name -> "bridge-name",
        component_name -> "component-name",
        port_type -> "port-type",
        pvid -> "pvid",
        acceptable_frame -> "acceptable-frame",
        enable_ingress_filtering -> "enable-ingress-filtering",
        port_number -> "port-number",
        ieee802_dot1q_pb_cvid_registration -> "ieee802-dot1q-pb:cvid-registration",
        enable_vid_translation_table -> "enable-vid-translation-table",
        enable_egress_vid_translation_table -> "enable-egress-vid-translation-table",
        vid_translations -> "vid-translations"
    }
    Map JSON_ieee802_dot1q_pb_cvid_registration_item to "JSON.ieee802-dot1q-pb:cvid-registration.item" in SOURCE_MAPPING as JSON_ieee802_dot1q_pb_cvid_registration_item_SOURCE_MAPPING {
        cvid -> "cvid",
        svid -> "svid",
        untagged_pep -> "untagged-pep",
        untagged_cep -> "untagged-cep"
    }
    Map JSON_vid_translations_item to "JSON.vid-translations.item" in SOURCE_MAPPING as JSON_vid_translations_item_SOURCE_MAPPING {
        local_vid -> "local-vid",
        relay_vid -> "relay-vid"
    }
}